;PROJECT=TFC_isa_v3

SOURCEDEFS

; a natural source
;id   position    directivity  aim-position [roll]
 A0  -2.85 0.5 0.2     OMNI     0.0 d/2 1.41
 Lp1m_a   = Lp_white 94 ; white spectrum, 94 dB at 1kHz

;id   position    directivity  aim-position [roll]
 A1  2.95 8.4 0.2     OMNI     0.0 d/2 1.41
 Lp1m_a   = Lp_white 94 ; white spectrum, 94 dB at 1kHz

; an electro-acoustical source (syntax 1 specifying Gain_a)
;B0  -2.0 3.0 3.7  Catt.SD0  0.0 7.0 1.7
; Lp1m_a   = Lp_voice_normal
; Gain_a   = <20 20 20 20 20 20> ; calculates Lp1m_ea
; Delay_e  = 0

; an electro-acoustical source (syntax 2 specifying Lp1m_ea)
; B1   2.0 3.0 3.7  Catt.SD0  0.0 7.0 1.7
; Lp1m_a   = Lp_voice_normal
; Lp1m_ea  = <75 80 82 85 88 88>  ; at 1m on source axis
; Delay_e  = 0

