/COM,ANSYS RELEASE 12.1    UP20091102       15:26:14    11/26/2010

 *** WARNING ***                         CP =       1.203   TIME= 15:26:18
 Using 1 iteration per substep may result in unconverged solutions for   
 nonlinear analysis and the program may not indicate divergence in this  
 case.  Check your results.                                              

 *** WARNING ***                         CP =       1.312   TIME= 15:26:18
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** WARNING ***                         CP =       1.734   TIME= 15:26:18
 Material number 7 (used by element 13251 ) should normally have at      
 least one MP or one TB type command associated with it.  Output of      
 energy by material may not be available.                                
