generator : "PAM-RTM 2010.0";
format_version : 2010.0;
date : "Fri Jun 03 16:26:03 2011";
injected_resin : "Default Resin";
General_Parameters {
	geometry_file : "Prueba3_salpi.unv";
	simulation_type : isothermal_filling;
	simulation_description : "";
	output_format : ideas_universal;
	sampling_period : 10;
	recover_sampling_period : 500;
	max_experiment_time : 1.000000E+006;
	fixed_dt_max : 1.000000E+025;
	max_nb_steps : 1000000;
	overfill_factor : 1.200000E+000;
	use_gravity : 0;
	gravity_x : 0.000000E+000;
	gravity_y : 0.000000E+000;
	gravity_z : -1.000000E+000;
	gravity_norm : 9.800000E+000;
	use_thermal_dispersion : 0;
	use_kinetic : 1;
	initial_fibers_temperature : 3.000000E+002;
	initial_mold_temperature : 3.000000E+002;
	initial_resin_cure : 1.000000E-005;
	save_filling : 0;
	save_filling_compact : 1;
	save_pressure : 1;
	save_porosity : 0;
	save_fiber_content : 0;
	save_thickness : 0;
	save_permeability : 0;
	save_velocity : 0;
	save_temperature : 0;
	save_curing : 0;
	save_exothermy : 0;
	save_capillary_numbers : 0;
	save_closing_force : 0;
	use_local_thickness_file : 0;
	use_local_porosity_file : 0;
	use_local_permeability_files : 0;
	use_temperature_dof_file : 0;
	temperature_dof_file : "noname.dof";
	use_extent_of_cure_dof_file : 0;
	extent_of_cure_dof_file : "noname.dof";
	continue_overfilling : 0;
	overfilling_time : 3.000000E+002;
	overfilling_steps : 100;
	continue_curing : 0;
	curing_stop_option : max_curing_time;
	degree_of_cure_target : 1.000000E+000;
	curing_time : 3.600000E+003;
	curing_time_step : 1.000000E+000;
	one_shot : 0;
	use_pro_solver : 0;
	use_genports : 0;
}
material {
	name : "Default Resin";
	family : material;
	type : resin;
	density : 1.000000E+003;
	nb_vars_specific_heat : 0;
	specific_heat {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 7.000000E+002;
	}
	nb_vars_thermal_conductivity_K1 : 0;
	thermal_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K2 : 0;
	thermal_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K3 : 0;
	thermal_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_viscosity : 0;
	viscosity_func {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
}
material {
	name : "Default Fabric";
	family : material;
	type : reinforcement;
	density : 1.000000E+003;
	nb_vars_specific_heat : 0;
	specific_heat {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 7.000000E+002;
	}
	nb_vars_thermal_conductivity_K1 : 0;
	thermal_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K2 : 0;
	thermal_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K3 : 0;
	thermal_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	reinforcement_type : fabric;
	permeability_curve_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	permeability_curve_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	permeability_curve_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K1_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K2_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K3_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Rotation_Angle_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 0.000000E+000;
	}
	nb_vars_effective_conductivity_k1 : 0;
	effective_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	nb_vars_effective_conductivity_K2 : 0;
	effective_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	nb_vars_effective_conductivity_k3 : 0;
	effective_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	characteristic_length : 0.000000E+000;
	natural_thickness : 5.000000E-003;
	superficial_density : 0.000000E+000;
	compressibility_curve_format : stress_strain;
	compressibility_curve {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 0.000000E+000;
	}
	locking_angle : 9.000000E+001;
}
material {
	name : "Default UD";
	family : material;
	type : reinforcement;
	density : 1.000000E+003;
	nb_vars_specific_heat : 0;
	specific_heat {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 7.000000E+002;
	}
	nb_vars_thermal_conductivity_K1 : 0;
	thermal_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K2 : 0;
	thermal_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K3 : 0;
	thermal_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	reinforcement_type : ud;
	permeability_curve_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	permeability_curve_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	permeability_curve_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K1_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K2_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Permeability_K3_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 1.000000E-009;
	}
	Sheared_Rotation_Angle_Alpha_FC {
		family : function;
		name : noname;
		nb_ind_vars : 2;
		type : Constant;
		C : 0.000000E+000;
	}
	nb_vars_effective_conductivity_k1 : 0;
	effective_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	nb_vars_effective_conductivity_K2 : 0;
	effective_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	nb_vars_effective_conductivity_k3 : 0;
	effective_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 3.000000E-001;
	}
	characteristic_length : 0.000000E+000;
	natural_thickness : 5.000000E-003;
	superficial_density : 0.000000E+000;
	compressibility_curve_format : stress_strain;
	compressibility_curve {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 0.000000E+000;
	}
	grid_stretch : 2.000000E+002;
	grid_shear : 1.050000E+002;
}
material {
	name : "Default Laminate";
	family : material;
	type : laminate;
	density : 1.000000E+003;
	nb_vars_specific_heat : 0;
	specific_heat {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 7.000000E+002;
	}
	nb_vars_thermal_conductivity_K1 : 0;
	thermal_conductivity_k1 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K2 : 0;
	thermal_conductivity_k2 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	nb_vars_thermal_conductivity_K3 : 0;
	thermal_conductivity_k3 {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 1.000000E-001;
	}
	 {
		family : layer;
		index : 0;
		material_name : "Default Fabric";
		angle : 0.000000E+000;
		thickness : 1.000000E-003;
		porosity : 5.000000E-001;
		shear_angle : 0.000000E+000;
	}
}
zone_1 {
	family : zone;
	zone_id : 1;
	zone_name : "Thin Shell1";
	material_name : "Default Fabric";
	zone_porosity : 0.700000;
	shell_thickness : 0.003000;
}
group {
	family : group;
	group_name : "unspecified";
	group_id : 1;
	group_type : pressure;
	{
		family : group_coefficient;
		name : Pressure;
		curve {
			family : function;
			name : noname;
			nb_ind_vars : 1;
			type : Constant;
			C : 1.000000E+005;
		}
	}
	{
		family : group_coefficient;
		name : State;
		curve {
			family : function;
			name : noname;
			nb_ind_vars : 1;
			type : Constant;
			C : 1.000000E+000;
		}
	}
	{
		family : group_coefficient;
		name : Resin_Temperature;
		curve {
			family : function;
			name : noname;
			nb_ind_vars : 1;
			type : Constant;
			C : 3.000000E+002;
		}
	}
	max_pressure : 2.00000E+006;
}
sensor {
	family : sensor;
	name : "Sensor 1";
	x : 4.824000E-001;
	y : 1.712011E-001;
	z : 2.811123E-001;
	element_id : 828;
}
sensor {
	family : sensor;
	name : "Sensor 2";
	x : 6.905000E-001;
	y : 1.712011E-001;
	z : 2.811118E-001;
	element_id : 627;
}
sensor {
	family : sensor;
	name : "Sensor 3";
	x : 3.750000E-001;
	y : 1.691030E-001;
	z : 1.844700E-001;
	element_id : 1987;
}
sensor {
	family : sensor;
	name : "Sensor 4";
	x : 8.021000E-001;
	y : 1.709993E-001;
	z : 1.846225E-001;
	element_id : 6895;
}
sensor {
	family : sensor;
	name : "Sensor 5";
	x : 8.624000E-002;
	y : 1.692024E-001;
	z : 1.844757E-001;
	element_id : 1927;
}
sensor {
	family : sensor;
	name : "Sensor 6";
	x : 1.082000E+000;
	y : 1.710990E-001;
	z : 1.846320E-001;
	element_id : 6833;
}
void_opt_parameters {
	compute_injection_rate_optm : 0;
	resin_capillary_coef : 2.000000E-002;
	optimum_capillary_nbr : 6.900000E-003;
	max_optim_capillary_iter : 3;
	optim_tolerance : 1.000000E-004;
	micro_voids {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 0.000000E+000;
	}
	macro_voids {
		family : function;
		name : noname;
		nb_ind_vars : 1;
		type : Constant;
		C : 0.000000E+000;
	}
}
GenPorts_Parameters {
	nb_inlets : 1;
	nb_generations : 2000;
	population : 100;
	prob_mutation : 4.000000E-001;
	steady_gen : 30;
}
darcy_solver {
	solver : cg;
	preconditioner : diag;
	preconditioner_2 : diag;
	max_iter : 1000;
	tolerance : 1.000000E-005;
	eig_min : 1.000000E-002;
	eig_max : 3.000000E+000;
	gmres_restart : 32;
}
thermic_solver {
	solver : gmres;
	preconditioner : ilu;
	preconditioner_2 : diag;
	max_iter : 1000;
	tolerance : 1.000000E-007;
	eig_min : 1.000000E-002;
	eig_max : 3.000000E+000;
	gmres_restart : 32;
}
