INTERFACE_FILE_VERSION: 2.0.0
3DFLOW_PROGRAM_VERSION: flow analysis ami2010-ma09034-001 09034-001
EXECUTION_DATE_TIME: Sat Aug 27 12:29:18 2011
# Model Information
PLASTIC_MODEL: placa_persiana_aluminio_(n=0_3)_automatico.udm
PLASTIC_MODEL_PROJECTED_AREA: 0.09
PLASTIC_MODEL_VOLUME: 0.000410368
# Machine Information
# Material Information
MATERIAL_DATABASE: Generic PP : Generic Default #3
MATERIAL_SUPPLIER: Dani
MATERIAL_GRADE: VI(240)76
MATERIAL_VISCOSITY_MODEL: Cross-WLF viscosity
MATERIAL_PVT_MODEL: 2-domain modified Tait material pvT
3DFLOW_EXTENSIONAL_VISCOSITY: OFF
MATERIAL_MOLD_TEMPERATURE_RANGE:  100 120
MATERIAL_MELT_TEMPERATURE_RANGE:  525 560
# Machine Setup Information
MOLD_TEMPERATURE: 120
MELT_TEMPERATURE: 650
INJECTION_TIME: 0.005
3DFLOW_FILL_INJECTION_PROFILE_FLOW_VOL:  \
0 0 \
0 1 \
1 1
3DFLOW_FILL_INJECTION_PROFILE_FLOW_VOL_NOMINAL_FLOW_RATE: 0.0820736
3DFLOW_RESULT_FILL_TIME: 0.0835167
3DFLOW_RESULT_MAXIMUM_PRESSURE_END_OF_FILL: 150073
3DFLOW_RESULT_ADDITIONAL_PACKING_TIME: 0
3DFLOW_RESULT_ADDITIONAL_COOLING_TIME: 0.75
3DFLOW_VELOCITY_PHASE: COMPLETE
# Machine Information
MACHINE_IDENTIFICATION_CODE: Default injection molding machine
MACHINE_MANUFACTURER: n/a
MACHINE_MANUFACTURER_MODEL_CODE: Default molding machine
MACHINE_MANUFACTURED_YEAR: 
MACHINE_INJECTION_MAXIMUM_INJECTION_PRESSURE: 1.8e+008
MACHINE_INJECTION_MAXIMUM_INJECTION_VELOCITY: 
MACHINE_INJECTION_CARRIAGE_STROKE: 
MACHINE_INJECTION_RESPONSE_TIME: 0.01
MACHINE_INJECTION_SCREW_INTENSIFICATION_RATIO: 10
MACHINE_INJECTION_SCREW_DIAMETER: 
MACHINE_INJECTION_SCREW_MAXIMUM_STROKE: 
MACHINE_INJECTION_SCREW_MAXIMUM_SPEED: 
MACHINE_CLAMP: HYDRAULIC
MACHINE_CLAMP_MAXIMUM_CLAMP_FORCE: 6.867e+007
MACHINE_CLAMP_PLATEN_HORIZONTAL_SIZE: 
MACHINE_CLAMP_PLATEN_VERTICAL_SIZE: 
MACHINE_CLAMP_PLATEN_MAXIMUM_DAYLIGHT: 
MACHINE_CLAMP_TIE_BAR_CLEARANCE_HORIZONTAL: 
MACHINE_CLAMP_TIE_BAR_CLEARANCE_VERTICAL: 
MACHINE_CLAMP_DIE_HEIGHT_MAXIMUM: 
MACHINE_CLAMP_DIE_HEIGHT_MINIMUM: 
MACHINE_CLAMP_EJECTOR_FORCE: 
MACHINE_CLAMP_EJECTOR_STROKE: 
MACHINE_CONTROLLER_CODE: Process controller defaults
MACHINE_CONTROLLER_MAXIMUM_VELOCITY_STEPS: 10
MACHINE_CONTROLLER_VELOCITY_PROFILE_TYPES_CONSTANT: OFF
MACHINE_CONTROLLER_VELOCITY_PROFILE_TYPES_LINEAR: ON
MACHINE_CONTROLLER_VELOCITY_PROFILE_RAM_POSITION_RAM_VELOCITY: ON
MACHINE_CONTROLLER_VELOCITY_PROFILE_ZONE_RAM_VELOCITY: OFF
MACHINE_CONTROLLER_MAXIMUM_PRESSURE_STEPS:       10
MACHINE_CONTROLLER_PRESSURE_PROFILE_TYPES_CONSTANT: OFF
MACHINE_CONTROLLER_PRESSURE_PROFILE_TYPES_LINEAR: ON
MACHINE_CONTROLLER_PRESSURE_PROFILE_PRESSURE_TIME: ON
MACHINE_CONTROLLER_PRESSURE_PROFILE_ZONE_PRESSURE: OFF
