Static Call Graph - [.\Targets\STM32F4_Discovery\project.axf]

# Static Call Graph for image .\Targets\STM32F4_Discovery\project.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Sat Feb 18 17:04:02 2017

### Maximum Stack Usage = 120 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

USBD_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FPU_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - FSMC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PVD_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RCC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - Reset_Handler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f40_41xxx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART4_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - UART5_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART1_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART2_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART3_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USART6_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - USBD_DataInStage from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_DataOutStage from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_IsoINIncomplete from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_IsoOUTIncomplete from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_Reset from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_Resume from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_SOF from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_SetupStage from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_Suspend from usbd_core.o(.text) referenced 2 times from usbd_core.o(.data)
  - USBD_USR_ConfigStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_DeviceConfigured from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_DeviceConnected from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_DeviceDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_DeviceDisconnected from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_DeviceReset from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_DeviceResumed from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_DeviceSuspended from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_Init from usbd_usr.o(.text) referenced 2 times from usbd_usr.o(.data)
  - USBD_USR_InterfaceStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_LangIDStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_ManufacturerStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_ProductStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_USR_SerialStrDescriptor from usbd_desc.o(.text) referenced 2 times from usbd_desc.o(.data)
  - USBD_cdc_GetCfgDesc from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - VCP_Ctrl from usbd_cdc_vcp.o(.text) referenced 2 times from usbd_cdc_vcp.o(.data)
  - VCP_DataRx from usbd_cdc_vcp.o(.text) referenced 2 times from usbd_cdc_vcp.o(.data)
  - VCP_DataTx from usbd_cdc_vcp.o(.text) referenced 2 times from usbd_cdc_vcp.o(.data)
  - VCP_DeInit from usbd_cdc_vcp.o(.text) referenced 2 times from usbd_cdc_vcp.o(.data)
  - VCP_Init from usbd_cdc_vcp.o(.text) referenced 2 times from usbd_cdc_vcp.o(.data)
  - WWDG_IRQHandler from startup_stm32f40_41xxx.o(.text) referenced from startup_stm32f40_41xxx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f40_41xxx.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - usbd_cdc_DataIn from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_DataOut from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_DeInit from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_EP0_RxReady from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_Init from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_SOF from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)
  - usbd_cdc_Setup from usbd_cdc_core.o(.text) referenced 2 times from usbd_cdc_core.o(.data)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  OTG_HS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f40_41xxx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text))
  [Called By]

  - >> USB_OTG_BSP_EnableInterrupt

  NVIC_Init (Thumb, 96 bytes, Stack size 12 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> USB_OTG_BSP_EnableInterrupt

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 20 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  RCC_DeInit (Thumb, 68 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> TM_DELAY_Init

  RCC_GetFlagStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 44 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Calls]

  - >> RCC_GetFlagStatus
  [Called By]
  - >> TM_DELAY_Init

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 134 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_DISCO_ButtonInit
  - >> TM_DISCO_LedInit
  - >> USB_OTG_BSP_Init

  RCC_AHB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USB_OTG_BSP_Init

  RCC_AHB3PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USB_OTG_BSP_Init

  RCC_AHB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 64 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 216 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 120 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> TM_DISCO_ButtonInit
  - >> TM_DISCO_LedInit
  - >> USB_OTG_BSP_Init

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> USB_OTG_BSP_Init

  EXTI_DeInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 108 bytes, Stack size 12 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_StructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> OTG_FS_WKUP_IRQHandler

  TimingDelay_Decrement (Thumb, 26 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TimingDelay_Decrement
  [Called By]
  - >> SysTick_Handler

  TM_DELAY_Init (Thumb, 82 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text), UNUSED)
  [Calls]

  - >> RCC_WaitForHSEStartUp
  - >> RCC_HSEConfig

  TM_DELAY_EnableDelayTimer (Thumb, 22 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DELAY_DisableDelayTimer (Thumb, 14 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DISCO_LedInit (Thumb, 48 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TM_DISCO_LedInit ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  TM_DISCO_ButtonInit (Thumb, 44 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd

  TM_DISCO_ButtonOnPressed (Thumb, 26 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  TM_DISCO_ButtonOnReleased (Thumb, 26 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  main (Thumb, 62 bytes, Stack size 8 bytes, main.o(.text))
  [Stack]

  - Max Depth = 96
  - Call Chain = main ⇒ TM_USB_VCP_Init ⇒ USBD_Init ⇒ DCD_Init ⇒ USB_OTG_CoreInitDev ⇒ USB_OTG_FlushRxFifo
  [Calls]
  - >> TM_DISCO_LedInit
  - >> SystemInit
  - >> TM_USB_VCP_Putc
  - >> TM_USB_VCP_Init
  - >> TM_USB_VCP_Getc
  - >> TM_USB_VCP_GetStatus
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f40_41xxx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ TimingDelay_Decrement
  [Calls]
  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Called By]
  - >> main
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(.text)

  SystemCoreClockUpdate (Thumb, 108 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  TM_USB_VCP_Init (Thumb, 36 bytes, Stack size 8 bytes, tm_stm32f4_usb_vcp.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = TM_USB_VCP_Init ⇒ USBD_Init ⇒ DCD_Init ⇒ USB_OTG_CoreInitDev ⇒ USB_OTG_FlushRxFifo
  [Calls]
  - >> USBD_Init
  [Called By]
  - >> main

  TM_USB_VCP_BufferEmpty (Thumb, 14 bytes, Stack size 0 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Called By]

  - >> TM_USB_VCP_Gets

  TM_USB_VCP_BufferFull (Thumb, 16 bytes, Stack size 0 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Called By]

  - >> TM_USB_VCP_Gets

  TM_USB_VCP_FindCharacter (Thumb, 54 bytes, Stack size 12 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Called By]

  - >> TM_USB_VCP_Gets

  TM_USB_VCP_Getc (Thumb, 52 bytes, Stack size 8 bytes, tm_stm32f4_usb_vcp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TM_USB_VCP_Getc
  [Called By]
  - >> TM_USB_VCP_Gets
  - >> main

  TM_USB_VCP_Putc (Thumb, 24 bytes, Stack size 16 bytes, tm_stm32f4_usb_vcp.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TM_USB_VCP_Putc ⇒ VCP_DataTx
  [Calls]
  - >> VCP_DataTx
  [Called By]
  - >> TM_USB_VCP_Puts
  - >> main

  TM_USB_VCP_Puts (Thumb, 20 bytes, Stack size 8 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Calls]

  - >> TM_USB_VCP_Putc

  TM_USB_VCP_Send (Thumb, 10 bytes, Stack size 8 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Calls]

  - >> VCP_DataTx

  TM_USB_VCP_Gets (Thumb, 72 bytes, Stack size 20 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)
  [Calls]

  - >> TM_USB_VCP_FindCharacter
  - >> TM_USB_VCP_BufferFull
  - >> TM_USB_VCP_BufferEmpty
  - >> TM_USB_VCP_Getc

  TM_INT_USB_VCP_AddReceived (Thumb, 42 bytes, Stack size 8 bytes, tm_stm32f4_usb_vcp.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TM_INT_USB_VCP_AddReceived
  [Called By]
  - >> VCP_DataRx

  TM_USB_VCP_GetStatus (Thumb, 16 bytes, Stack size 0 bytes, tm_stm32f4_usb_vcp.o(.text))
  [Called By]

  - >> main

  TM_USB_VCP_GetSettings (Thumb, 28 bytes, Stack size 0 bytes, tm_stm32f4_usb_vcp.o(.text), UNUSED)

  USB_OTG_BSP_Init (Thumb, 154 bytes, Stack size 32 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = USB_OTG_BSP_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> USBD_Init

  USB_OTG_BSP_EnableInterrupt (Thumb, 40 bytes, Stack size 8 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_OTG_BSP_EnableInterrupt ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> USBD_Init

  USB_OTG_BSP_uDelay (Thumb, 22 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Called By]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo
  - >> USB_OTG_CoreReset
  - >> USB_OTG_BSP_mDelay

  USB_OTG_BSP_mDelay (Thumb, 8 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Calls]

  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> DCD_DevDisconnect
  - >> DCD_DevConnect
  - >> USB_OTG_ActiveRemoteWakeup
  - >> USB_OTG_SetCurrentMode
  - >> USB_OTG_CoreInit

  OTG_FS_WKUP_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Calls]

  - >> EXTI_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = OTG_FS_IRQHandler ⇒ USBD_OTG_ISR_Handler ⇒ DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_OTG_ISR_Handler
  [Address Reference Count : 1]
  - startup_stm32f40_41xxx.o(RESET)

  USB_OTG_WritePacket (Thumb, 40 bytes, Stack size 12 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_OTG_WritePacket
  [Called By]
  - >> DCD_WriteEmptyTxFifo
  - >> USB_OTG_EPStartXfer

  USB_OTG_ReadPacket (Thumb, 32 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_ReadPacket
  [Called By]
  - >> DCD_HandleRxStatusQueueLevel_ISR

  USB_OTG_SelectCore (Thumb, 188 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_OTG_SelectCore
  [Called By]
  - >> DCD_Init

  USB_OTG_CoreInit (Thumb, 128 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = USB_OTG_CoreInit ⇒ USB_OTG_CoreReset
  [Calls]
  - >> USB_OTG_CoreReset
  - >> USB_OTG_BSP_mDelay
  [Called By]
  - >> DCD_Init

  USB_OTG_EnableGlobalInt (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_Init

  USB_OTG_DisableGlobalInt (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_Init

  USB_OTG_FlushTxFifo (Thumb, 62 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_OTG_FlushTxFifo
  [Calls]
  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_EP_Flush
  - >> USB_OTG_StopDevice
  - >> USB_OTG_CoreInitDev

  USB_OTG_FlushRxFifo (Thumb, 54 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_OTG_FlushRxFifo
  [Calls]
  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> DCD_EP_Flush
  - >> USB_OTG_StopDevice
  - >> USB_OTG_CoreInitDev

  USB_OTG_SetCurrentMode (Thumb, 42 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_SetCurrentMode
  [Calls]
  - >> USB_OTG_BSP_mDelay
  [Called By]
  - >> DCD_Init

  USB_OTG_GetMode (Thumb, 10 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_IsDeviceMode (Thumb, 18 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_IsHostMode (Thumb, 14 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_ReadCoreItr (Thumb, 10 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_ReadOtgItr (Thumb, 6 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_InitDevSpeed (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USB_OTG_CoreInitDev

  USB_OTG_EnableDevInt (Thumb, 66 bytes, Stack size 12 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_OTG_EnableDevInt
  [Called By]
  - >> USB_OTG_CoreInitDev

  USB_OTG_CoreInitDev (Thumb, 312 bytes, Stack size 24 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = USB_OTG_CoreInitDev ⇒ USB_OTG_FlushRxFifo
  [Calls]
  - >> USB_OTG_EnableDevInt
  - >> USB_OTG_InitDevSpeed
  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo
  [Called By]
  - >> DCD_Init

  USB_OTG_GetDeviceSpeed (Thumb, 38 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_EP0Activate (Thumb, 58 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_EP0Activate
  [Called By]
  - >> USBD_OTG_ISR_Handler

  USB_OTG_EPActivate (Thumb, 82 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_OTG_EPActivate
  [Called By]
  - >> DCD_EP_Open

  USB_OTG_EPDeactivate (Thumb, 52 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_OTG_EPDeactivate
  [Called By]
  - >> DCD_EP_Close

  USB_OTG_EPStartXfer (Thumb, 298 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_WritePacket
  [Called By]
  - >> DCD_EP_Tx
  - >> DCD_EP_PrepareRx

  USB_OTG_EP0StartXfer (Thumb, 184 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_OTG_EP0StartXfer
  [Called By]
  - >> DCD_EP_Tx
  - >> DCD_EP_PrepareRx

  USB_OTG_EPSetStall (Thumb, 48 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_EP_Stall
  - >> USB_OTG_SetEPStatus

  USB_OTG_EPClearStall (Thumb, 50 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_EPClearStall
  [Called By]
  - >> DCD_EP_ClrStall
  - >> USB_OTG_SetEPStatus

  USB_OTG_ReadDevAllOutEp_itr (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleOutEP_ISR

  USB_OTG_ReadDevOutEP_itr (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleOutEP_ISR

  USB_OTG_ReadDevAllInEPItr (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleInEP_ISR

  USB_OTG_EP0_OutStart (Thumb, 32 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_CtlSendStatus
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlError
  - >> DCD_HandleOutEP_ISR
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_HandleInEP_ISR

  USB_OTG_ActiveRemoteWakeup (Thumb, 66 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  USB_OTG_UngateClock (Thumb, 30 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_StopDevice (Thumb, 72 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo

  USB_OTG_GetEPStatus (Thumb, 66 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_GetEPStatus

  USB_OTG_SetEPStatus (Thumb, 106 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_EPClearStall
  - >> USB_OTG_EPSetStall
  [Called By]
  - >> DCD_SetEPStatus

  DCD_Init (Thumb, 146 bytes, Stack size 16 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = DCD_Init ⇒ USB_OTG_CoreInitDev ⇒ USB_OTG_FlushRxFifo
  [Calls]
  - >> USB_OTG_CoreInitDev
  - >> USB_OTG_SetCurrentMode
  - >> USB_OTG_DisableGlobalInt
  - >> USB_OTG_EnableGlobalInt
  - >> USB_OTG_CoreInit
  - >> USB_OTG_SelectCore
  [Called By]
  - >> USBD_Init

  DCD_EP_Open (Thumb, 60 bytes, Stack size 16 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = DCD_EP_Open ⇒ USB_OTG_EPActivate
  [Calls]
  - >> USB_OTG_EPActivate
  [Called By]
  - >> USBD_Reset
  - >> usbd_cdc_Init

  DCD_EP_Close (Thumb, 44 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DCD_EP_Close ⇒ USB_OTG_EPDeactivate
  [Calls]
  - >> USB_OTG_EPDeactivate
  [Called By]
  - >> usbd_cdc_DeInit

  DCD_EP_PrepareRx (Thumb, 68 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0StartXfer
  - >> USB_OTG_EPStartXfer
  [Called By]
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueRx
  - >> USBD_CtlPrepareRx
  - >> usbd_cdc_DataOut
  - >> usbd_cdc_Init

  DCD_EP_Tx (Thumb, 62 bytes, Stack size 16 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0StartXfer
  - >> USB_OTG_EPStartXfer
  [Called By]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueSendData
  - >> USBD_CtlSendData
  - >> Handle_USBAsynchXfer
  - >> usbd_cdc_DataIn

  DCD_EP_Stall (Thumb, 56 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DCD_EP_Stall
  [Calls]
  - >> USB_OTG_EPSetStall
  [Called By]
  - >> USBD_StdEPReq
  - >> USBD_SetupStage
  - >> USBD_CtlError

  DCD_EP_ClrStall (Thumb, 56 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DCD_EP_ClrStall ⇒ USB_OTG_EPClearStall
  [Calls]
  - >> USB_OTG_EPClearStall
  [Called By]
  - >> USBD_StdEPReq

  DCD_EP_Flush (Thumb, 24 bytes, Stack size 8 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo

  DCD_EP_SetAddress (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text))
  [Called By]

  - >> USBD_StdDevReq

  DCD_DevConnect (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  DCD_DevDisconnect (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  DCD_GetEPStatus (Thumb, 38 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_GetEPStatus

  DCD_SetEPStatus (Thumb, 38 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_SetEPStatus

  USBD_OTG_ISR_Handler (Thumb, 326 bytes, Stack size 32 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = USBD_OTG_ISR_Handler ⇒ DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_HandleOutEP_ISR
  - >> DCD_HandleUSBSuspend_ISR
  - >> DCD_HandleRxStatusQueueLevel_ISR
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_HandleInEP_ISR
  - >> USB_OTG_EP0Activate
  - >> USB_OTG_GetDeviceSpeed
  - >> USB_OTG_ReadCoreItr
  - >> USB_OTG_IsDeviceMode
  [Called By]
  - >> OTG_FS_IRQHandler

  VCP_DataTx (Thumb, 42 bytes, Stack size 20 bytes, usbd_cdc_vcp.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = VCP_DataTx
  [Called By]
  - >> TM_USB_VCP_Send
  - >> TM_USB_VCP_Putc
  [Address Reference Count : 1]
  - usbd_cdc_vcp.o(.data)

  VCP_DataRx (Thumb, 26 bytes, Stack size 16 bytes, usbd_cdc_vcp.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = VCP_DataRx ⇒ TM_INT_USB_VCP_AddReceived
  [Calls]
  - >> TM_INT_USB_VCP_AddReceived
  [Address Reference Count : 1]
  - usbd_cdc_vcp.o(.data)

  USBD_DeInit (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(.text), UNUSED)

  USBD_Init (Thumb, 52 bytes, Stack size 24 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_Init ⇒ DCD_Init ⇒ USB_OTG_CoreInitDev ⇒ USB_OTG_FlushRxFifo
  [Calls]
  - >> DCD_Init
  - >> USB_OTG_BSP_EnableInterrupt
  - >> USB_OTG_BSP_Init
  [Called By]
  - >> TM_USB_VCP_Init

  USBD_SetCfg (Thumb, 26 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SetCfg
  [Called By]
  - >> USBD_SetConfig

  USBD_ClrCfg (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_ClrCfg
  [Called By]
  - >> USBD_SetConfig

  USBD_USR_DeviceDescriptor (Thumb, 8 bytes, Stack size 0 bytes, usbd_desc.o(.text))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_USR_LangIDStrDescriptor (Thumb, 10 bytes, Stack size 0 bytes, usbd_desc.o(.text))
  [Address Reference Count : 1]

  - usbd_desc.o(.data)

  USBD_USR_ProductStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_USR_ProductStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_USR_ManufacturerStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_USR_ManufacturerStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_USR_SerialStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_USR_SerialStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_USR_ConfigStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_USR_ConfigStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_USR_InterfaceStrDescriptor (Thumb, 16 bytes, Stack size 8 bytes, usbd_desc.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USBD_USR_InterfaceStrDescriptor ⇒ USBD_GetString
  [Calls]
  - >> USBD_GetString
  [Address Reference Count : 1]
  - usbd_desc.o(.data)

  USBD_CtlSendData (Thumb, 32 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Called By]
  - >> USBD_GetDescriptor
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> usbd_cdc_Setup

  USBD_CtlContinueSendData (Thumb, 18 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlContinueSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Called By]
  - >> USBD_DataInStage

  USBD_CtlPrepareRx (Thumb, 32 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_CtlPrepareRx ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  [Called By]
  - >> usbd_cdc_Setup

  USBD_CtlContinueRx (Thumb, 18 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_CtlContinueRx ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  [Called By]
  - >> USBD_DataOutStage

  USBD_CtlSendStatus (Thumb, 34 bytes, Stack size 16 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  - >> USB_OTG_EP0_OutStart
  [Called By]
  - >> USBD_SetFeature
  - >> USBD_SetConfig
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_DataOutStage

  USBD_CtlReceiveStatus (Thumb, 34 bytes, Stack size 16 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlReceiveStatus ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  - >> USB_OTG_EP0_OutStart
  [Called By]
  - >> USBD_DataInStage

  USBD_GetRxCount (Thumb, 16 bytes, Stack size 0 bytes, usbd_ioreq.o(.text), UNUSED)

  USBD_CtlError (Thumb, 28 bytes, Stack size 8 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_CtlError ⇒ DCD_EP_Stall
  [Calls]
  - >> DCD_EP_Stall
  - >> USB_OTG_EP0_OutStart
  [Called By]
  - >> USBD_GetDescriptor
  - >> USBD_SetConfig
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> usbd_cdc_Setup

  USBD_StdDevReq (Thumb, 236 bytes, Stack size 24 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = USBD_StdDevReq ⇒ USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_SetFeature
  - >> USBD_GetDescriptor
  - >> USBD_SetConfig
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> DCD_EP_SetAddress
  [Called By]
  - >> USBD_SetupStage

  USBD_StdItfReq (Thumb, 54 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdItfReq ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlError
  [Called By]
  - >> USBD_SetupStage

  USBD_StdEPReq (Thumb, 208 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdEPReq ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> DCD_EP_ClrStall
  - >> DCD_EP_Stall
  [Called By]
  - >> USBD_SetupStage

  USBD_ParseSetupRequest (Thumb, 68 bytes, Stack size 0 bytes, usbd_req.o(.text))
  [Called By]

  - >> USBD_SetupStage

  USBD_GetString (Thumb, 70 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_GetString
  [Called By]
  - >> USBD_USR_InterfaceStrDescriptor
  - >> USBD_USR_ConfigStrDescriptor
  - >> USBD_USR_SerialStrDescriptor
  - >> USBD_USR_ManufacturerStrDescriptor
  - >> USBD_USR_ProductStrDescriptor

  USBD_USR_Init (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceReset (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceConfigured (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceSuspended (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceResumed (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceConnected (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_USR_DeviceDisconnected (Thumb, 8 bytes, Stack size 0 bytes, usbd_usr.o(.text))
  [Address Reference Count : 1]

  - usbd_usr.o(.data)

  USBD_User_GetStatus (Thumb, 6 bytes, Stack size 0 bytes, usbd_usr.o(.text), UNUSED)

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __decompress (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __decompress1 (Thumb, 86 bytes, Stack size unknown bytes, __dczerorl2.o(.text), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  ### Local Symbols

  SetSysClock (Thumb, 162 bytes, Stack size 12 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  USB_OTG_CoreReset (Thumb, 84 bytes, Stack size 24 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = USB_OTG_CoreReset
  [Calls]
  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> USB_OTG_CoreInit

  DCD_HandleInEP_ISR (Thumb, 198 bytes, Stack size 24 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_WriteEmptyTxFifo
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_ReadDevAllInEPItr
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleUsbReset_ISR (Thumb, 128 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = DCD_HandleUsbReset_ISR ⇒ USB_OTG_FlushTxFifo
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_FlushTxFifo
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleRxStatusQueueLevel_ISR (Thumb, 124 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DCD_HandleRxStatusQueueLevel_ISR ⇒ USB_OTG_ReadPacket
  [Calls]
  - >> USB_OTG_ReadPacket
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleUSBSuspend_ISR (Thumb, 102 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DCD_HandleUSBSuspend_ISR
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_WriteEmptyTxFifo (Thumb, 112 bytes, Stack size 32 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_WritePacket
  [Called By]
  - >> DCD_HandleInEP_ISR

  DCD_HandleOutEP_ISR (Thumb, 174 bytes, Stack size 24 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DCD_HandleOutEP_ISR
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_ReadDevOutEP_itr
  - >> USB_OTG_ReadDevAllOutEp_itr
  [Called By]
  - >> USBD_OTG_ISR_Handler

  usbd_cdc_Init (Thumb, 70 bytes, Stack size 8 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = usbd_cdc_Init ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  - >> DCD_EP_Open
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  usbd_cdc_DeInit (Thumb, 36 bytes, Stack size 8 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = usbd_cdc_DeInit ⇒ DCD_EP_Close ⇒ USB_OTG_EPDeactivate
  [Calls]
  - >> DCD_EP_Close
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  usbd_cdc_Setup (Thumb, 174 bytes, Stack size 16 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = usbd_cdc_Setup ⇒ USBD_CtlSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlPrepareRx
  - >> USBD_CtlError
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  usbd_cdc_EP0_RxReady (Thumb, 32 bytes, Stack size 8 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = usbd_cdc_EP0_RxReady
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  usbd_cdc_DataIn (Thumb, 68 bytes, Stack size 16 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = usbd_cdc_DataIn ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  usbd_cdc_DataOut (Thumb, 42 bytes, Stack size 8 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = usbd_cdc_DataOut ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  Handle_USBAsynchXfer (Thumb, 96 bytes, Stack size 16 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = Handle_USBAsynchXfer ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Called By]
  - >> usbd_cdc_SOF

  usbd_cdc_SOF (Thumb, 28 bytes, Stack size 8 bytes, usbd_cdc_core.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = usbd_cdc_SOF ⇒ Handle_USBAsynchXfer ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> Handle_USBAsynchXfer
  [Address Reference Count : 1]
  - usbd_cdc_core.o(.data)

  USBD_cdc_GetCfgDesc (Thumb, 10 bytes, Stack size 0 bytes, usbd_cdc_core.o(.text))
  [Address Reference Count : 1]

  - usbd_cdc_core.o(.data)

  VCP_Init (Thumb, 4 bytes, Stack size 0 bytes, usbd_cdc_vcp.o(.text))
  [Address Reference Count : 1]

  - usbd_cdc_vcp.o(.data)

  VCP_DeInit (Thumb, 4 bytes, Stack size 0 bytes, usbd_cdc_vcp.o(.text))
  [Address Reference Count : 1]

  - usbd_cdc_vcp.o(.data)

  VCP_Ctrl (Thumb, 82 bytes, Stack size 0 bytes, usbd_cdc_vcp.o(.text))
  [Address Reference Count : 1]

  - usbd_cdc_vcp.o(.data)

  USBD_SetupStage (Thumb, 72 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = USBD_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_ParseSetupRequest
  - >> DCD_EP_Stall
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_DataOutStage (Thumb, 116 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_DataOutStage ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueRx
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_DataInStage (Thumb, 172 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_DataInStage ⇒ USBD_CtlReceiveStatus ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueSendData
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Reset (Thumb, 46 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_Reset ⇒ DCD_EP_Open ⇒ USB_OTG_EPActivate
  [Calls]
  - >> DCD_EP_Open
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Resume (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_Resume
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Suspend (Thumb, 28 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_Suspend
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_SOF (Thumb, 16 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SOF
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_IsoINIncomplete (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_IsoINIncomplete
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_IsoOUTIncomplete (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_IsoOUTIncomplete
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_SetConfig (Thumb, 110 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_ClrCfg
  - >> USBD_SetCfg
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_GetDescriptor (Thumb, 206 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetFeature (Thumb, 122 bytes, Stack size 8 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_SetFeature ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  ### Undefined Global Symbols