Static Call Graph - [.\Targets\STM32F429_Discovery\project.axf]

# Static Call Graph for image .\Targets\STM32F429_Discovery\project.axf

#<CALLGRAPH># ARM Linker, 5060061: Last Updated: Fri Sep 22 11:19:58 2017

### Maximum Stack Usage = 344 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ trapez4 ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round

### Mutually Recursive functions

- ADC_IRQHandler ⇒ ADC_IRQHandler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- BusFault_Handler ⇒ BusFault_Handler
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - BusFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN1_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_RX1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_SCE_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CAN2_TX_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - CRYP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DCMI_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA1_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2D_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream0_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DMA2_Stream7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - DebugMon_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - ETH_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI0_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI1_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI2_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI3_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI4_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - EXTI9_5_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FLASH_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FMC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - FPU_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HASH_RNG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - HardFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - I2C3_EV_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_ER_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - LTDC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - MemManage_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - NMI_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_FS_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_IN_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_EP1_OUT_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - OTG_HS_WKUP_IRQHandler from usb_bsp.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PVD_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - PendSV_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RCC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - RTC_WKUP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - Reset_Handler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SAI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SDIO_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SPI6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SVC_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SysTick_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - SystemInit from system_stm32f4xx.o(.text) referenced from startup_stm32f429_439xx.o(.text)
  - TAMP_STAMP_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_BRK_TIM9_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_TRG_COM_TIM11_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM1_UP_TIM10_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM2_IRQHandler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM6_DAC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_BRK_TIM12_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_TRG_COM_TIM14_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - TIM8_UP_TIM13_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART4_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART5_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART7_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - UART8_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART1_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART2_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART3_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USART6_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - USBD_DataInStage from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_DataOutStage from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_IsoINIncomplete from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_IsoOUTIncomplete from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_Reset from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_Resume from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_SOF from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_SetupStage from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - USBD_Suspend from usbd_core.o(.text) referenced from usbd_core.o(.data)
  - UsageFault_Handler from stm32f4xx_it.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - WWDG_IRQHandler from startup_stm32f429_439xx.o(.text) referenced from startup_stm32f429_439xx.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f429_439xx.o(.text)
  - main from main.o(.text) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000D))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$0000000F))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ADC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Calls]

  - >> ADC_IRQHandler
  [Called By]
  - >> ADC_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CAN2_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  CRYP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DCMI_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA1_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2D_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DMA2_Stream7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  ETH_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  FPU_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HASH_RNG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  I2C3_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  LTDC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  OTG_FS_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  RTC_WKUP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SAI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SPI6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TAMP_STAMP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_BRK_TIM9_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_TRG_COM_TIM11_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM1_UP_TIM10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM6_DAC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_BRK_TIM12_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_TRG_COM_TIM14_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  TIM8_UP_TIM13_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  UART8_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  USART6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f429_439xx.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)
  [Called By]

  - >> USB_OTG_BSP_EnableInterrupt

  NVIC_Init (Thumb, 96 bytes, Stack size 12 bytes, misc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = NVIC_Init
  [Called By]
  - >> USB_OTG_BSP_EnableInterrupt
  - >> Configure_GPIOF_EXTI
  - >> Control_TimerInit
  - >> Configure_GPIOB_EXTI

  NVIC_SetVectorTable (Thumb, 14 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  NVIC_SystemLPConfig (Thumb, 20 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  SysTick_CLKSourceConfig (Thumb, 24 bytes, Stack size 0 bytes, misc.o(.text), UNUSED)

  RCC_DeInit (Thumb, 68 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSEConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> TM_DELAY_Init

  RCC_GetFlagStatus (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> RCC_WaitForHSEStartUp

  RCC_WaitForHSEStartUp (Thumb, 44 bytes, Stack size 12 bytes, stm32f4xx_rcc.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_GetFlagStatus
  [Called By]
  - >> TM_DELAY_Init

  RCC_AdjustHSICalibrationValue (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLI2SCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAIConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PLLSAICmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClockSecuritySystemCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO1Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_MCO2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SYSCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetSYSCLKSource (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_HCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK1Config (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_PCLK2Config (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetClocksFreq (Thumb, 134 bytes, Stack size 16 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKConfig (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_RTCCLKCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_BackupResetCmd (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_I2SCLKConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockACLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIBlockBCLKConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLI2SClkDivConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_SAIPLLSAIClkDivConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LTDCCLKDivConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_TIMCLKPresConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USB_OTG_BSP_Init
  - >> Configure_GPIOF_EXTI
  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config
  - >> dac_init
  - >> Configure_GPIOB_EXTI
  - >> TM_DISCO_ButtonInit
  - >> TM_DISCO_LedInit

  RCC_AHB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> encoder1_config
  - >> dac_init
  - >> Control_TimerInit

  RCC_APB2PeriphClockCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text))
  [Called By]

  - >> USB_OTG_BSP_Init
  - >> Configure_GPIOF_EXTI
  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> Configure_GPIOB_EXTI

  RCC_AHB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> GPIO_DeInit

  RCC_AHB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> DAC_DeInit
  - >> TIM_DeInit

  RCC_APB2PeriphResetCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)
  [Called By]

  - >> SYSCFG_DeInit
  - >> TIM_DeInit

  RCC_AHB1PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB2PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_AHB3PeriphClockLPModeCmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB1PeriphClockLPModeCmd (Thumb, 64 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_APB2PeriphClockLPModeCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_LSEModeConfig (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ITConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearFlag (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  RCC_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_rcc.o(.text), UNUSED)

  GPIO_DeInit (Thumb, 216 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)
  [Calls]

  - >> RCC_AHB1PeriphResetCmd

  GPIO_Init (Thumb, 120 bytes, Stack size 20 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_Init
  [Called By]
  - >> USB_OTG_BSP_Init
  - >> Configure_GPIOF_EXTI
  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config
  - >> dac_init
  - >> Configure_GPIOB_EXTI
  - >> TM_DISCO_ButtonInit
  - >> TM_DISCO_LedInit

  GPIO_StructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinLockConfig (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadInputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputDataBit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ReadOutputData (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_Write (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_ToggleBits (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_gpio.o(.text), UNUSED)

  GPIO_PinAFConfig (Thumb, 32 bytes, Stack size 8 bytes, stm32f4xx_gpio.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = GPIO_PinAFConfig
  [Called By]
  - >> USB_OTG_BSP_Init
  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config

  EXTI_DeInit (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_Init (Thumb, 108 bytes, Stack size 12 bytes, stm32f4xx_exti.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = EXTI_Init
  [Called By]
  - >> Configure_GPIOF_EXTI
  - >> Configure_GPIOB_EXTI

  EXTI_StructInit (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GenerateSWInterrupt (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetFlagStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_ClearFlag (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text), UNUSED)

  EXTI_GetITStatus (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> EXTI9_5_IRQHandler
  - >> EXTI4_IRQHandler
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler
  - >> EXTI1_IRQHandler
  - >> EXTI0_IRQHandler

  EXTI_ClearITPendingBit (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_exti.o(.text))
  [Called By]

  - >> OTG_HS_WKUP_IRQHandler
  - >> EXTI9_5_IRQHandler
  - >> EXTI4_IRQHandler
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler
  - >> EXTI1_IRQHandler
  - >> EXTI0_IRQHandler

  TIM_DeInit (Thumb, 284 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd
  - >> RCC_APB1PeriphResetCmd

  TIM_TimeBaseInit (Thumb, 96 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_TimeBaseInit
  [Called By]
  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config
  - >> Control_TimerInit

  TIM_TimeBaseStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_PrescalerConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CounterModeConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetAutoreload (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config

  TIM_GetCounter (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> paradacontrolada
  - >> EXTI9_5_IRQHandler
  - >> EXTI4_IRQHandler

  TIM_GetPrescaler (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_UpdateDisableConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_UpdateRequestConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ARRPreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectOnePulseMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetClockDivision (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> PWM
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config
  - >> Control_TimerInit

  TIM_OC1Init (Thumb, 88 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_OC2Init (Thumb, 120 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_OC3Init (Thumb, 116 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_OC4Init (Thumb, 88 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_OCStructInit (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_SelectOCxM (Thumb, 130 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetCompare4 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC1Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC2Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC3Config (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ForcedOC4Config (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1PreloadConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2PreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3PreloadConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4PreloadConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2FastConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3FastConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4FastConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC1Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC2Ref (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC3Ref (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearOC4Ref (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1PolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC1NPolarityConfig (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC2NPolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC3NPolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_OC4PolarityConfig (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCxCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCxNCmd (Thumb, 22 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SetIC4Prescaler (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC3Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ICInit

  TIM_SetIC2Prescaler (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_SetIC1Prescaler (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TIM_ICInit (Thumb, 164 bytes, Stack size 24 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TIM_SetIC3Prescaler
  - >> TIM_SetIC4Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_ICStructInit (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_PWMIConfig (Thumb, 104 bytes, Stack size 24 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SetIC1Prescaler
  - >> TIM_SetIC2Prescaler
  - >> TI1_Config
  - >> TI2_Config

  TIM_GetCapture1 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture2 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture3 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetCapture4 (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_BDTRConfig (Thumb, 34 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_BDTRStructInit (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> PWM

  TIM_CtrlPWMOutputs (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectCOM (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_CCPreloadControl (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ITConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> PWM
  - >> paradacontrolada

  TIM_GenerateEvent (Thumb, 4 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetFlagStatus (Thumb, 14 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_ClearFlag (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_GetITStatus (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> TIM2_IRQHandler

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text))
  [Called By]

  - >> TIM2_IRQHandler

  TIM_DMAConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_DMACmd (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectCCDMA (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_InternalClockConfig (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectInputTrigger (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_ITRxExternalClockConfig

  TIM_ITRxExternalClockConfig (Thumb, 18 bytes, Stack size 4 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger

  TIM_TIxExternalClockConfig (Thumb, 46 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_SelectInputTrigger
  - >> TI1_Config
  - >> TI2_Config

  TIM_ETRConfig (Thumb, 24 bytes, Stack size 12 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_ETRClockMode2Config
  - >> TIM_ETRClockMode1Config

  TIM_ETRClockMode1Config (Thumb, 18 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_ETRClockMode2Config (Thumb, 18 bytes, Stack size 8 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Calls]

  - >> TIM_ETRConfig

  TIM_SelectOutputTrigger (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_SelectMasterSlaveMode (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_EncoderInterfaceConfig (Thumb, 50 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = TIM_EncoderInterfaceConfig
  [Called By]
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config

  TIM_SelectHallSensor (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  TIM_RemapConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_tim.o(.text), UNUSED)

  DAC_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_dac.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB1PeriphResetCmd

  DAC_Init (Thumb, 36 bytes, Stack size 12 bytes, stm32f4xx_dac.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = DAC_Init
  [Called By]
  - >> dac_init

  DAC_StructInit (Thumb, 12 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_Cmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text))
  [Called By]

  - >> dac_init

  DAC_SoftwareTriggerCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_DualSoftwareTriggerCmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_WaveGenerationCmd (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_SetChannel1Data (Thumb, 14 bytes, Stack size 8 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_SetChannel2Data (Thumb, 14 bytes, Stack size 8 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_SetDualChannelData (Thumb, 22 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_GetDataOutputValue (Thumb, 18 bytes, Stack size 8 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_DMACmd (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_GetFlagStatus (Thumb, 20 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_ClearFlag (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_GetITStatus (Thumb, 30 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  DAC_ClearITPendingBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f4xx_dac.o(.text), UNUSED)

  SYSCFG_DeInit (Thumb, 24 bytes, Stack size 8 bytes, stm32f4xx_syscfg.o(.text), UNUSED)
  [Calls]

  - >> RCC_APB2PeriphResetCmd

  SYSCFG_MemoryRemapConfig (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_MemorySwappingBank (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_EXTILineConfig (Thumb, 42 bytes, Stack size 8 bytes, stm32f4xx_syscfg.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = SYSCFG_EXTILineConfig
  [Called By]
  - >> Configure_GPIOF_EXTI
  - >> Configure_GPIOB_EXTI

  SYSCFG_ETH_MediaInterfaceConfig (Thumb, 8 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_CompensationCellCmd (Thumb, 6 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  SYSCFG_GetCompensationCellStatus (Thumb, 16 bytes, Stack size 0 bytes, stm32f4xx_syscfg.o(.text), UNUSED)

  FMC_NORSRAMDeInit (Thumb, 38 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NORSRAMInit (Thumb, 264 bytes, Stack size 12 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NORSRAMStructInit (Thumb, 46 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NORSRAMCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NANDDeInit (Thumb, 40 bytes, Stack size 8 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NANDInit (Thumb, 158 bytes, Stack size 12 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NANDStructInit (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NANDCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_NANDECCCmd (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_GetECC (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_PCCARDDeInit (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_PCCARDInit (Thumb, 116 bytes, Stack size 8 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_PCCARDStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_PCCARDCmd (Thumb, 28 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_SDRAMDeInit (Thumb, 42 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_SDRAMInit (Thumb, 308 bytes, Stack size 20 bytes, stm32f4xx_fmc.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = FMC_SDRAMInit
  [Called By]
  - >> TM_SDRAM_Init

  FMC_SDRAMStructInit (Thumb, 60 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_SDRAMCmdConfig (Thumb, 34 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text))
  [Called By]

  - >> TM_SDRAM_Init

  FMC_GetModeStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_SetRefreshCount (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text))
  [Called By]

  - >> TM_SDRAM_Init

  FMC_SetAutoRefresh_Number (Thumb, 18 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_SDRAMWriteProtectionConfig (Thumb, 32 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_ITConfig (Thumb, 102 bytes, Stack size 12 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_GetFlagStatus (Thumb, 54 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text))
  [Called By]

  - >> TM_SDRAM_Init

  FMC_ClearFlag (Thumb, 56 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_GetITStatus (Thumb, 80 bytes, Stack size 12 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  FMC_ClearITPendingBit (Thumb, 62 bytes, Stack size 0 bytes, stm32f4xx_fmc.o(.text), UNUSED)

  TimingDelay_Decrement (Thumb, 26 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TimingDelay_Decrement
  [Called By]
  - >> SysTick_Handler

  TM_DELAY_Init (Thumb, 82 bytes, Stack size 8 bytes, tm_stm32f4_delay.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = TM_DELAY_Init ⇒ RCC_WaitForHSEStartUp
  [Calls]
  - >> RCC_WaitForHSEStartUp
  - >> RCC_HSEConfig
  [Called By]
  - >> main

  TM_DELAY_EnableDelayTimer (Thumb, 22 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DELAY_DisableDelayTimer (Thumb, 14 bytes, Stack size 0 bytes, tm_stm32f4_delay.o(.text), UNUSED)

  TM_DISCO_LedInit (Thumb, 48 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TM_DISCO_LedInit ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  TM_DISCO_ButtonInit (Thumb, 44 bytes, Stack size 16 bytes, tm_stm32f4_disco.o(.text), UNUSED)
  [Calls]

  - >> GPIO_Init
  - >> RCC_AHB1PeriphClockCmd

  TM_DISCO_ButtonOnPressed (Thumb, 26 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  TM_DISCO_ButtonOnReleased (Thumb, 26 bytes, Stack size 0 bytes, tm_stm32f4_disco.o(.text), UNUSED)

  TM_GPIO_GetPortSource (Thumb, 10 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text))
  [Called By]

  - >> TM_GPIO_GetFreePins
  - >> TM_GPIO_GetUsedPins
  - >> TM_GPIO_INT_DisableClock
  - >> TM_GPIO_DeInit
  - >> TM_GPIO_INT_EnableClock
  - >> TM_GPIO_INT_Init

  TM_GPIO_INT_Init (Thumb, 130 bytes, Stack size 36 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_GetPortSource
  [Called By]
  - >> TM_GPIO_InitAlternate
  - >> TM_GPIO_Init

  TM_GPIO_INT_EnableClock (Thumb, 20 bytes, Stack size 4 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 4
  - Call Chain = TM_GPIO_INT_EnableClock
  [Calls]
  - >> TM_GPIO_GetPortSource
  [Called By]
  - >> TM_GPIO_InitAlternate
  - >> TM_GPIO_Init

  TM_GPIO_Init (Thumb, 34 bytes, Stack size 28 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_INT_EnableClock
  - >> TM_GPIO_INT_Init

  TM_GPIO_InitAlternate (Thumb, 92 bytes, Stack size 44 bytes, tm_stm32f4_gpio.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_GPIO_INT_EnableClock
  - >> TM_GPIO_INT_Init
  [Called By]
  - >> TM_SDRAM_InitPins

  TM_GPIO_DeInit (Thumb, 66 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_GetPortSource

  TM_GPIO_SetPinAsInput (Thumb, 38 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsOutput (Thumb, 46 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsAnalog (Thumb, 38 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPinAsAlternate (Thumb, 48 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_SetPullResistor (Thumb, 46 bytes, Stack size 20 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_Lock (Thumb, 16 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_GetPinSource (Thumb, 18 bytes, Stack size 0 bytes, tm_stm32f4_gpio.o(.text), UNUSED)

  TM_GPIO_INT_DisableClock (Thumb, 20 bytes, Stack size 4 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_GetPortSource

  TM_GPIO_GetUsedPins (Thumb, 14 bytes, Stack size 4 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_GetPortSource

  TM_GPIO_GetFreePins (Thumb, 18 bytes, Stack size 4 bytes, tm_stm32f4_gpio.o(.text), UNUSED)
  [Calls]

  - >> TM_GPIO_GetPortSource

  main (Thumb, 244 bytes, Stack size 80 bytes, main.o(.text))
  [Stack]

  - Max Depth = 344
  - Call Chain = main ⇒ trapez4 ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> trapez4
  - >> escalado
  - >> encoder4_config
  - >> encoder3_config
  - >> encoder2_config
  - >> encoder1_config
  - >> dac_init
  - >> TM_SDRAM_Init
  - >> Control_TimerInit
  - >> Configure_GPIOB_EXTI
  - >> NVIC_EnableIRQ
  - >> TM_DISCO_LedInit
  - >> TM_DELAY_Init
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f4xx_it.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f429_439xx.o(RESET)

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SysTick_Handler ⇒ TimingDelay_Decrement
  [Calls]
  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  TIM2_IRQHandler (Thumb, 36 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM2_IRQHandler
  [Calls]
  - >> TIM_ClearITPendingBit
  - >> TIM_GetITStatus
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI0_IRQHandler (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = EXTI0_IRQHandler ⇒ paradacontrolada ⇒ PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> paradacontrolada
  - >> escalado
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI1_IRQHandler (Thumb, 54 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = EXTI1_IRQHandler ⇒ paradacontrolada ⇒ PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> paradacontrolada
  - >> escalado
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI2_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = EXTI2_IRQHandler ⇒ paradacontrolada ⇒ PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> paradacontrolada
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI3_IRQHandler (Thumb, 38 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 128
  - Call Chain = EXTI3_IRQHandler ⇒ paradacontrolada ⇒ PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> paradacontrolada
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI4_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI4_IRQHandler
  [Calls]
  - >> TIM_GetCounter
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> escalado
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 62 bytes, Stack size 8 bytes, stm32f4xx_it.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = EXTI9_5_IRQHandler
  [Calls]
  - >> TIM_GetCounter
  - >> EXTI_ClearITPendingBit
  - >> EXTI_GetITStatus
  - >> escalado
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  SystemInit (Thumb, 74 bytes, Stack size 8 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = SystemInit ⇒ SetSysClock
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(.text)

  SystemCoreClockUpdate (Thumb, 108 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text), UNUSED)

  TM_SDRAM_InitCustomPinsCallback (Thumb, 4 bytes, Stack size 0 bytes, tm_stm32f4_sdram.o(.text))
  [Called By]

  - >> TM_SDRAM_InitPins

  TM_SDRAM_Init (Thumb, 368 bytes, Stack size 128 bytes, tm_stm32f4_sdram.o(.text))
  [Stack]

  - Max Depth = 232
  - Call Chain = TM_SDRAM_Init ⇒ TM_SDRAM_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> FMC_GetFlagStatus
  - >> FMC_SetRefreshCount
  - >> FMC_SDRAMCmdConfig
  - >> FMC_SDRAMInit
  - >> TM_SDRAM_InitPins
  [Called By]
  - >> main

  Control_TimerInit (Thumb, 124 bytes, Stack size 40 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = Control_TimerInit ⇒ TIM_TimeBaseInit
  [Calls]
  - >> TIM_Cmd
  - >> TIM_TimeBaseInit
  - >> RCC_APB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  encoder1_config (Thumb, 138 bytes, Stack size 32 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = encoder1_config ⇒ GPIO_Init
  [Calls]
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_Cmd
  - >> TIM_SetAutoreload
  - >> TIM_TimeBaseInit
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  encoder2_config (Thumb, 136 bytes, Stack size 32 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = encoder2_config ⇒ GPIO_Init
  [Calls]
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_Cmd
  - >> TIM_SetAutoreload
  - >> TIM_TimeBaseInit
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  encoder3_config (Thumb, 134 bytes, Stack size 32 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = encoder3_config ⇒ GPIO_Init
  [Calls]
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_Cmd
  - >> TIM_SetAutoreload
  - >> TIM_TimeBaseInit
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  encoder4_config (Thumb, 134 bytes, Stack size 32 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = encoder4_config ⇒ GPIO_Init
  [Calls]
  - >> TIM_EncoderInterfaceConfig
  - >> TIM_Cmd
  - >> TIM_SetAutoreload
  - >> TIM_TimeBaseInit
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  dac_init (Thumb, 98 bytes, Stack size 32 bytes, config.o(.text))
  [Stack]

  - Max Depth = 52
  - Call Chain = dac_init ⇒ GPIO_Init
  [Calls]
  - >> DAC_Cmd
  - >> DAC_Init
  - >> GPIO_Init
  - >> RCC_APB1PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> main

  PWM (Thumb, 336 bytes, Stack size 80 bytes, config.o(.text), UNUSED)
  [Calls]

  - >> TIM_ITConfig
  - >> TIM_BDTRStructInit
  - >> TIM_BDTRConfig
  - >> TIM_OCStructInit
  - >> TIM_OC4Init
  - >> TIM_OC3Init
  - >> TIM_OC2Init
  - >> TIM_OC1Init
  - >> TIM_Cmd
  - >> TIM_TimeBaseStructInit
  - >> TIM_TimeBaseInit
  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd

  Configure_GPIOB_EXTI (Thumb, 208 bytes, Stack size 48 bytes, config.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = Configure_GPIOB_EXTI ⇒ GPIO_Init
  [Calls]
  - >> SYSCFG_EXTILineConfig
  - >> EXTI_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> NVIC_Init
  [Called By]
  - >> main

  Configure_GPIOF_EXTI (Thumb, 148 bytes, Stack size 40 bytes, config.o(.text), UNUSED)
  [Calls]

  - >> SYSCFG_EXTILineConfig
  - >> EXTI_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  - >> NVIC_Init

  check_sign (Thumb, 20 bytes, Stack size 0 bytes, trapez.o(.text))
  [Called By]

  - >> trapez
  - >> trapez4

  trapez4 (Thumb, 2042 bytes, Stack size 176 bytes, trapez.o(.text))
  [Stack]

  - Max Depth = 264
  - Call Chain = trapez4 ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> check_sign
  - >> malloc
  - >> __hardfp_sqrt
  [Called By]
  - >> main

  trapez (Thumb, 854 bytes, Stack size 96 bytes, trapez.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> __aeabi_d2f
  - >> check_sign
  - >> malloc
  - >> __hardfp_sqrt

  vel_reference (Thumb, 50 bytes, Stack size 0 bytes, functions.o(.text))
  [Called By]

  - >> paradacontrolada

  speed_estimation (Thumb, 10 bytes, Stack size 0 bytes, functions.o(.text))
  [Called By]

  - >> paradacontrolada

  PPR_to_Rad (Thumb, 114 bytes, Stack size 24 bytes, functions.o(.text))
  [Stack]

  - Max Depth = 112
  - Call Chain = PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_f2d
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_d2f
  [Called By]
  - >> paradacontrolada

  escalado (Thumb, 38 bytes, Stack size 0 bytes, functions.o(.text))
  [Called By]

  - >> paradacontrolada
  - >> EXTI9_5_IRQHandler
  - >> EXTI4_IRQHandler
  - >> EXTI1_IRQHandler
  - >> EXTI0_IRQHandler
  - >> main

  PI_action (Thumb, 44 bytes, Stack size 0 bytes, controller.o(.text))
  [Called By]

  - >> paradacontrolada

  PD_action (Thumb, 40 bytes, Stack size 0 bytes, controller.o(.text), UNUSED)

  paradacontrolada (Thumb, 266 bytes, Stack size 8 bytes, paradaconrolada.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = paradacontrolada ⇒ PPR_to_Rad ⇒ __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> TIM_ITConfig
  - >> TIM_GetCounter
  - >> PI_action
  - >> PPR_to_Rad
  - >> speed_estimation
  - >> vel_reference
  - >> escalado
  [Called By]
  - >> EXTI3_IRQHandler
  - >> EXTI2_IRQHandler
  - >> EXTI1_IRQHandler
  - >> EXTI0_IRQHandler

  USB_OTG_BSP_Init (Thumb, 170 bytes, Stack size 32 bytes, usb_bsp.o(.text), UNUSED)
  [Calls]

  - >> GPIO_PinAFConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_AHB1PeriphClockCmd
  [Called By]
  - >> USBD_Init

  USB_OTG_BSP_EnableInterrupt (Thumb, 104 bytes, Stack size 16 bytes, usb_bsp.o(.text), UNUSED)
  [Calls]

  - >> NVIC_Init
  - >> NVIC_PriorityGroupConfig
  [Called By]
  - >> USBD_Init

  USB_OTG_BSP_uDelay (Thumb, 22 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Called By]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo
  - >> USB_OTG_CoreReset
  - >> USB_OTG_BSP_mDelay

  USB_OTG_BSP_mDelay (Thumb, 8 bytes, Stack size 0 bytes, usb_bsp.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> USB_OTG_ActiveRemoteWakeup
  - >> USB_OTG_SetCurrentMode
  - >> USB_OTG_CoreInit
  - >> DCD_DevDisconnect
  - >> DCD_DevConnect

  OTG_HS_WKUP_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Calls]

  - >> EXTI_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = OTG_HS_IRQHandler ⇒ USBD_OTG_ISR_Handler ⇒ DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_OTG_ISR_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_IN_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = OTG_HS_EP1_IN_IRQHandler ⇒ USBD_OTG_EP1IN_ISR_Handler ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_OTG_EP1IN_ISR_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  OTG_HS_EP1_OUT_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, usb_bsp.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = OTG_HS_EP1_OUT_IRQHandler ⇒ USBD_OTG_EP1OUT_ISR_Handler
  [Calls]
  - >> USBD_OTG_EP1OUT_ISR_Handler
  [Address Reference Count : 1]
  - startup_stm32f429_439xx.o(RESET)

  USB_OTG_WritePacket (Thumb, 40 bytes, Stack size 12 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = USB_OTG_WritePacket
  [Called By]
  - >> USB_OTG_EPStartXfer
  - >> DCD_WriteEmptyTxFifo

  USB_OTG_ReadPacket (Thumb, 32 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_ReadPacket
  [Called By]
  - >> DCD_HandleRxStatusQueueLevel_ISR

  USB_OTG_SelectCore (Thumb, 192 bytes, Stack size 16 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_Init

  USB_OTG_CoreInit (Thumb, 128 bytes, Stack size 16 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_CoreReset
  - >> USB_OTG_BSP_mDelay
  [Called By]
  - >> DCD_Init

  USB_OTG_EnableGlobalInt (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_Init

  USB_OTG_DisableGlobalInt (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_Init

  USB_OTG_FlushTxFifo (Thumb, 62 bytes, Stack size 16 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USB_OTG_FlushTxFifo
  [Calls]
  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> USB_OTG_StopDevice
  - >> USB_OTG_CoreInitDev
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_EP_Flush

  USB_OTG_FlushRxFifo (Thumb, 54 bytes, Stack size 16 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> USB_OTG_StopDevice
  - >> USB_OTG_CoreInitDev
  - >> DCD_EP_Flush

  USB_OTG_SetCurrentMode (Thumb, 42 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay
  [Called By]
  - >> DCD_Init

  USB_OTG_GetMode (Thumb, 10 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_IsDeviceMode (Thumb, 18 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_IsHostMode (Thumb, 14 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_ReadCoreItr (Thumb, 10 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_ReadOtgItr (Thumb, 6 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_InitDevSpeed (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> USB_OTG_CoreInitDev

  USB_OTG_EnableDevInt (Thumb, 66 bytes, Stack size 12 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> USB_OTG_CoreInitDev

  USB_OTG_CoreInitDev (Thumb, 364 bytes, Stack size 24 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_EnableDevInt
  - >> USB_OTG_InitDevSpeed
  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo
  [Called By]
  - >> DCD_Init

  USB_OTG_GetDeviceSpeed (Thumb, 38 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_OTG_ISR_Handler

  USB_OTG_EP0Activate (Thumb, 58 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_EP0Activate
  [Called By]
  - >> USBD_OTG_ISR_Handler

  USB_OTG_EPActivate (Thumb, 104 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_OTG_EPActivate
  [Called By]
  - >> DCD_EP_Open

  USB_OTG_EPDeactivate (Thumb, 78 bytes, Stack size 20 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_EP_Close

  USB_OTG_EPStartXfer (Thumb, 298 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_WritePacket
  [Called By]
  - >> DCD_EP_Tx
  - >> DCD_EP_PrepareRx

  USB_OTG_EP0StartXfer (Thumb, 184 bytes, Stack size 20 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 20
  - Call Chain = USB_OTG_EP0StartXfer
  [Called By]
  - >> DCD_EP_Tx
  - >> DCD_EP_PrepareRx

  USB_OTG_EPSetStall (Thumb, 48 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USB_OTG_SetEPStatus
  - >> DCD_EP_Stall

  USB_OTG_EPClearStall (Thumb, 50 bytes, Stack size 8 bytes, usb_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USB_OTG_EPClearStall
  [Called By]
  - >> USB_OTG_SetEPStatus
  - >> DCD_EP_ClrStall

  USB_OTG_ReadDevAllOutEp_itr (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleOutEP_ISR

  USB_OTG_ReadDevOutEP_itr (Thumb, 16 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleOutEP_ISR

  USB_OTG_ReadDevAllInEPItr (Thumb, 12 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> DCD_HandleInEP_ISR

  USB_OTG_EP0_OutStart (Thumb, 32 bytes, Stack size 0 bytes, usb_core.o(.text))
  [Called By]

  - >> USBD_CtlSendStatus
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlError
  - >> DCD_HandleOutEP_ISR
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_HandleInEP_ISR

  USB_OTG_ActiveRemoteWakeup (Thumb, 66 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  USB_OTG_UngateClock (Thumb, 30 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)

  USB_OTG_StopDevice (Thumb, 72 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo

  USB_OTG_GetEPStatus (Thumb, 66 bytes, Stack size 0 bytes, usb_core.o(.text), UNUSED)
  [Called By]

  - >> DCD_GetEPStatus

  USB_OTG_SetEPStatus (Thumb, 106 bytes, Stack size 8 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_EPClearStall
  - >> USB_OTG_EPSetStall
  [Called By]
  - >> DCD_SetEPStatus

  DCD_Init (Thumb, 146 bytes, Stack size 16 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_CoreInitDev
  - >> USB_OTG_SetCurrentMode
  - >> USB_OTG_DisableGlobalInt
  - >> USB_OTG_EnableGlobalInt
  - >> USB_OTG_CoreInit
  - >> USB_OTG_SelectCore
  [Called By]
  - >> USBD_Init

  DCD_EP_Open (Thumb, 60 bytes, Stack size 16 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 36
  - Call Chain = DCD_EP_Open ⇒ USB_OTG_EPActivate
  [Calls]
  - >> USB_OTG_EPActivate
  [Called By]
  - >> USBD_Reset

  DCD_EP_Close (Thumb, 44 bytes, Stack size 8 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_EPDeactivate

  DCD_EP_PrepareRx (Thumb, 68 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0StartXfer
  - >> USB_OTG_EPStartXfer
  [Called By]
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueRx
  - >> USBD_CtlPrepareRx

  DCD_EP_Tx (Thumb, 62 bytes, Stack size 16 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0StartXfer
  - >> USB_OTG_EPStartXfer
  [Called By]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueSendData
  - >> USBD_CtlSendData

  DCD_EP_Stall (Thumb, 56 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = DCD_EP_Stall
  [Calls]
  - >> USB_OTG_EPSetStall
  [Called By]
  - >> USBD_StdEPReq
  - >> USBD_SetupStage
  - >> USBD_CtlError

  DCD_EP_ClrStall (Thumb, 56 bytes, Stack size 8 bytes, usb_dcd.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DCD_EP_ClrStall ⇒ USB_OTG_EPClearStall
  [Calls]
  - >> USB_OTG_EPClearStall
  [Called By]
  - >> USBD_StdEPReq

  DCD_EP_Flush (Thumb, 24 bytes, Stack size 8 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_FlushRxFifo
  - >> USB_OTG_FlushTxFifo

  DCD_EP_SetAddress (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text))
  [Called By]

  - >> USBD_StdDevReq

  DCD_DevConnect (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  DCD_DevDisconnect (Thumb, 16 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_mDelay

  DCD_GetEPStatus (Thumb, 38 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_GetEPStatus

  DCD_SetEPStatus (Thumb, 38 bytes, Stack size 0 bytes, usb_dcd.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_SetEPStatus

  USBD_OTG_EP1OUT_ISR_Handler (Thumb, 74 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_OTG_EP1OUT_ISR_Handler
  [Called By]
  - >> OTG_HS_EP1_OUT_IRQHandler

  USBD_OTG_EP1IN_ISR_Handler (Thumb, 116 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 60
  - Call Chain = USBD_OTG_EP1IN_ISR_Handler ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_WriteEmptyTxFifo
  [Called By]
  - >> OTG_HS_EP1_IN_IRQHandler

  USBD_OTG_ISR_Handler (Thumb, 324 bytes, Stack size 32 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 100
  - Call Chain = USBD_OTG_ISR_Handler ⇒ DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0Activate
  - >> USB_OTG_GetDeviceSpeed
  - >> USB_OTG_ReadCoreItr
  - >> USB_OTG_IsDeviceMode
  - >> DCD_HandleOutEP_ISR
  - >> DCD_HandleUSBSuspend_ISR
  - >> DCD_HandleRxStatusQueueLevel_ISR
  - >> DCD_HandleUsbReset_ISR
  - >> DCD_HandleInEP_ISR
  [Called By]
  - >> OTG_HS_IRQHandler

  USBD_DeInit (Thumb, 4 bytes, Stack size 0 bytes, usbd_core.o(.text), UNUSED)

  USBD_Init (Thumb, 52 bytes, Stack size 24 bytes, usbd_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_EnableInterrupt
  - >> USB_OTG_BSP_Init
  - >> DCD_Init

  USBD_SetCfg (Thumb, 26 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SetCfg
  [Called By]
  - >> USBD_SetConfig

  USBD_ClrCfg (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_ClrCfg
  [Called By]
  - >> USBD_SetConfig

  USBD_CtlSendData (Thumb, 32 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Called By]
  - >> USBD_GetDescriptor
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq

  USBD_CtlContinueSendData (Thumb, 18 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlContinueSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_Tx
  [Called By]
  - >> USBD_DataInStage

  USBD_CtlPrepareRx (Thumb, 32 bytes, Stack size 8 bytes, usbd_ioreq.o(.text), UNUSED)
  [Calls]

  - >> DCD_EP_PrepareRx

  USBD_CtlContinueRx (Thumb, 18 bytes, Stack size 8 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = USBD_CtlContinueRx ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> DCD_EP_PrepareRx
  [Called By]
  - >> USBD_DataOutStage

  USBD_CtlSendStatus (Thumb, 34 bytes, Stack size 16 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> DCD_EP_Tx
  [Called By]
  - >> USBD_SetFeature
  - >> USBD_SetConfig
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_DataOutStage

  USBD_CtlReceiveStatus (Thumb, 34 bytes, Stack size 16 bytes, usbd_ioreq.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = USBD_CtlReceiveStatus ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> DCD_EP_PrepareRx
  [Called By]
  - >> USBD_DataInStage

  USBD_GetRxCount (Thumb, 16 bytes, Stack size 0 bytes, usbd_ioreq.o(.text), UNUSED)

  USBD_CtlError (Thumb, 28 bytes, Stack size 8 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = USBD_CtlError ⇒ DCD_EP_Stall
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> DCD_EP_Stall
  [Called By]
  - >> USBD_GetDescriptor
  - >> USBD_SetConfig
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq

  USBD_StdDevReq (Thumb, 236 bytes, Stack size 24 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = USBD_StdDevReq ⇒ USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_SetFeature
  - >> USBD_GetDescriptor
  - >> USBD_SetConfig
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> DCD_EP_SetAddress
  [Called By]
  - >> USBD_SetupStage

  USBD_StdItfReq (Thumb, 54 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdItfReq ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlError
  [Called By]
  - >> USBD_SetupStage

  USBD_StdEPReq (Thumb, 208 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_StdEPReq ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  - >> DCD_EP_ClrStall
  - >> DCD_EP_Stall
  [Called By]
  - >> USBD_SetupStage

  USBD_ParseSetupRequest (Thumb, 68 bytes, Stack size 0 bytes, usbd_req.o(.text))
  [Called By]

  - >> USBD_SetupStage

  USBD_GetString (Thumb, 78 bytes, Stack size 16 bytes, usbd_req.o(.text), UNUSED)

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dadd ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> trapez
  - >> trapez4
  - >> __aeabi_drsub
  - >> __aeabi_dsub

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> PPR_to_Rad
  - >> trapez
  - >> trapez4

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> PPR_to_Rad
  - >> trapez
  - >> trapez4

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> PPR_to_Rad

  __aeabi_f2d (Thumb, 38 bytes, Stack size 0 bytes, f2d.o(.text))
  [Called By]

  - >> PPR_to_Rad
  - >> trapez
  - >> trapez4

  __aeabi_d2f (Thumb, 56 bytes, Stack size 8 bytes, d2f.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2f
  [Calls]
  - >> _float_round
  [Called By]
  - >> PPR_to_Rad
  - >> trapez
  - >> trapez4

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_dadd
  - >> _double_epilogue

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text))
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  __I$use$fp (Thumb, 0 bytes, Stack size 0 bytes, iusefp.o(.text), UNUSED)

  _float_round (Thumb, 18 bytes, Stack size 0 bytes, fepilogue.o(.text))
  [Called By]

  - >> __aeabi_d2f

  _float_epilogue (Thumb, 92 bytes, Stack size 4 bytes, fepilogue.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> __aeabi_dadd
  - >> _double_epilogue
  - >> _dsqrt

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  _dsqrt (Thumb, 162 bytes, Stack size 32 bytes, dsqrt.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _dsqrt ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> _double_round
  [Called By]
  - >> __hardfp_sqrt

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> _double_epilogue
  - >> _dsqrt

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __hardfp_sqrt (Thumb, 122 bytes, Stack size 32 bytes, sqrt.o(i.__hardfp_sqrt))
  [Stack]

  - Max Depth = 72
  - Call Chain = __hardfp_sqrt ⇒ _dsqrt ⇒ _double_round
  [Calls]
  - >> __set_errno
  - >> _dsqrt
  [Called By]
  - >> trapez
  - >> trapez4

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  __set_errno (Thumb, 6 bytes, Stack size 0 bytes, errno.o(i.__set_errno))
  [Called By]

  - >> __hardfp_sqrt

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> trapez
  - >> trapez4

  ### Local Symbols

  TI2_Config (Thumb, 54 bytes, Stack size 20 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  TI1_Config (Thumb, 46 bytes, Stack size 16 bytes, stm32f4xx_tim.o(.text), UNUSED)
  [Called By]

  - >> TIM_TIxExternalClockConfig
  - >> TIM_PWMIConfig
  - >> TIM_ICInit

  NVIC_EnableIRQ (Thumb, 22 bytes, Stack size 0 bytes, main.o(.text))
  [Called By]

  - >> main

  SetSysClock (Thumb, 190 bytes, Stack size 16 bytes, system_stm32f4xx.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = SetSysClock
  [Called By]
  - >> SystemInit

  TM_SDRAM_InitPins (Thumb, 120 bytes, Stack size 24 bytes, tm_stm32f4_sdram.o(.text))
  [Stack]

  - Max Depth = 104
  - Call Chain = TM_SDRAM_InitPins ⇒ TM_GPIO_InitAlternate ⇒ TM_GPIO_INT_Init
  [Calls]
  - >> TM_SDRAM_InitCustomPinsCallback
  - >> TM_GPIO_InitAlternate
  [Called By]
  - >> TM_SDRAM_Init

  USB_OTG_CoreReset (Thumb, 84 bytes, Stack size 24 bytes, usb_core.o(.text), UNUSED)
  [Calls]

  - >> USB_OTG_BSP_uDelay
  [Called By]
  - >> USB_OTG_CoreInit

  DCD_WriteEmptyTxFifo (Thumb, 114 bytes, Stack size 32 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_WritePacket
  [Called By]
  - >> USBD_OTG_EP1IN_ISR_Handler
  - >> DCD_HandleInEP_ISR

  DCD_HandleInEP_ISR (Thumb, 198 bytes, Stack size 24 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 68
  - Call Chain = DCD_HandleInEP_ISR ⇒ DCD_WriteEmptyTxFifo ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_ReadDevAllInEPItr
  - >> DCD_WriteEmptyTxFifo
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleUsbReset_ISR (Thumb, 138 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 32
  - Call Chain = DCD_HandleUsbReset_ISR ⇒ USB_OTG_FlushTxFifo
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_FlushTxFifo
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleRxStatusQueueLevel_ISR (Thumb, 128 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DCD_HandleRxStatusQueueLevel_ISR ⇒ USB_OTG_ReadPacket
  [Calls]
  - >> USB_OTG_ReadPacket
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleUSBSuspend_ISR (Thumb, 102 bytes, Stack size 16 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = DCD_HandleUSBSuspend_ISR
  [Called By]
  - >> USBD_OTG_ISR_Handler

  DCD_HandleOutEP_ISR (Thumb, 164 bytes, Stack size 24 bytes, usb_dcd_int.o(.text))
  [Stack]

  - Max Depth = 24
  - Call Chain = DCD_HandleOutEP_ISR
  [Calls]
  - >> USB_OTG_EP0_OutStart
  - >> USB_OTG_ReadDevOutEP_itr
  - >> USB_OTG_ReadDevAllOutEp_itr
  [Called By]
  - >> USBD_OTG_ISR_Handler

  USBD_SetupStage (Thumb, 72 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 120
  - Call Chain = USBD_SetupStage ⇒ USBD_StdDevReq ⇒ USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_StdItfReq
  - >> USBD_StdEPReq
  - >> USBD_StdDevReq
  - >> USBD_ParseSetupRequest
  - >> DCD_EP_Stall
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_DataOutStage (Thumb, 116 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_DataOutStage ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_CtlContinueRx
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_DataInStage (Thumb, 172 bytes, Stack size 16 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_DataInStage ⇒ USBD_CtlReceiveStatus ⇒ DCD_EP_PrepareRx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlReceiveStatus
  - >> USBD_CtlContinueSendData
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Reset (Thumb, 46 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 44
  - Call Chain = USBD_Reset ⇒ DCD_EP_Open ⇒ USB_OTG_EPActivate
  [Calls]
  - >> DCD_EP_Open
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Resume (Thumb, 22 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_Resume
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_Suspend (Thumb, 28 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_Suspend
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_SOF (Thumb, 16 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_SOF
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_IsoINIncomplete (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_IsoINIncomplete
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_IsoOUTIncomplete (Thumb, 14 bytes, Stack size 8 bytes, usbd_core.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = USBD_IsoOUTIncomplete
  [Address Reference Count : 1]
  - usbd_core.o(.data)

  USBD_SetConfig (Thumb, 110 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 80
  - Call Chain = USBD_SetConfig ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  - >> USBD_ClrCfg
  - >> USBD_SetCfg
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_GetDescriptor (Thumb, 288 bytes, Stack size 16 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_GetDescriptor ⇒ USBD_CtlSendData ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendData
  - >> USBD_CtlError
  [Called By]
  - >> USBD_StdDevReq

  USBD_SetFeature (Thumb, 118 bytes, Stack size 8 bytes, usbd_req.o(.text))
  [Stack]

  - Max Depth = 72
  - Call Chain = USBD_SetFeature ⇒ USBD_CtlSendStatus ⇒ DCD_EP_Tx ⇒ USB_OTG_EPStartXfer ⇒ USB_OTG_WritePacket
  [Calls]
  - >> USBD_CtlSendStatus
  [Called By]
  - >> USBD_StdDevReq

  ### Undefined Global Symbols