
 ANSYS Multiphysics                                


 *------------------------------------------------------------------*
 |                                                                  |
 |   W E L C O M E   T O   T H E   A N S Y S (R)  P R O G R A M     |
 |                                                                  |
 *------------------------------------------------------------------*




 ***************************************************************
 *            ANSYS Release 17.0     LEGAL NOTICES             *
 ***************************************************************
 *                                                             *
 * Copyright 2015 SAS IP, Inc.  All rights reserved.           *
 * Unauthorized use, distribution or duplication is            *
 * prohibited.                                                 *
 *                                                             *
 * Ansys is a registered trademark of ANSYS, Inc. or its       *
 * subsidiaries in the United States or other countries.       *
 * See the ANSYS, Inc. online documentation or the ANSYS, Inc. *
 * documentation CD or online help for the complete Legal      *
 * Notice.                                                     *
 *                                                             *
 ***************************************************************
 *                                                             *
 * THIS ANSYS SOFTWARE PRODUCT AND PROGRAM DOCUMENTATION       *
 * INCLUDE TRADE SECRETS AND CONFIDENTIAL AND PROPRIETARY      *
 * PRODUCTS OF ANSYS, INC., ITS SUBSIDIARIES, OR LICENSORS.    *
 * The software products and documentation are furnished by    *
 * ANSYS, Inc. or its subsidiaries under a software license    *
 * agreement that contains provisions concerning               *
 * non-disclosure, copying, length and nature of use,          *
 * compliance with exporting laws, warranties, disclaimers,    *
 * limitations of liability, and remedies, and other           *
 * provisions.  The software products and documentation may be *
 * used, disclosed, transferred, or copied only in accordance  *
 * with the terms and conditions of that software license      *
 * agreement.                                                  *
 *                                                             *
 * ANSYS, Inc. is a UL registered                              *
 * ISO 9001:2008 company.                                      *
 *                                                             *
 ***************************************************************
 *                                                             *
 * This product is subject to U.S. laws governing export and   *
 * re-export.                                                  *
 *                                                             *
 * For U.S. Government users, except as specifically granted   *
 * by the ANSYS, Inc. software license agreement, the use,     *
 * duplication, or disclosure by the United States Government  *
 * is subject to restrictions stated in the ANSYS, Inc.        *
 * software license agreement and FAR 12.212 (for non-DOD      *
 * licenses).                                                  *
 *                                                             *
 ***************************************************************

 Release 17.0
     
 Point Releases and Patches installed:   
     
 ANSYS, Inc. Products Release 17.0   
 ANSYS Mechanical Products Release 17.0  
 ANSYS Autodyn Release 17.0  
 ANSYS LS-DYNA Release 17.0  
 ANSYS AIM Release 17.0  
 ANSYS CFX (includes ANSYS CFD-Post) Release 17.0
 ANSYS Fluent (includes ANSYS CFD-Post) Release 17.0 
 ANSYS TurboGrid Release 17.0
 ANSYS Polyflow (includes ANSYS CFD-Post) Release 17.0   
 ANSYS Forte Release 17.0
 ANSYS ICEM CFD Release 17.0 
 ANSYS Aqwa Release 17.0 
 ANSYS Composite PrepPost Release 17.0   
 ANSYS Icepak (includes ANSYS CFD-Post) Release 17.0 
 AutoCAD Release 17.0
 ACIS Release 17.0   
 Catia, Version 4 Release 17.0   
 Catia, Version 6 Release 17.0   
 Creo Elements/Direct Modeling Release 17.0  
 Inventor Release 17.0   
 JTOpen Release 17.0 
 NX Release 17.0 
 Parasolid Release 17.0  
 Creo Parametric (formerly Pro/ENGINEER) Release 17.0
 Solid Edge Release 17.0 
 SolidWorks Release 17.0 
 ANSYS, Inc. License Manager Release 17.0


          *****  ANSYS COMMAND LINE ARGUMENTS  *****
  BATCH MODE REQUESTED (-b)    = NOLIST
  INPUT FILE COPY MODE (-c)    = COPY
  DISTRIBUTED MEMORY PARALLEL REQUESTED
       2 PARALLEL PROCESSES REQUESTED WITH SINGLE THREAD PER PROCESS
    TOTAL OF     2 CORES REQUESTED
  MPI OPTION                   = INTELMPI
  INPUT FILE NAME              = C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScratch\Scr48FB\dummy.dat
  OUTPUT FILE NAME             = C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScratch\Scr48FB\solve.out
  START-UP FILE MODE           = NOREAD
  STOP FILE MODE               = NOREAD

 RELEASE= Release 17.0         BUILD= 17.0      UP20151214   VERSION=WINDOWS x64 
 CURRENT JOBNAME=file0  11:41:13  JUN 15, 2019 CP=      1.453


 PARAMETER _DS_PROGRESS =     999.0000000    

 /INPUT FILE= ds.dat  LINE=       0



 *** NOTE ***                            CP =       1.641   TIME= 11:41:13
 The /CONFIG,NOELDB command is not valid in a Distributed ANSYS          
 solution.  Command is ignored.                                          

 *GET  _WALLSTRT  FROM  ACTI  ITEM=TIME WALL  VALUE=  11.6869444    

 TITLE= 
 unsaved_project--Static Structural (A5)                                       


 SET PARAMETER DIMENSIONS ON  _WB_PROJECTSCRATCH_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_PROJECTSCRATCH_DIR(1) = C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScratch\Scr48FB\

 SET PARAMETER DIMENSIONS ON  _WB_SOLVERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_SOLVERFILES_DIR(1) = C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\unsaved_project_files\dp0\SYS\MECH\

 SET PARAMETER DIMENSIONS ON  _WB_USERFILES_DIR
  TYPE=STRI  DIMENSIONS=      248        1        1

 PARAMETER _WB_USERFILES_DIR(1) = C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\unsaved_project_files\user_files\
 --- Data in consistent MKS units. See Solving Units in the help system for more

 MKS UNITS SPECIFIED FOR INTERNAL    
  LENGTH        (l)  = METER (M)
  MASS          (M)  = KILOGRAM (KG)
  TIME          (t)  = SECOND (SEC)
  TEMPERATURE   (T)  = CELSIUS (C)
  TOFFSET            = 273.0
  CHARGE        (Q)  = COULOMB
  FORCE         (f)  = NEWTON (N) (KG-M/SEC2)
  HEAT               = JOULE (N-M)

  PRESSURE           = PASCAL (NEWTON/M**2)
  ENERGY        (W)  = JOULE (N-M)
  POWER         (P)  = WATT (N-M/SEC)
  CURRENT       (i)  = AMPERE (COULOMBS/SEC)
  CAPACITANCE   (C)  = FARAD
  INDUCTANCE    (L)  = HENRY
  MAGNETIC FLUX      = WEBER
  RESISTANCE    (R)  = OHM
  ELECTRIC POTENTIAL = VOLT

 INPUT  UNITS ARE ALSO SET TO MKS 

 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 17.0     17.0     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   11:41:13  JUN 15, 2019 CP=      1.641

 unsaved_project--Static Structural (A5)                                       



          ***** ANSYS ANALYSIS DEFINITION (PREP7) *****
 *********** Nodes for the whole assembly ***********
 *********** Elements for Body 1 "Part 1" ***********
 *********** Elements for Body 2 "Part 2" ***********
 *********** Elements for Body 3 "Part 3" ***********
 *********** Elements for Body 4 "Part 4" ***********
 *********** Elements for Body 5 "Part 5" ***********
 *********** Elements for Body 6 "Part 6" ***********
 *********** Elements for Body 7 "Part 7" ***********
 *********** Elements for Body 8 "Part 8" ***********
 *********** Elements for Body 9 "Part 9" ***********
 *********** Elements for Body 10 "Part 10" ***********
 *********** Elements for Body 11 "Part 11" ***********
 *********** Elements for Body 12 "Part 12" ***********
 *********** Elements for Body 13 "Part 13" ***********
 *********** Elements for Body 14 "Part 14" ***********
 *********** Elements for Body 15 "Part 15" ***********
 *********** Elements for Body 16 "Part 16" ***********
 *********** Elements for Body 17 "Part 17" ***********
 *********** Elements for Body 18 "Part 18" ***********
 *********** Elements for Body 19 "Part 19" ***********
 *********** Elements for Body 20 "Part 20" ***********
 *********** Elements for Body 21 "Part 21" ***********
 *********** Elements for Body 22 "Part 22" ***********
 *********** Elements for Body 23 "Part 23" ***********
 *********** Elements for Body 24 "Part 24" ***********
 *********** Elements for Body 25 "Part 25" ***********
 *********** Elements for Body 26 "Part 26" ***********
 *********** Elements for Body 27 "Part 27" ***********
 *********** Elements for Body 28 "Part 28" ***********
 *********** Elements for Body 29 "Part 29" ***********
 *********** Elements for Body 30 "Part 30" ***********
 *********** Elements for Body 31 "Part 31" ***********
 *********** Elements for Body 32 "Part 32" ***********
 *********** Elements for Body 33 "Part 33" ***********
 *********** Elements for Body 34 "Part 34" ***********
 *********** Elements for Body 35 "Part 35" ***********
 *********** Elements for Body 36 "Part 36" ***********
 *********** Elements for Body 37 "Part 37" ***********
 *********** Elements for Body 38 "Part 38" ***********
 *********** Elements for Body 39 "Part 39" ***********
 *********** Elements for Body 40 "Part 40" ***********
 *********** Elements for Body 41 "Part 41" ***********
 *********** Elements for Body 42 "Part 42" ***********
 *********** Elements for Body 43 "Part 43" ***********
 *********** Elements for Body 44 "Part 44" ***********
 *********** Elements for Body 45 "Part 45" ***********
 *********** Elements for Body 46 "Part 46" ***********
 *********** Elements for Body 47 "Part 47" ***********
 *********** Elements for Body 48 "Part 48" ***********
 *********** Elements for Body 49 "Part 49" ***********
 *********** Elements for Body 50 "Part 50" ***********
 *********** Elements for Body 51 "Part 51" ***********
 *********** Elements for Body 52 "Part 52" ***********
 *********** Elements for Body 53 "Part 53" ***********
 *********** Elements for Body 54 "Part 54" ***********
 *********** Elements for Body 55 "Part 55" ***********
 *********** Elements for Body 56 "Part 56" ***********
 *********** Send User Defined Coordinate System(s) ***********
 *********** Set Reference Temperature ***********
 *********** Send Materials ***********
 *********** Create Contact "Contact Region" ***********
             Real Constant Set For Above Contact Is 58 & 57
 *********** Create Contact "Contact Region 2" ***********
             Real Constant Set For Above Contact Is 60 & 59
 *********** Create Contact "Contact Region 3" ***********
             Real Constant Set For Above Contact Is 62 & 61
 *********** Create Contact "Contact Region 4" ***********
             Real Constant Set For Above Contact Is 64 & 63
 *********** Create Contact "Contact Region 5" ***********
             Real Constant Set For Above Contact Is 66 & 65
 *********** Create Contact "Contact Region 6" ***********
             Real Constant Set For Above Contact Is 68 & 67
 *********** Create Contact "Contact Region 7" ***********
             Real Constant Set For Above Contact Is 70 & 69
 *********** Create Contact "Contact Region 8" ***********
             Real Constant Set For Above Contact Is 72 & 71
 *********** Create Contact "Contact Region 9" ***********
             Real Constant Set For Above Contact Is 74 & 73
 *********** Create Contact "Contact Region 10" ***********
             Real Constant Set For Above Contact Is 76 & 75
 *********** Create Contact "Contact Region 11" ***********
             Real Constant Set For Above Contact Is 78 & 77
 *********** Create Contact "Contact Region 12" ***********
             Real Constant Set For Above Contact Is 80 & 79
 *********** Create Contact "Contact Region 13" ***********
             Real Constant Set For Above Contact Is 82 & 81
 *********** Create Contact "Contact Region 14" ***********
             Real Constant Set For Above Contact Is 84 & 83
 *********** Create Contact "Contact Region 15" ***********
             Real Constant Set For Above Contact Is 86 & 85
 *********** Create Contact "Contact Region 16" ***********
             Real Constant Set For Above Contact Is 88 & 87
 *********** Create Contact "Contact Region 17" ***********
             Real Constant Set For Above Contact Is 90 & 89
 *********** Create Contact "Contact Region 18" ***********
             Real Constant Set For Above Contact Is 92 & 91
 *********** Create Contact "Contact Region 19" ***********
             Real Constant Set For Above Contact Is 94 & 93
 *********** Create Contact "Contact Region 20" ***********
             Real Constant Set For Above Contact Is 96 & 95
 *********** Create Contact "Contact Region 21" ***********
             Real Constant Set For Above Contact Is 98 & 97
 *********** Create Contact "Contact Region 22" ***********
             Real Constant Set For Above Contact Is 100 & 99
 *********** Create Contact "Contact Region 23" ***********
             Real Constant Set For Above Contact Is 102 & 101
 *********** Create Contact "Contact Region 24" ***********
             Real Constant Set For Above Contact Is 104 & 103
 *********** Create Contact "Contact Region 25" ***********
             Real Constant Set For Above Contact Is 106 & 105
 *********** Create Contact "Contact Region 26" ***********
             Real Constant Set For Above Contact Is 108 & 107
 *********** Create Contact "No Separation - Part 27 To Part 31" ***********
             Real Constant Set For Above Contact Is 110 & 109
 *********** Create Contact "No Separation - Part 27 To Part 32" ***********
             Real Constant Set For Above Contact Is 112 & 111
 *********** Create Contact "No Separation - Part 28 To Part 31" ***********
             Real Constant Set For Above Contact Is 114 & 113
 *********** Create Contact "No Separation - Part 28 To Part 32" ***********
             Real Constant Set For Above Contact Is 116 & 115
 *********** Create Contact "No Separation - Part 29 To Part 31" ***********
             Real Constant Set For Above Contact Is 118 & 117
 *********** Create Contact "Contact Region 32" ***********
             Real Constant Set For Above Contact Is 120 & 119
 *********** Create Contact "Contact Region 33" ***********
             Real Constant Set For Above Contact Is 122 & 121
 *********** Create Contact "Contact Region 34" ***********
             Real Constant Set For Above Contact Is 124 & 123
 *********** Create Contact "Contact Region 35" ***********
             Real Constant Set For Above Contact Is 126 & 125
 *********** Create Contact "Contact Region 36" ***********
             Real Constant Set For Above Contact Is 128 & 127
 *********** Create Contact "Contact Region 37" ***********
             Real Constant Set For Above Contact Is 130 & 129
 *********** Create Contact "Contact Region 38" ***********
             Real Constant Set For Above Contact Is 132 & 131
 *********** Create Contact "Contact Region 39" ***********
             Real Constant Set For Above Contact Is 134 & 133
 *********** Create Contact "Contact Region 40" ***********
             Real Constant Set For Above Contact Is 136 & 135
 *********** Create Contact "Contact Region 41" ***********
             Real Constant Set For Above Contact Is 138 & 137
 *********** Create Contact "Contact Region 42" ***********
             Real Constant Set For Above Contact Is 140 & 139
 *********** Create Contact "Contact Region 43" ***********
             Real Constant Set For Above Contact Is 142 & 141
 *********** Create Contact "Contact Region 44" ***********
             Real Constant Set For Above Contact Is 144 & 143
 *********** Create Contact "Contact Region 45" ***********
             Real Constant Set For Above Contact Is 146 & 145
 *********** Create Contact "Contact Region 46" ***********
             Real Constant Set For Above Contact Is 148 & 147
 *********** Create Contact "Contact Region 47" ***********
             Real Constant Set For Above Contact Is 150 & 149
 *********** Create Contact "Contact Region 48" ***********
             Real Constant Set For Above Contact Is 152 & 151
 *********** Create Contact "Contact Region 49" ***********
             Real Constant Set For Above Contact Is 154 & 153
 *********** Create Contact "Contact Region 50" ***********
             Real Constant Set For Above Contact Is 156 & 155
 *********** Create Contact "Contact Region 51" ***********
             Real Constant Set For Above Contact Is 158 & 157
 *********** Create Contact "Contact Region 52" ***********
             Real Constant Set For Above Contact Is 160 & 159
 *********** Create Contact "Contact Region 53" ***********
             Real Constant Set For Above Contact Is 162 & 161
 *********** Create Contact "Contact Region 54" ***********
             Real Constant Set For Above Contact Is 164 & 163
 *********** Create Contact "Contact Region 55" ***********
             Real Constant Set For Above Contact Is 166 & 165
 *********** Create Contact "Contact Region 56" ***********
             Real Constant Set For Above Contact Is 168 & 167
 *********** Create Contact "Contact Region 57" ***********
             Real Constant Set For Above Contact Is 170 & 169
 *********** Create Contact "Contact Region 58" ***********
             Real Constant Set For Above Contact Is 172 & 171
 *********** Create Contact "Contact Region 59" ***********
             Real Constant Set For Above Contact Is 174 & 173
 *********** Create Contact "Contact Region 60" ***********
             Real Constant Set For Above Contact Is 176 & 175
 *********** Create Contact "Contact Region 61" ***********
             Real Constant Set For Above Contact Is 178 & 177
 *********** Create Contact "Contact Region 62" ***********
             Real Constant Set For Above Contact Is 180 & 179
 *********** Create Contact "Contact Region 63" ***********
             Real Constant Set For Above Contact Is 182 & 181
 *********** Create Contact "Contact Region 64" ***********
             Real Constant Set For Above Contact Is 184 & 183
 *********** Create Contact "Contact Region 65" ***********
             Real Constant Set For Above Contact Is 186 & 185
 *********** Create Contact "Contact Region 66" ***********
             Real Constant Set For Above Contact Is 188 & 187
 *********** Create Contact "Contact Region 67" ***********
             Real Constant Set For Above Contact Is 190 & 189
 *********** Create Contact "Contact Region 68" ***********
             Real Constant Set For Above Contact Is 192 & 191
 *********** Create Contact "Contact Region 69" ***********
             Real Constant Set For Above Contact Is 194 & 193
 *********** Create Contact "Contact Region 70" ***********
             Real Constant Set For Above Contact Is 196 & 195
 *********** Create Contact "Contact Region 71" ***********
             Real Constant Set For Above Contact Is 198 & 197
 *********** Create Contact "Contact Region 72" ***********
             Real Constant Set For Above Contact Is 200 & 199
 *********** Create Contact "Contact Region 73" ***********
             Real Constant Set For Above Contact Is 202 & 201
 *********** Create Contact "Contact Region 74" ***********
             Real Constant Set For Above Contact Is 204 & 203
 *********** Create Contact "Contact Region 75" ***********
             Real Constant Set For Above Contact Is 206 & 205
 *********** Create Contact "Contact Region 76" ***********
             Real Constant Set For Above Contact Is 208 & 207
 *********** Create Contact "Contact Region 77" ***********
             Real Constant Set For Above Contact Is 210 & 209
 *********** Create Contact "Contact Region 78" ***********
             Real Constant Set For Above Contact Is 212 & 211
 *********** Create Contact "Contact Region 79" ***********
             Real Constant Set For Above Contact Is 214 & 213
 *********** Create Contact "Contact Region 80" ***********
             Real Constant Set For Above Contact Is 216 & 215
 *********** Create Contact "Contact Region 81" ***********
             Real Constant Set For Above Contact Is 218 & 217
 *********** Create Contact "Contact Region 82" ***********
             Real Constant Set For Above Contact Is 220 & 219
 *********** Create Contact "Contact Region 83" ***********
             Real Constant Set For Above Contact Is 222 & 221
 *********** Create Contact "Contact Region 84" ***********
             Real Constant Set For Above Contact Is 224 & 223
 *********** Create Contact "Contact Region 85" ***********
             Real Constant Set For Above Contact Is 226 & 225
 *********** Create Contact "Contact Region 86" ***********
             Real Constant Set For Above Contact Is 228 & 227
 *********** Create Contact "Contact Region 87" ***********
             Real Constant Set For Above Contact Is 230 & 229
 *********** Create Contact "Contact Region 88" ***********
             Real Constant Set For Above Contact Is 232 & 231
 *********** Create Contact "Contact Region 89" ***********
             Real Constant Set For Above Contact Is 234 & 233
 *********** Create Contact "Contact Region 90" ***********
             Real Constant Set For Above Contact Is 236 & 235
 *********** Create Contact "Contact Region 91" ***********
             Real Constant Set For Above Contact Is 238 & 237
 *********** Create Contact "Contact Region 92" ***********
             Real Constant Set For Above Contact Is 240 & 239
 *********** Create Contact "Contact Region 93" ***********
             Real Constant Set For Above Contact Is 242 & 241
 *********** Create Contact "Contact Region 94" ***********
             Real Constant Set For Above Contact Is 244 & 243
 *********** Create Contact "Contact Region 95" ***********
             Real Constant Set For Above Contact Is 246 & 245
 *********** Create Contact "Contact Region 96" ***********
             Real Constant Set For Above Contact Is 248 & 247
 *********** Create Contact "Contact Region 97" ***********
             Real Constant Set For Above Contact Is 250 & 249
 *********** Create Contact "Contact Region 98" ***********
             Real Constant Set For Above Contact Is 252 & 251
 *********** Create Contact "Contact Region 99" ***********
             Real Constant Set For Above Contact Is 254 & 253
 *********** Create Contact "Contact Region 100" ***********
             Real Constant Set For Above Contact Is 256 & 255
 *********** Create Contact "Contact Region 101" ***********
             Real Constant Set For Above Contact Is 258 & 257
 *********** Create Contact "Contact Region 102" ***********
             Real Constant Set For Above Contact Is 260 & 259
 *********** Create Contact "Contact Region 103" ***********
             Real Constant Set For Above Contact Is 262 & 261
 *********** Create Contact "Contact Region 104" ***********
             Real Constant Set For Above Contact Is 264 & 263
 *********** Create Contact "Contact Region 105" ***********
             Real Constant Set For Above Contact Is 266 & 265
 *********** Create Contact "Contact Region 106" ***********
             Real Constant Set For Above Contact Is 268 & 267
 *********** Create Contact "Contact Region 107" ***********
             Real Constant Set For Above Contact Is 270 & 269
 *********** Create Contact "Contact Region 108" ***********
             Real Constant Set For Above Contact Is 272 & 271
 *********** Create Contact "Contact Region 109" ***********
             Real Constant Set For Above Contact Is 274 & 273
 *********** Create Contact "Bonded - Part 46 To Part 52" ***********
             Real Constant Set For Above Contact Is 276 & 275
 *********** Fixed Supports ***********
 *********** Define Pressure Vector Using Surface Effect Elements ***********
 *********** Define Body Force Temperature ***********


 ***** ROUTINE COMPLETED *****  CP =         5.984


 --- Number of total nodes = 176706
 --- Number of contact elements = 42817
 --- Number of spring elements = 0
 --- Number of bearing elements = 0
 --- Number of solid elements = 82524
 --- Number of total elements = 125689

 *GET  _WALLBSOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  11.6875000    
 ****************************************************************************
 *************************    SOLUTION       ********************************
 ****************************************************************************

 *****  ANSYS SOLUTION ROUTINE  *****


 PERFORM A STATIC ANALYSIS
  THIS WILL BE A NEW ANALYSIS

 USE A MAXIMUM OF     1 EQUILIBRIUM ITERATIONS EACH SUBSTEP

 *** WARNING ***                         CP =       6.047   TIME= 11:41:15
 Using 1 iteration per substep may result in unconverged solutions for   
 nonlinear analysis and the program may not indicate divergence in this  
 case.  Check your results.                                              

 DO NOT USE PREDICTOR METHOD FOR  ALL DEGREES OF FREEDOM

 USE SPARSE MATRIX DIRECT SOLVER

 CONTACT INFORMATION PRINTOUT LEVEL       1

 DO NOT COMBINE ELEMENT MATRIX FILES (.emat) AFTER DISTRIBUTED PARALLEL SOLUTION

 DO NOT COMBINE ELEMENT SAVE DATA FILES (.esav) AFTER DISTRIBUTED PARALLEL SOLUTION

 NLDIAG: Nonlinear diagnostics CONT option is set to ON. 
         Writing frequency : each ITERATION.

 DO NOT SAVE ANY RESTART FILES AT ALL
 ****************************************************
 ******************* SOLVE FOR LS 1 ****************

 SELECT       FOR ITEM=TYPE COMPONENT=    
  IN RANGE       277 TO        277 STEP          1

       9113  ELEMENTS (OF     125689  DEFINED) SELECTED BY  ESEL  COMMAND.

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

    22648 NODES (OF   176706  DEFINED) SELECTED FROM
     9113 SELECTED ELEMENTS BY NSLE COMMAND.

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  1   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI523X                   

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  2   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI523Y                   

 SPECIFIED SURFACE LOAD PRES FOR ALL SELECTED ELEMENTS  LKEY =  3   KVAL = 1
      SET ACCORDING TO TABLE PARAMETER = _LOADVARI523Z                   

 ALL SELECT   FOR ITEM=NODE COMPONENT=    
  IN RANGE         1 TO     176706 STEP          1

     176706  NODES (OF     176706  DEFINED) SELECTED BY NSEL  COMMAND.

 ALL SELECT   FOR ITEM=ELEM COMPONENT=    
  IN RANGE         1 TO     125689 STEP          1

     125689  ELEMENTS (OF     125689  DEFINED) SELECTED BY  ESEL  COMMAND.

 PRINTOUT RESUMED BY /GOP

 SELECT      COMPONENT _CM525                          

 SELECT      ALL NODES HAVING ANY ELEMENT IN ELEMENT SET.

   175778 NODES (OF   176706  DEFINED) SELECTED FROM
    82384 SELECTED ELEMENTS BY NSLE COMMAND.

 SPECIFIED BODY FORCE TEMP FOR ALL SELECTED NODES SET ACCORDING TO
 TABLE PARAMETER = _LOADVARI525 

 ALL SELECT   FOR ITEM=NODE COMPONENT=    
  IN RANGE         1 TO     176706 STEP          1

     176706  NODES (OF     176706  DEFINED) SELECTED BY NSEL  COMMAND.

 ALL SELECT   FOR ITEM=ELEM COMPONENT=    
  IN RANGE         1 TO     125689 STEP          1

     125689  ELEMENTS (OF     125689  DEFINED) SELECTED BY  ESEL  COMMAND.

 USE       1 SUBSTEPS INITIALLY THIS LOAD STEP FOR ALL  DEGREES OF FREEDOM
 FOR AUTOMATIC TIME STEPPING:
   USE      1 SUBSTEPS AS A MAXIMUM
   USE      1 SUBSTEPS AS A MINIMUM

 TIME=  1.0000    

 ERASE THE CURRENT DATABASE OUTPUT CONTROL TABLE.


 WRITE ALL  ITEMS TO THE DATABASE WITH A FREQUENCY OF NONE
   FOR ALL APPLICABLE ENTITIES

 WRITE NSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE RSOL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE STRS ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE EPEL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE EPPL ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 WRITE EPTH ITEMS TO THE DATABASE WITH A FREQUENCY OF ALL 
   FOR ALL APPLICABLE ENTITIES

 NONLINEAR STABILIZATION CONTROL:
 KEY=OFF 


 *GET  ANSINTER_  FROM  ACTI  ITEM=INT        VALUE=  0.00000000    

 *IF  ANSINTER_                         ( =   0.00000     )  NE  
      0                                 ( =   0.00000     )  THEN    

 *ENDIF

 *****  ANSYS SOLVE    COMMAND  *****

 *** WARNING ***                         CP =       6.484   TIME= 11:41:16
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** NOTE ***                            CP =       6.922   TIME= 11:41:16
 The model data was checked and warning messages were found.             
  Please review output or errors file (                                  
 C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScrat 
 tch\Scr48FB\file0.err ) for these warning messages.                     

 *** SELECTION OF ELEMENT TECHNOLOGIES FOR APPLICABLE ELEMENTS ***
      --- GIVE SUGGESTIONS AND RESET THE KEY OPTIONS ---

 ELEMENT TYPE    1 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    2 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    3 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    4 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    5 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    6 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    7 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    8 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE    9 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   10 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   11 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   12 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   13 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   14 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   15 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   16 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   17 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   18 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   19 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   20 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   21 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   22 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   23 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   24 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   25 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   26 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   27 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   28 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   29 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   30 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   31 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   32 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   33 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   34 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   35 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   36 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   37 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   38 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   39 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   40 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   41 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   42 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE   43 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   44 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   45 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE   46 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   47 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   48 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   49 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   50 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   51 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   52 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   53 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE   54 IS SOLID186. KEYOPT(2)=0 IS SUGGESTED AND HAS BEEN RESET.
  KEYOPT(1-12)=    0    0    0    0    0    0    0    0    0    0    0    0

 ELEMENT TYPE   55 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.

 ELEMENT TYPE   56 IS SOLID187. IT IS NOT ASSOCIATED WITH FULLY INCOMPRESSIBLE
 HYPERELASTIC MATERIALS. NO SUGGESTION IS AVAILABLE AND NO RESETTING IS NEEDED.



 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 17.0     17.0     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   11:41:16  JUN 15, 2019 CP=      7.047

 unsaved_project--Static Structural (A5)                                       



                       S O L U T I O N   O P T I O N S

   PROBLEM DIMENSIONALITY. . . . . . . . . . . . .3-D                  
   DEGREES OF FREEDOM. . . . . . UX   UY   UZ  
   ANALYSIS TYPE . . . . . . . . . . . . . . . . .STATIC (STEADY-STATE)
   OFFSET TEMPERATURE FROM ABSOLUTE ZERO . . . . .  273.15    
   EQUATION SOLVER OPTION. . . . . . . . . . . . .SPARSE             
   NEWTON-RAPHSON OPTION . . . . . . . . . . . . .PROGRAM CHOSEN   
   GLOBALLY ASSEMBLED MATRIX . . . . . . . . . . .SYMMETRIC  

 *** WARNING ***                         CP =       7.422   TIME= 11:41:16
 Material number 277 (used by element 116577 ) should normally have at   
 least one MP or one TB type command associated with it.  Output of      
 energy by material may not be available.                                

 *** NOTE ***                            CP =       7.594   TIME= 11:41:16
 The step data was checked and warning messages were found.              
  Please review output or errors file (                                  
 C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScrat 
 tch\Scr48FB\file0.err ) for these warning messages.                     

 *** NOTE ***                            CP =       7.594   TIME= 11:41:16
 This nonlinear analysis defaults to using the full Newton-Raphson       
 solution procedure.  This can be modified using the NROPT command.      

 *** NOTE ***                            CP =       7.594   TIME= 11:41:16
 The conditions for direct assembly have been met.  No .emat or .erot    
 files will be produced.                                                 
 *WARNING*: Some target elements on target surface specified by real     
 constant set 275 belong to symmetric contact (e.g.  242 and 275), some  
 do not.                                                                 

 *** NOTE ***                            CP =      10.188   TIME= 11:41:18
 Smoothing on certain target nodes (e.g.160291) for pair ID 275 may      
 have accuracy issue.  Please verify element normal of connected target  
 elements (e.g.116533 & 116576).                                         

 *** NOTE ***                            CP =      10.797   TIME= 11:41:19
 It is highly recommended to use the auto contact setting option by      
 issuing CNCHECK,AUTO command for this problem in order to achieve       
 better convergence.                                                     

 *** NOTE ***                            CP =      10.797   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 57 and contact element type 57 has been set up.  The       
 companion pair has real constant set ID 58.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11164E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43825E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.797   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 82789 and target element 83023.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= 4.162816645E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 58 and contact element type 57 has been set up.  The       
 companion pair has real constant set ID 57.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11164E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37623E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32394E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64788E-01
 Average contact pair depth                   0.37623E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94056E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 82899 and target element 82609.                                 
 You may move entire target surface by : x= -5.23630289E-18, y=          
 -8.993364942E-05, z= -4.100852339E-17,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 59 and contact element type 59 has been set up.  The       
 companion pair has real constant set ID 60.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11036E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17223E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21919E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43837E-01
 Average contact pair depth                   0.17223E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43058E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 83396 and target element 83660.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= 4.162816038E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 60 and contact element type 59 has been set up.  The       
 companion pair has real constant set ID 59.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11036E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38059E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32373E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64747E-01
 Average contact pair depth                   0.38059E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95146E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 83598 and target element 83308.                                 
 You may move entire target surface by : x= -1.450546119E-18, y=         
 8.993356416E-05, z= 9.676711305E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 61 and contact element type 61 has been set up.  The       
 companion pair has real constant set ID 62.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10972E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17387E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21900E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43800E-01
 Average contact pair depth                   0.17387E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43467E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 84005 and target element 84262.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814827E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 62 and contact element type 61 has been set up.  The       
 companion pair has real constant set ID 61.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10972E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38278E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32384E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64769E-01
 Average contact pair depth                   0.38278E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95694E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 84138 and target element 83825.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 63 and contact element type 63 has been set up.  The       
 companion pair has real constant set ID 64.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11099E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17436E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21900E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43800E-01
 Average contact pair depth                   0.17436E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43590E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 84613 and target element 84848.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162819039E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 64 and contact element type 63 has been set up.  The       
 companion pair has real constant set ID 63.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11099E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37840E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32389E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64777E-01
 Average contact pair depth                   0.37840E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94600E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 84806 and target element 84524.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 65 and contact element type 65 has been set up.  The       
 companion pair has real constant set ID 66.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11136E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17373E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21918E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43836E-01
 Average contact pair depth                   0.17373E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43432E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 85222 and target element 85477.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814857E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 66 and contact element type 65 has been set up.  The       
 companion pair has real constant set ID 65.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11136E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37717E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32378E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64757E-01
 Average contact pair depth                   0.37717E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94293E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 85353 and target element 85042.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 67 and contact element type 67 has been set up.  The       
 companion pair has real constant set ID 68.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11637E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17455E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21935E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43870E-01
 Average contact pair depth                   0.17455E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43636E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 85829 and target element 86097.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.16281903E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 68 and contact element type 67 has been set up.  The       
 companion pair has real constant set ID 67.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11637E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36092E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28948E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57896E-01
 Average contact pair depth                   0.36092E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90229E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 85961 and target element 85649.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 69 and contact element type 69 has been set up.  The       
 companion pair has real constant set ID 70.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11498E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21925E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43849E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 86462 and target element 86696.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814821E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 70 and contact element type 69 has been set up.  The       
 companion pair has real constant set ID 69.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11498E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36527E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31208E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62417E-01
 Average contact pair depth                   0.36527E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91317E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993352533E-05 was detected between contact  
 element 86654 and target element 86372.                                 
 You may move entire target surface by : x= 5.866560076E-19, y=          
 8.993352533E-05, z= 9.676707127E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 71 and contact element type 71 has been set up.  The       
 companion pair has real constant set ID 72.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11712E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17320E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43824E-01
 Average contact pair depth                   0.17320E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43300E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 87069 and target element 87326.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162819003E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 72 and contact element type 71 has been set up.  The       
 companion pair has real constant set ID 71.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11712E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35862E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31204E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62408E-01
 Average contact pair depth                   0.35862E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.89654E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 87202 and target element 86889.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 73 and contact element type 73 has been set up.  The       
 companion pair has real constant set ID 74.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11231E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17354E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17354E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43384E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 87678 and target element 87940.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= 4.162816691E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 74 and contact element type 73 has been set up.  The       
 companion pair has real constant set ID 73.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11231E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37396E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31208E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62416E-01
 Average contact pair depth                   0.37396E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93491E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993352533E-05 was detected between contact  
 element 87878 and target element 87586.                                 
 You may move entire target surface by : x= -1.598128476E-18, y=         
 8.993352533E-05, z= -2.804076686E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 75 and contact element type 75 has been set up.  The       
 companion pair has real constant set ID 76.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11236E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17320E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43824E-01
 Average contact pair depth                   0.17320E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43300E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 88286 and target element 88507.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814826E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 76 and contact element type 75 has been set up.  The       
 companion pair has real constant set ID 75.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11236E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37380E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33959E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.67918E-01
 Average contact pair depth                   0.37380E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93449E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 88466 and target element 88196.                                 
 You may move entire target surface by : x= -5.903321888E-19, y=         
 8.993356416E-05, z= 4.787035643E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 77 and contact element type 77 has been set up.  The       
 companion pair has real constant set ID 78.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10826E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17383E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21900E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43800E-01
 Average contact pair depth                   0.17383E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43458E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 88869 and target element 89104.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162819064E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 78 and contact element type 77 has been set up.  The       
 companion pair has real constant set ID 77.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10826E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38796E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32398E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64796E-01
 Average contact pair depth                   0.38796E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96990E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 89062 and target element 88779.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 79 and contact element type 79 has been set up.  The       
 companion pair has real constant set ID 80.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11808E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18138E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22477E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.44955E-01
 Average contact pair depth                   0.18138E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.45346E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 89444 and target element 89697.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814844E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 80 and contact element type 79 has been set up.  The       
 companion pair has real constant set ID 79.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11808E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35570E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28307E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.56613E-01
 Average contact pair depth                   0.35570E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88925E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 89569 and target element 89284.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 81 and contact element type 81 has been set up.  The       
 companion pair has real constant set ID 82.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15953E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19573E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.39146E-01
 Average contact pair depth                   0.15953E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39883E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 89953 and target element 90038.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814853E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 82 and contact element type 81 has been set up.  The       
 companion pair has real constant set ID 81.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35045E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25853E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51706E-01
 Average contact pair depth                   0.35045E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.87613E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 89974 and target element 89869.                                 
 You may move entire target surface by : x= -1.501698361E-19, y=         
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 83 and contact element type 83 has been set up.  The       
 companion pair has real constant set ID 84.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12568E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15882E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19506E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.39012E-01
 Average contact pair depth                   0.15882E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39704E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559008852E-05 was detected between contact  
 element 90250 and target element 90349.                                 
 You may move entire target surface by : x= -1.122902607E-06, y=         
 -8.558272222E-05, z= -2.165879755E-11,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 84 and contact element type 83 has been set up.  The       
 companion pair has real constant set ID 83.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12568E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.33419E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25298E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50596E-01
 Average contact pair depth                   0.33419E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.83548E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993352533E-05 was detected between contact  
 element 90282 and target element 90166.                                 
 You may move entire target surface by : x= -1.598128476E-18, y=         
 8.993352533E-05, z= 4.787033576E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 85 and contact element type 85 has been set up.  The       
 companion pair has real constant set ID 86.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11467E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18599E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.23072E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.46145E-01
 Average contact pair depth                   0.18599E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.46498E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 90607 and target element 90823.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162817686E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 86 and contact element type 85 has been set up.  The       
 companion pair has real constant set ID 85.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11467E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36627E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31105E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62211E-01
 Average contact pair depth                   0.36627E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91568E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.812   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 90761 and target element 90523.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 87 and contact element type 87 has been set up.  The       
 companion pair has real constant set ID 88.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10768E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43825E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 91192 and target element 91447.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.16281477E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 88 and contact element type 87 has been set up.  The       
 companion pair has real constant set ID 87.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10768E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.39004E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32393E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64786E-01
 Average contact pair depth                   0.39004E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.97511E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 91323 and target element 91012.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 89 and contact element type 89 has been set up.  The       
 companion pair has real constant set ID 90.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12184E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17402E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21942E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43883E-01
 Average contact pair depth                   0.17402E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43505E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 91799 and target element 92067.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818998E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 90 and contact element type 89 has been set up.  The       
 companion pair has real constant set ID 89.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12184E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34470E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28938E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57877E-01
 Average contact pair depth                   0.34470E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.86176E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 91931 and target element 91619.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 91 and contact element type 91 has been set up.  The       
 companion pair has real constant set ID 92.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11728E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17354E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17354E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43385E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 92432 and target element 92665.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= 4.162819053E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 92 and contact element type 91 has been set up.  The       
 companion pair has real constant set ID 91.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11728E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35811E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62436E-01
 Average contact pair depth                   0.35811E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.89529E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 92541 and target element 92252.                                 
 You may move entire target surface by : x= -5.23630289E-18, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 93 and contact element type 93 has been set up.  The       
 companion pair has real constant set ID 94.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11261E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17455E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21929E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43859E-01
 Average contact pair depth                   0.17455E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43637E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 93039 and target element 93297.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162819038E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 94 and contact element type 93 has been set up.  The       
 companion pair has real constant set ID 93.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11261E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37296E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31209E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62417E-01
 Average contact pair depth                   0.37296E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93239E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 93173 and target element 92859.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 95 and contact element type 95 has been set up.  The       
 companion pair has real constant set ID 96.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11602E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17373E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21942E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43883E-01
 Average contact pair depth                   0.17373E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43432E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 93647 and target element 93905.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818942E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 96 and contact element type 95 has been set up.  The       
 companion pair has real constant set ID 95.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11602E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36202E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62436E-01
 Average contact pair depth                   0.36202E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90505E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 93781 and target element 93467.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 97 and contact element type 97 has been set up.  The       
 companion pair has real constant set ID 98.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11288E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17238E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21900E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43800E-01
 Average contact pair depth                   0.17238E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43096E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 94255 and target element 94476.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= 4.162816057E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 98 and contact element type 97 has been set up.  The       
 companion pair has real constant set ID 97.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11288E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37207E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33965E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.67930E-01
 Average contact pair depth                   0.37207E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93017E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 94364 and target element 94075.                                 
 You may move entire target surface by : x= -5.23630289E-18, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 99 and contact element type 99 has been set up.  The       
 companion pair has real constant set ID 100.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11861E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17391E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21929E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43858E-01
 Average contact pair depth                   0.17391E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43479E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 94839 and target element 95074.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818982E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 100 and contact element type 99 has been set up.  The      
 companion pair has real constant set ID 99.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11861E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35409E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32383E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64767E-01
 Average contact pair depth                   0.35409E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88522E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 95032 and target element 94748.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 101 and contact element type 101 has been set up.  The     
 companion pair has real constant set ID 102.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11657E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17436E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17436E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43590E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 95450 and target element 95703.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814798E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 102 and contact element type 101 has been set up.  The     
 companion pair has real constant set ID 101.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11657E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36029E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32379E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64757E-01
 Average contact pair depth                   0.36029E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90073E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 95579 and target element 95270.                                 
 You may move entire target surface by : x= -1.501698361E-19, y=         
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 103 and contact element type 103 has been set up.  The     
 companion pair has real constant set ID 104.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11418E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17489E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17489E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43723E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 96056 and target element 96312.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814874E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 104 and contact element type 103 has been set up.  The     
 companion pair has real constant set ID 103.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11418E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36783E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32383E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64767E-01
 Average contact pair depth                   0.36783E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91957E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 96188 and target element 95876.                                 
 You may move entire target surface by : x= -1.501698361E-19, y=         
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 105 and contact element type 105 has been set up.  The     
 companion pair has real constant set ID 106.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11198E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17402E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21923E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43846E-01
 Average contact pair depth                   0.17402E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43505E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 96663 and target element 96898.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162817691E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 106 and contact element type 105 has been set up.  The     
 companion pair has real constant set ID 105.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11198E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37506E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32384E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64768E-01
 Average contact pair depth                   0.37506E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93766E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 96856 and target element 96572.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 107 and contact element type 107 has been set up.  The     
 companion pair has real constant set ID 108.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11253E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17436E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17436E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43590E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 97272 and target element 97539.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814891E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 108 and contact element type 107 has been set up.  The     
 companion pair has real constant set ID 107.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11253E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37322E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.29035E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.58070E-01
 Average contact pair depth                   0.37322E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93306E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 97403 and target element 97092.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 109 and contact element type 109 has been set up.  The     
 companion pair has real constant set ID 110.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10487E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.67522E-03
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.22390E-01
 Average contact pair depth                   0.67522E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.16880E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 3.330669074E-16 was detected between contact  
 element 97813 and target element 97947.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 97916 and target element 97947.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 110 and contact element type 109 has been set up.  The     
 companion pair has real constant set ID 109.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10487E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38143E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.11922    
 Average contact pair depth                   0.38143E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95357E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 8.1071713E-03 was detected between contact    
 element 97932 and target element 97710.                                 
 You may move entire target surface by : x= -1.330375753E-18, y=         
 -8.1071713E-03, z= 3.816313692E-08,to reduce initial penetration.       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 111 and contact element type 111 has been set up.  The     
 companion pair has real constant set ID 112.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11928E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27156E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.15502E-01
 Average contact pair depth                   0.27156E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.67891E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 97991 and target element 98027.                                 
  
 Max.  Geometric gap 5.516840776E-04 has been detected between contact   
 element 98000 and target element 98027.                                 
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 112 and contact element type 111 has been set up.  The     
 companion pair has real constant set ID 111.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11928E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35212E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.11737    
 Average contact pair depth                   0.35212E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88030E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Min.  Initial gap 5.728620916E-03 was detected between contact element  
 98021 and target element 97982.                                         
 The gap is closed due to initial settings.                              
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 113 and contact element type 113 has been set up.  The     
 companion pair has real constant set ID 114.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10034E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.67178E-03
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.22342E-01
 Average contact pair depth                   0.67178E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.16795E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 98198 and target element 98333.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 98308 and target element 98333.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.828   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 114 and contact element type 113 has been set up.  The     
 companion pair has real constant set ID 113.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10034E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.39866E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.12931    
 Average contact pair depth                   0.39866E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.99664E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.1072301E-03 was detected between contact    
 element 98317 and target element 98156.                                 
 You may move entire target surface by : x= 1.574184064E-19, y=          
 -8.1072301E-03, z= 3.816341428E-08,to reduce initial penetration.       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 115 and contact element type 115 has been set up.  The     
 companion pair has real constant set ID 116.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10922E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27545E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.14809E-01
 Average contact pair depth                   0.27545E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.68862E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 98380 and target element 98411.                                 
  
 Max.  Geometric gap 1.145269919E-03 has been detected between contact   
 element 98381 and target element 98412.                                 
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 116 and contact element type 115 has been set up.  The     
 companion pair has real constant set ID 115.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10922E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38455E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.12818    
 Average contact pair depth                   0.38455E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96138E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 117 and contact element type 117 has been set up.  The     
 companion pair has real constant set ID 118.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10298E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.74505E-03
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.24712E-01
 Average contact pair depth                   0.74505E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18626E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 98560 and target element 98675.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 98644 and target element 98673.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 118 and contact element type 117 has been set up.  The     
 companion pair has real constant set ID 117.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10298E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38843E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.12243    
 Average contact pair depth                   0.38843E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.97108E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.1072301E-03 was detected between contact    
 element 98649 and target element 98461.                                 
 You may move entire target surface by : x= -1.57423643E-19, y=          
 -8.1072301E-03, z= -3.816341395E-08,to reduce initial penetration.      
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 119 and contact element type 119 has been set up.  The     
 companion pair has real constant set ID 120.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13779E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.29029E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.76545E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15309E-01
 Average contact pair depth                   0.29029E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.72573E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.33226763E-15 was detected between contact   
 element 98724 and target element 98765.                                 
  
 Max.  Geometric gap 5.516841203E-04 has been detected between contact   
 element 98733 and target element 98771.                                 
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 120 and contact element type 119 has been set up.  The     
 companion pair has real constant set ID 119.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13779E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.29450E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.49083E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.98167E-01
 Average contact pair depth                   0.29450E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.73625E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 121 and contact element type 121 has been set up.  The     
 companion pair has real constant set ID 122.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10383E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.74241E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12342E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24683E-01
 Average contact pair depth                   0.74241E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18560E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 98905 and target element 99032.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 99001 and target element 99044.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 122 and contact element type 121 has been set up.  The     
 companion pair has real constant set ID 121.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10383E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38524E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.58789E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11758    
 Average contact pair depth                   0.38524E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96309E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.1071713E-03 was detected between contact    
 element 99006 and target element 98785.                                 
 You may move entire target surface by : x= 1.33033867E-18, y=           
 -8.1071713E-03, z= -3.816313684E-08,to reduce initial penetration.      
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 123 and contact element type 123 has been set up.  The     
 companion pair has real constant set ID 124.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12819E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.28904E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.77549E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15510E-01
 Average contact pair depth                   0.28904E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.72259E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 99077 and target element 99113.                                 
  
 Max.  Geometric gap 5.516840776E-04 has been detected between contact   
 element 99091 and target element 99113.                                 
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 124 and contact element type 123 has been set up.  The     
 companion pair has real constant set ID 123.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12819E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.32764E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.54607E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10921    
 Average contact pair depth                   0.32764E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.81911E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Min.  Initial gap 3.794080692E-03 was detected between contact element  
 99106 and target element 99067.                                         
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 125 and contact element type 125 has been set up.  The     
 companion pair has real constant set ID 126.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10593E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37759E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.56164E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11233    
 Average contact pair depth                   0.37759E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94398E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.115374111E-03 was detected between contact  
 element 99488 and target element 100297.                                
 You may move entire target surface by : x= -3.374355362E-17, y=         
 -2.505102115E-03, z= -7.719051778E-03,to reduce initial penetration.    
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 126 and contact element type 125 has been set up.  The     
 companion pair has real constant set ID 125.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10593E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34093E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.56673E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11335    
 Average contact pair depth                   0.34093E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.85233E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.05300714E-02 was detected between contact   
 element 99957 and target element 99242.                                 
 You may move entire target surface by : x= 3.036964736E-18, y=          
 -6.136189423E-17, z= 1.05300714E-02,to reduce initial penetration.      
 *WARNING*: The detected penetration is larger than the pair based       
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 127 and contact element type 127 has been set up.  The     
 companion pair has real constant set ID 128.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10669E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37202E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.49023E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.98046E-01
 Average contact pair depth                   0.37202E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93005E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Min.  Initial gap 6.1950979E-03 was detected between contact element    
 100452 and target element 100570.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 128 and contact element type 127 has been set up.  The     
 companion pair has real constant set ID 127.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10669E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.39368E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33067E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.66134E-01
 Average contact pair depth                   0.39368E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.98420E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Min.  Initial gap 6.1950979E-03 was detected between contact element    
 100541 and target element 100420.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 129 and contact element type 129 has been set up.  The     
 companion pair has real constant set ID 130.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10944E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36549E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10381    
 Average contact pair depth                   0.36549E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91374E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Min.  Initial gap 9.804903E-03 was detected between contact element     
 100659 and target element 100773.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The detected gap is larger than the pair based pinball.      
 Please verify the pinball radius carefully.                             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 130 and contact element type 129 has been set up.  The     
 companion pair has real constant set ID 129.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10944E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37608E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33403E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.66806E-01
 Average contact pair depth                   0.37608E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94021E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Min.  Initial gap 9.804903E-03 was detected between contact element     
 100714 and target element 100630.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The detected gap is larger than the pair based pinball.      
 Please verify the pinball radius carefully.                             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 131 and contact element type 131 has been set up.  The     
 companion pair has real constant set ID 132.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68339E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38513E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.57691E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11538    
 Average contact pair depth                   0.38513E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96282E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 9.692389274E-03 was detected between contact  
 element 101150 and target element 101354.                               
 You may move entire target surface by : x= 2.021933325E-18, y=          
 -2.991904633E-03, z= 9.219051822E-03,to reduce initial penetration.     
 *WARNING*: The detected penetration is larger than the pair based       
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 132 and contact element type 131 has been set up.  The     
 companion pair has real constant set ID 131.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68339E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.61458E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10243E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.20486    
 Average contact pair depth                   0.61458E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.15365E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.247884654E-02 was detected between contact  
 element 101245 and target element 100930.                               
 You may move entire target surface by : x= 1.877065729E-18, y=          
 4.810942987E-18, z= -1.247884654E-02,to reduce initial penetration.     
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 133 and contact element type 133 has been set up.  The     
 companion pair has real constant set ID 134.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36272E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11579E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22340E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.44679E-01
 Average contact pair depth                   0.11579    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.28948E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 101370 and target element 101396.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 134 and contact element type 133 has been set up.  The     
 companion pair has real constant set ID 133.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36272E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15437E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25220E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50439E-01
 Average contact pair depth                   0.15437E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38593E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 101384 
 and target element 101359.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 135 and contact element type 135 has been set up.  The     
 companion pair has real constant set ID 136.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28622E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14674E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22943E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.45887E-01
 Average contact pair depth                   0.14674    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36686E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 101411 and target element 101450.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 136 and contact element type 135 has been set up.  The     
 companion pair has real constant set ID 135.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28622E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15444E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25328E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50656E-01
 Average contact pair depth                   0.15444E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38610E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 101432 
 and target element 101406.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 137 and contact element type 137 has been set up.  The     
 companion pair has real constant set ID 138.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.52769E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.79592E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13265E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.26531    
 Average contact pair depth                   0.79592E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19898E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 4.E-03 was detected between contact element   
 101465 and target element 101553.                                       
 You may move entire target surface by : x= 1.088634287E-17, y=          
 1.657933389E-17, z= 4.E-03,to reduce initial penetration.               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 138 and contact element type 137 has been set up.  The     
 companion pair has real constant set ID 137.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.52769E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14771E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14040E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28079E-01
 Average contact pair depth                   0.14771E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36928E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 101476 and target element 101452.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 139 and contact element type 139 has been set up.  The     
 companion pair has real constant set ID 140.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.70574E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.59512E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.99186E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.19837    
 Average contact pair depth                   0.59512E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.14878E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 140 and contact element type 139 has been set up.  The     
 companion pair has real constant set ID 139.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.70574E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.58176E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.16959E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.33917E-01
 Average contact pair depth                   0.58176E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.14544E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 101574 and target element 101563.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 141 and contact element type 141 has been set up.  The     
 companion pair has real constant set ID 142.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.53293E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.88822E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17764    
 Average contact pair depth                   0.53293E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13323E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 142 and contact element type 141 has been set up.  The     
 companion pair has real constant set ID 141.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69719E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24773E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49547E-01
 Average contact pair depth                   0.69719E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17430E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.844   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 101601 and target element 101595.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 143 and contact element type 143 has been set up.  The     
 companion pair has real constant set ID 144.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11973E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35079E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.58464E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11693    
 Average contact pair depth                   0.35079E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.87697E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.E-03 was detected between contact element   
 101696 and target element 101979.                                       
 You may move entire target surface by : x= 1.178561474E-17, y= -8.E-03, 
 z= 9.38202545E-19,to reduce initial penetration.                        
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 144 and contact element type 143 has been set up.  The     
 companion pair has real constant set ID 143.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11973E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19029E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28805E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57611E-01
 Average contact pair depth                   0.19029E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.47573E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 101758 and target element 101616.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 145 and contact element type 145 has been set up.  The     
 companion pair has real constant set ID 146.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11815E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35547E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.59245E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11849    
 Average contact pair depth                   0.35547E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88868E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.E-03 was detected between contact element   
 102180 and target element 102519.                                       
 You may move entire target surface by : x= -1.329399072E-17, y=         
 -8.E-03, z= -2.223577107E-19,to reduce initial penetration.             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 146 and contact element type 145 has been set up.  The     
 companion pair has real constant set ID 145.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11815E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17456E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27904E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.55809E-01
 Average contact pair depth                   0.17456E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43640E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 102207 and target element 102074.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 147 and contact element type 147 has been set up.  The     
 companion pair has real constant set ID 148.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79862E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.49517E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.26832E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.53665E-02
 Average contact pair depth                   0.49517E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12379E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 5.551115123E-17 was detected between contact  
 element 102577 and target element 102592.                               
  
 Max.  Geometric gap 2.02697948E-03 has been detected between contact    
 element 102570 and target element 102588.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 148 and contact element type 147 has been set up.  The     
 companion pair has real constant set ID 147.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79862E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.52591E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.87651E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17530    
 Average contact pair depth                   0.52591E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13148E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 149 and contact element type 149 has been set up.  The     
 companion pair has real constant set ID 150.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.54699E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.76784E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12797E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25595    
 Average contact pair depth                   0.76784E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19196E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 5.E-03 was detected between contact element   
 102696 and target element 103942.                                       
 You may move entire target surface by : x= 3.581433001E-18, y=          
 -2.290348622E-17, z= -5.E-03,to reduce initial penetration.             
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 150 and contact element type 149 has been set up.  The     
 companion pair has real constant set ID 149.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.54699E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10713E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.17855E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.35709E-01
 Average contact pair depth                   0.10713E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.26782E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 103373 and target element 102660.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 151 and contact element type 151 has been set up.  The     
 companion pair has real constant set ID 152.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.34706E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15203E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24804E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49608E-01
 Average contact pair depth                   0.15203E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38008E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 105073 
 and target element 105142.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 152 and contact element type 151 has been set up.  The     
 companion pair has real constant set ID 151.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.34706E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12102E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11145E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22290E-01
 Average contact pair depth                   0.12102    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.30254E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105111 and target element 105023.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 153 and contact element type 153 has been set up.  The     
 companion pair has real constant set ID 154.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15565E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25649E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51297E-01
 Average contact pair depth                   0.15565E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38913E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 154 and contact element type 153 has been set up.  The     
 companion pair has real constant set ID 153.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.67639E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13528E-01
 Average contact pair depth                   0.30625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.76563E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105182 and target element 105166.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 155 and contact element type 155 has been set up.  The     
 companion pair has real constant set ID 156.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.20984E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15444E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25328E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50656E-01
 Average contact pair depth                   0.15444E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38610E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 105214 
 and target element 105227.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 156 and contact element type 155 has been set up.  The     
 companion pair has real constant set ID 155.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.20984E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.20015E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22503E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.45007E-01
 Average contact pair depth                   0.20015    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.50038E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 2.664535259E-15 was detected between contact  
 element 105220 and target element 105185.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 157 and contact element type 157 has been set up.  The     
 companion pair has real constant set ID 158.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11284E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12806E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.15224E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.30447E-01
 Average contact pair depth                   0.12806E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.32016E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 105284 and target element 105397.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 158 and contact element type 157 has been set up.  The     
 companion pair has real constant set ID 157.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11284E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37220E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.87203E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17441E-01
 Average contact pair depth                   0.37220E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93050E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 1.33226763E-15 was detected between contact   
 element 105344 and target element 105255.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 159 and contact element type 159 has been set up.  The     
 companion pair has real constant set ID 160.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15619E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25600E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51201E-01
 Average contact pair depth                   0.15619E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39046E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 160 and contact element type 159 has been set up.  The     
 companion pair has real constant set ID 159.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11694E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23388E-01
 Average contact pair depth                   0.30625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.76563E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 105443 and target element 105427.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 161 and contact element type 161 has been set up.  The     
 companion pair has real constant set ID 162.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.27941E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15281E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24923E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49846E-01
 Average contact pair depth                   0.15281E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38202E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105522 and target element 105583.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 162 and contact element type 161 has been set up.  The     
 companion pair has real constant set ID 161.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.27941E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15032E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11186E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22372E-01
 Average contact pair depth                   0.15032    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37579E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105557 and target element 105479.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 163 and contact element type 163 has been set up.  The     
 companion pair has real constant set ID 164.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12904E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12676E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14927E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.29854E-01
 Average contact pair depth                   0.12676E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.31690E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105669 and target element 105765.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 164 and contact element type 163 has been set up.  The     
 companion pair has real constant set ID 163.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12904E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.32548E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.84725E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.16945E-01
 Average contact pair depth                   0.32548E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.81369E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105690 and target element 105607.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 165 and contact element type 165 has been set up.  The     
 companion pair has real constant set ID 166.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40232E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15061E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24462E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48924E-01
 Average contact pair depth                   0.15061E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37652E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 105822 and target element 105932.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 166 and contact element type 165 has been set up.  The     
 companion pair has real constant set ID 165.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.40232E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10440E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13947E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.27894E-01
 Average contact pair depth                   0.10440    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.26099E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 105869 and target element 105791.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 167 and contact element type 167 has been set up.  The     
 companion pair has real constant set ID 168.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.87707E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12701E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.15873E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.31745E-01
 Average contact pair depth                   0.12701E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.31752E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 105971 and target element 106017.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 168 and contact element type 167 has been set up.  The     
 companion pair has real constant set ID 167.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.87707E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.47887E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11026E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22052E-01
 Average contact pair depth                   0.47887E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.11972E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 106002 and target element 105950.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 169 and contact element type 169 has been set up.  The     
 companion pair has real constant set ID 170.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14230E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20299E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.40597E-01
 Average contact pair depth                   0.14230E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35575E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 106090 
 and target element 106125.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 170 and contact element type 169 has been set up.  The     
 companion pair has real constant set ID 169.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14417E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28833E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 106109 and target element 106054.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 171 and contact element type 171 has been set up.  The     
 companion pair has real constant set ID 172.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.48538E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15135E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24571E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49141E-01
 Average contact pair depth                   0.15135E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37837E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 106178 
 and target element 106290.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 172 and contact element type 171 has been set up.  The     
 companion pair has real constant set ID 171.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.48538E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.86530E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13039E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.26078E-01
 Average contact pair depth                   0.86530E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.21632E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 106236 and target element 106138.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 173 and contact element type 173 has been set up.  The     
 companion pair has real constant set ID 174.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18830E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15437E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25220E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50439E-01
 Average contact pair depth                   0.15437E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38593E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106322 and target element 106335.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.859   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 174 and contact element type 173 has been set up.  The     
 companion pair has real constant set ID 173.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18830E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.22305E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.23006E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.46013E-01
 Average contact pair depth                   0.22305    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.55763E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106332 and target element 106304.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 175 and contact element type 175 has been set up.  The     
 companion pair has real constant set ID 176.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11601E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12702E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.15559E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.31117E-01
 Average contact pair depth                   0.12702E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.31755E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 106394 and target element 106434.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 176 and contact element type 175 has been set up.  The     
 companion pair has real constant set ID 175.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11601E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36204E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10598E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.21196E-01
 Average contact pair depth                   0.36204E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90510E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 106406 and target element 106345.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 177 and contact element type 177 has been set up.  The     
 companion pair has real constant set ID 178.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13811E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19315E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38631E-01
 Average contact pair depth                   0.13811E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.34528E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 106492 
 and target element 106530.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 178 and contact element type 177 has been set up.  The     
 companion pair has real constant set ID 177.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14417E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28833E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 106513 and target element 106445.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 179 and contact element type 179 has been set up.  The     
 companion pair has real constant set ID 180.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11309E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11714E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11764E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23528E-01
 Average contact pair depth                   0.11714E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29286E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106560 and target element 106598.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 180 and contact element type 179 has been set up.  The     
 companion pair has real constant set ID 179.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11309E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37138E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12111E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24221E-01
 Average contact pair depth                   0.37138E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.92845E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106575 and target element 106550.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 181 and contact element type 181 has been set up.  The     
 companion pair has real constant set ID 182.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41485E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15360E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25018E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50036E-01
 Average contact pair depth                   0.15360E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38400E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 106624 
 and target element 106643.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 182 and contact element type 181 has been set up.  The     
 companion pair has real constant set ID 181.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41485E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10124E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24274E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48547E-01
 Average contact pair depth                   0.10124    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.25310E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106635 and target element 106613.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 183 and contact element type 183 has been set up.  The     
 companion pair has real constant set ID 184.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13872E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19315E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38631E-01
 Average contact pair depth                   0.13872E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.34681E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 106692 and target element 106737.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 184 and contact element type 183 has been set up.  The     
 companion pair has real constant set ID 183.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13669E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.27338E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 106724 and target element 106653.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 185 and contact element type 185 has been set up.  The     
 companion pair has real constant set ID 186.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.16182E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14318E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20889E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.41778E-01
 Average contact pair depth                   0.14318E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35796E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 3.330669074E-16 was detected between contact  
 element 106849 and target element 106900.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 186 and contact element type 185 has been set up.  The     
 companion pair has real constant set ID 185.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.16182E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.25955E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19382E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38764E-01
 Average contact pair depth                   0.25955E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.64888E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106866 and target element 106783.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 187 and contact element type 187 has been set up.  The     
 companion pair has real constant set ID 188.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12193E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11651E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12118E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24236E-01
 Average contact pair depth                   0.11651E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29129E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106937 and target element 106960.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 188 and contact element type 187 has been set up.  The     
 companion pair has real constant set ID 187.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12193E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34447E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11642E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23283E-01
 Average contact pair depth                   0.34447E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.86118E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106949 and target element 106906.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 189 and contact element type 189 has been set up.  The     
 companion pair has real constant set ID 190.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.85740E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15311E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25047E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50094E-01
 Average contact pair depth                   0.15311E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38277E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 107000 and target element 107011.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 190 and contact element type 189 has been set up.  The     
 companion pair has real constant set ID 189.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.85740E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.48985E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27588E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.55176E-01
 Average contact pair depth                   0.48985E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12246E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 107006 and target element 106985.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 191 and contact element type 191 has been set up.  The     
 companion pair has real constant set ID 192.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14230E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20299E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.40597E-01
 Average contact pair depth                   0.14230E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35575E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 107051 and target element 107106.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 192 and contact element type 191 has been set up.  The     
 companion pair has real constant set ID 191.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13669E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.27338E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107095 and target element 107033.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 193 and contact element type 193 has been set up.  The     
 companion pair has real constant set ID 194.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18083E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14485E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21413E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.42826E-01
 Average contact pair depth                   0.14485E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36213E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 107204 and target element 107272.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 194 and contact element type 193 has been set up.  The     
 companion pair has real constant set ID 193.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18083E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23226E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19103E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38207E-01
 Average contact pair depth                   0.23226E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.58064E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 107244 and target element 107151.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 195 and contact element type 195 has been set up.  The     
 companion pair has real constant set ID 196.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12084E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13895E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19986E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.39972E-01
 Average contact pair depth                   0.13895E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.34737E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.736385355E-03 was detected between contact  
 element 107418 and target element 107468.                               
 You may move entire target surface by : x= 2.301910549E-17, y=          
 -2.736385355E-03, z= 3.452865824E-17,to reduce initial penetration.     
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 196 and contact element type 195 has been set up.  The     
 companion pair has real constant set ID 195.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12084E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34757E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.37441E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.74882E-01
 Average contact pair depth                   0.34757E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.86891E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.083423978E-03 was detected between contact  
 element 107432 and target element 107344.                               
 You may move entire target surface by : x= -6.310791901E-04, y=         
 8.803925556E-04, z= -2.134291991E-05,to reduce initial penetration.     
  
 Max.  Geometric gap 8.577457626E-03 has been detected between contact   
 element 107428 and target element 107284.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 197 and contact element type 197 has been set up.  The     
 companion pair has real constant set ID 198.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11307E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11824E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11743E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23485E-01
 Average contact pair depth                   0.11824E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29559E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107530 and target element 107623.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 198 and contact element type 197 has been set up.  The     
 companion pair has real constant set ID 197.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11307E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37145E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.91773E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.18355E-01
 Average contact pair depth                   0.37145E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.92862E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107564 and target element 107510.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 199 and contact element type 199 has been set up.  The     
 companion pair has real constant set ID 200.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79719E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15360E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25018E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50036E-01
 Average contact pair depth                   0.15360E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38400E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 107666 
 and target element 107676.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 200 and contact element type 199 has been set up.  The     
 companion pair has real constant set ID 199.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79719E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.52685E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.37798E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.75596E-01
 Average contact pair depth                   0.52685E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13171E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 107672 and target element 107650.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 201 and contact element type 201 has been set up.  The     
 companion pair has real constant set ID 202.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14163E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20589E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.41178E-01
 Average contact pair depth                   0.14163E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35408E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 2.750796574E-03 was detected between contact  
 element 107826 and target element 107878.                               
 You may move entire target surface by : x= -9.545563003E-18, y=         
 2.750796574E-03, z= -1.315037021E-17,to reduce initial penetration.     
  
 Max.  Geometric gap 5.E-03 has been detected between contact element    
 107778 and target element 107867.                                       
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 202 and contact element type 201 has been set up.  The     
 companion pair has real constant set ID 201.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35043E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.36614E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.73228E-01
 Average contact pair depth                   0.35043E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.87608E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Max.  Initial penetration 1.328182736E-03 was detected between contact  
 element 107843 and target element 107752.                               
 You may move entire target surface by : x= -8.265569157E-04, y=         
 -1.039517467E-03, z= -1.662770659E-05,to reduce initial penetration.    
  
 Max.  Geometric gap 7.046557409E-03 has been detected between contact   
 element 107838 and target element 107689.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.875   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 203 and contact element type 203 has been set up.  The     
 companion pair has real constant set ID 204.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11875E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11813E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12077E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24154E-01
 Average contact pair depth                   0.11813E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29531E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 107937 and target element 108046.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 204 and contact element type 203 has been set up.  The     
 companion pair has real constant set ID 203.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11875E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35367E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.88277E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17655E-01
 Average contact pair depth                   0.35367E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88418E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107989 and target element 107901.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 205 and contact element type 205 has been set up.  The     
 companion pair has real constant set ID 206.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.59139E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15311E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25047E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50094E-01
 Average contact pair depth                   0.15311E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38277E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 108072 
 and target element 108087.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 206 and contact element type 205 has been set up.  The     
 companion pair has real constant set ID 205.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.59139E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.71019E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27399E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54799E-01
 Average contact pair depth                   0.71019E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17755E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 108081 and target element 108062.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 207 and contact element type 207 has been set up.  The     
 companion pair has real constant set ID 208.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.81529E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.51515E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24285E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48571E-01
 Average contact pair depth                   0.51515E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12879E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 4.303286342E-04 was detected between contact  
 element 108183 and target element 108326.                               
 You may move entire target surface by : x= -2.320328472E-04, y=         
 -3.616434518E-04, z= -2.361154317E-05,to reduce initial penetration.    
  
 Max.  Geometric gap 9.E-03 has been detected between contact element    
 108156 and target element 108288.                                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 208 and contact element type 207 has been set up.  The     
 companion pair has real constant set ID 207.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.81529E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16450E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25670E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51340E-01
 Average contact pair depth                   0.16450E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.41125E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 3.615199155E-04 was detected between contact  
 element 108267 and target element 108120.                               
 You may move entire target surface by : x= 2.227331075E-04, y=          
 2.847570598E-04, z= 1.702904744E-07,to reduce initial penetration.      
  
 Max.  Geometric gap 3.184938432E-03 has been detected between contact   
 element 108259 and target element 108144.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 209 and contact element type 209 has been set up.  The     
 companion pair has real constant set ID 210.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.66576E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.63085E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24828E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49655E-01
 Average contact pair depth                   0.63085E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.15771E-01

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 One of the contact searching regions contains at least 55 target        
 elements.  You may reduce the pinball radius.                           
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 4.491127571E-04 was detected between contact  
 element 108425 and target element 108556.                               
 You may move entire target surface by : x= -2.208559608E-04, y=         
 3.907190955E-04, z= -1.623273335E-05,to reduce initial penetration.     
  
 Max.  Geometric gap 9.E-03 has been detected between contact element    
 108405 and target element 108542.                                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 210 and contact element type 209 has been set up.  The     
 companion pair has real constant set ID 209.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.66576E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16415E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25436E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50872E-01
 Average contact pair depth                   0.16415E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.41039E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 3.997438332E-04 was detected between contact  
 element 108494 and target element 108360.                               
 You may move entire target surface by : x= 2.462826662E-04, y=          
 -3.148649632E-04, z= 1.882939812E-07,to reduce initial penetration.     
  
 Max.  Geometric gap 3.176739077E-03 has been detected between contact   
 element 108509 and target element 108390.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 211 and contact element type 211 has been set up.  The     
 companion pair has real constant set ID 212.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.78817E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37162E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.60085E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12017    
 Average contact pair depth                   0.37162E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.92905E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 108674 
 and target element 108971.                                              
  
 Max.  Geometric gap 7.349455406E-04 has been detected between contact   
 element 108700 and target element 108921.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 212 and contact element type 211 has been set up.  The     
 companion pair has real constant set ID 211.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.78817E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.53288E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14483E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28966E-01
 Average contact pair depth                   0.53288E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13322E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 5.551115123E-17 was detected between contact  
 element 108746 and target element 108617.                               
  
 Max.  Geometric gap 9.748335779E-04 has been detected between contact   
 element 108872 and target element 108646.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 213 and contact element type 213 has been set up.  The     
 companion pair has real constant set ID 214.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27000E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13263E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.26527E-01
 Average contact pair depth                   0.27000E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.67500E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 3.E-03 was detected between contact element 109040    
 and target element 109058.                                              
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 214 and contact element type 213 has been set up.  The     
 companion pair has real constant set ID 213.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69719E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24773E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49547E-01
 Average contact pair depth                   0.69719E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17430E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 3.E-03 was detected between contact element 109048    
 and target element 109035.                                              
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 215 and contact element type 215 has been set up.  The     
 companion pair has real constant set ID 216.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.86566E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14428E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28855E-01
 Average contact pair depth                   0.86566E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.21641E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 216 and contact element type 215 has been set up.  The     
 companion pair has real constant set ID 215.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16331E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54436E-01
 Average contact pair depth                   0.16331E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.40827E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 217 and contact element type 217 has been set up.  The     
 companion pair has real constant set ID 218.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55030E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.59264E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.17600E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.35200E-01
 Average contact pair depth                   0.59264E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.14816E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 109107 and target element 109122.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 218 and contact element type 217 has been set up.  The     
 companion pair has real constant set ID 217.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55030E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.76323E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12720E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25441    
 Average contact pair depth                   0.76323E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19081E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 219 and contact element type 219 has been set up.  The     
 companion pair has real constant set ID 220.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68228E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.61558E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10260E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.20519    
 Average contact pair depth                   0.61558E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.15390E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 109209 
 and target element 109407.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 220 and contact element type 219 has been set up.  The     
 companion pair has real constant set ID 219.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68228E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.28146E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.46911E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.93821E-01
 Average contact pair depth                   0.28146E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.70366E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 5.E-03 was detected between contact element   
 109331 and target element 109172.                                       
 You may move entire target surface by : x= -2.010731742E-17, y=         
 2.902074441E-18, z= 5.E-03,to reduce initial penetration.               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 221 and contact element type 221 has been set up.  The     
 companion pair has real constant set ID 222.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61202E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.68625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24168E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48335E-01
 Average contact pair depth                   0.68625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17156E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 3.E-03 was detected between contact element 109467    
 and target element 109481.                                              
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 222 and contact element type 221 has been set up.  The     
 companion pair has real constant set ID 221.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61202E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27000E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.76685E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15337E-01
 Average contact pair depth                   0.27000E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.67500E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 3.E-03 was detected between contact element 109472    
 and target element 109462.                                              
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 223 and contact element type 223 has been set up.  The     
 companion pair has real constant set ID 224.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55205E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.68625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24168E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48335E-01
 Average contact pair depth                   0.68625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17156E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 109495 and target element 109505.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 224 and contact element type 223 has been set up.  The     
 companion pair has real constant set ID 223.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55205E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.76080E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12680E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25360    
 Average contact pair depth                   0.76080E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19020E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 225 and contact element type 225 has been set up.  The     
 companion pair has real constant set ID 226.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.90930E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.46190E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.76983E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15397    
 Average contact pair depth                   0.46190E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.11547E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 3.550953997E-04 was detected between contact element  
 109515 and target element 109553.                                       
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 226 and contact element type 225 has been set up.  The     
 companion pair has real constant set ID 225.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.90930E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34008E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.65113E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13023E-01
 Average contact pair depth                   0.34008E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.85020E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 109524 and target element 109508.                               
  
 Max.  Geometric gap 8.36518718E-04 has been detected between contact    
 element 109525 and target element 109507.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 227 and contact element type 227 has been set up.  The     
 companion pair has real constant set ID 228.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.92251E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.45528E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.75880E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15176    
 Average contact pair depth                   0.45528E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.11382E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Min.  Initial gap 4.163715002E-04 was detected between contact element  
 109574 and target element 109603.                                       
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 228 and contact element type 227 has been set up.  The     
 companion pair has real constant set ID 227.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.92251E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40998E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.64747E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12949E-01
 Average contact pair depth                   0.40998E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10249E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 109582 and target element 109565.                               
  
 Max.  Geometric gap 8.338280895E-04 has been detected between contact   
 element 109593 and target element 109566.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 229 and contact element type 229 has been set up.  The     
 companion pair has real constant set ID 230.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79313E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.47513E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.79188E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15838    
 Average contact pair depth                   0.47513E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.11878E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 109655 
 and target element 109936.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 230 and contact element type 229 has been set up.  The     
 companion pair has real constant set ID 229.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79313E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.52955E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14472E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28944E-01
 Average contact pair depth                   0.52955E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13239E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 1.33226763E-15 was detected between contact   
 element 109678 and target element 109627.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 231 and contact element type 231 has been set up.  The     
 companion pair has real constant set ID 232.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61026E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.68823E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11471E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22941    
 Average contact pair depth                   0.68823E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17206E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 6.E-03 was detected between contact element   
 110044 and target element 110201.                                       
 You may move entire target surface by : x= -4.837491939E-17, y=         
 -5.126235495E-18, z= -6.E-03,to reduce initial penetration.             
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 232 and contact element type 231 has been set up.  The     
 companion pair has real constant set ID 231.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61026E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.28146E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.46911E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.93821E-01
 Average contact pair depth                   0.28146E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.70366E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Max.  Initial penetration 6.E-03 was detected between contact element   
 110116 and target element 109990.                                       
 You may move entire target surface by : x= -4.158712246E-17, y=         
 2.497455176E-17, z= 6.E-03,to reduce initial penetration.               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.891   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 233 and contact element type 233 has been set up.  The     
 companion pair has real constant set ID 234.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.53998E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14771E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12175E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24349E-01
 Average contact pair depth                   0.14771E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36928E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 110326 and target element 110374.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 234 and contact element type 233 has been set up.  The     
 companion pair has real constant set ID 233.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.53998E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.77780E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12963E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25927    
 Average contact pair depth                   0.77780E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19445E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 4.E-03 was detected between contact element   
 110370 and target element 110311.                                       
 You may move entire target surface by : x= 3.142449627E-18, y=          
 -5.743553805E-17, z= 4.E-03,to reduce initial penetration.              
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 235 and contact element type 235 has been set up.  The     
 companion pair has real constant set ID 236.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.86566E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14428E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28855E-01
 Average contact pair depth                   0.86566E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.21641E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 236 and contact element type 235 has been set up.  The     
 companion pair has real constant set ID 235.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16331E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54436E-01
 Average contact pair depth                   0.16331E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.40827E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 237 and contact element type 237 has been set up.  The     
 companion pair has real constant set ID 238.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10291E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40813E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.68022E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13604    
 Average contact pair depth                   0.40813E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10203E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.E-03 was detected between contact element   
 110521 and target element 110818.                                       
 You may move entire target surface by : x= 2.240400286E-17, y= 8.E-03,  
 z= -2.473432853E-17,to reduce initial penetration.                      
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 238 and contact element type 237 has been set up.  The     
 companion pair has real constant set ID 237.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10291E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19225E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28954E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57908E-01
 Average contact pair depth                   0.19225E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48061E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 110556 and target element 110413.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 239 and contact element type 239 has been set up.  The     
 companion pair has real constant set ID 240.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10456E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40167E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.66945E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13389    
 Average contact pair depth                   0.40167E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10042E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.E-03 was detected between contact element   
 110933 and target element 111240.                                       
 You may move entire target surface by : x= -1.486686244E-16, y= 8.E-03, 
 z= 2.628680716E-18,to reduce initial penetration.                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 240 and contact element type 239 has been set up.  The     
 companion pair has real constant set ID 239.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10456E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17806E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28393E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.56787E-01
 Average contact pair depth                   0.17806E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.44516E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 111078 and target element 110901.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 241 and contact element type 241 has been set up.  The     
 companion pair has real constant set ID 242.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness       5299.0    
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13546E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27145E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54290E-01
 Average contact pair depth                   0.13546    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.33866E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 111501 and target element 111743.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 242 and contact element type 241 has been set up.  The     
 companion pair has real constant set ID 241.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness       5299.0    
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.79261E+09
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10631E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.21263    
 Average contact pair depth                   0.79261E+10
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19815E+10
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 111697 and target element 111366.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 243 and contact element type 243 has been set up.  The     
 companion pair has real constant set ID 244.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55389E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.75828E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12638E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25276    
 Average contact pair depth                   0.75828E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18957E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 5.E-03 was detected between contact element   
 111840 and target element 113431.                                       
 You may move entire target surface by : x= 2.604679454E-18, y=          
 -2.290348148E-17, z= -5.E-03,to reduce initial penetration.             
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 244 and contact element type 243 has been set up.  The     
 companion pair has real constant set ID 243.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55389E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10604E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.17673E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.35346E-01
 Average contact pair depth                   0.10604E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.26510E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 112571 and target element 111824.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 245 and contact element type 245 has been set up.  The     
 companion pair has real constant set ID 246.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61303E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40709E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.52605E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10521E-01
 Average contact pair depth                   0.40709E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10177E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 114200 and target element 114231.                               
  
 Max.  Geometric gap 3.948435618E-04 has been detected between contact   
 element 114202 and target element 114234.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 246 and contact element type 245 has been set up.  The     
 companion pair has real constant set ID 245.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.61303E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.68512E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51628E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10326    
 Average contact pair depth                   0.68512E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17128E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 114221 
 and target element 114163.                                              
  
 Max.  Geometric gap 3.423602906E-04 has been detected between contact   
 element 114227 and target element 114170.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 247 and contact element type 247 has been set up.  The     
 companion pair has real constant set ID 248.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38012E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.63353E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12671    
 Average contact pair depth                   0.38012E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95030E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 114393 and target element 114456.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 248 and contact element type 247 has been set up.  The     
 companion pair has real constant set ID 247.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69901E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48996E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97993E-01
 Average contact pair depth                   0.69901E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17475E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 114417 and target element 114246.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 249 and contact element type 249 has been set up.  The     
 companion pair has real constant set ID 250.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.39634E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18610E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31016E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62032E-01
 Average contact pair depth                   0.18610E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.46524E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 114485 
 and target element 114532.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 250 and contact element type 249 has been set up.  The     
 companion pair has real constant set ID 249.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.39634E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10597E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.38919E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.77838E-02
 Average contact pair depth                   0.10597    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.26492E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 114520 and target element 114468.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 251 and contact element type 251 has been set up.  The     
 companion pair has real constant set ID 252.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10347E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38920E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.54853E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10971E-01
 Average contact pair depth                   0.38920E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.97299E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 114581 and target element 114625.                               
  
 Max.  Geometric gap 1.70535368E-04 has been detected between contact    
 element 114588 and target element 114623.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 252 and contact element type 251 has been set up.  The     
 companion pair has real constant set ID 251.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10347E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40591E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48531E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97063E-01
 Average contact pair depth                   0.40591E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10148E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 114618 
 and target element 114573.                                              
  
 Max.  Geometric gap 1.952835099E-05 has been detected between contact   
 element 114613 and target element 114556.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 253 and contact element type 253 has been set up.  The     
 companion pair has real constant set ID 254.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38536E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.64226E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12845    
 Average contact pair depth                   0.38536E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96340E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 114736 and target element 114844.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 254 and contact element type 253 has been set up.  The     
 companion pair has real constant set ID 253.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69901E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48996E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97993E-01
 Average contact pair depth                   0.69901E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17475E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 114820 and target element 114708.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 255 and contact element type 255 has been set up.  The     
 companion pair has real constant set ID 256.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37836E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18170E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.30283E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.60566E-01
 Average contact pair depth                   0.18170E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.45424E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 114868 
 and target element 114934.                                              
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 256 and contact element type 255 has been set up.  The     
 companion pair has real constant set ID 255.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37836E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11100E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.41877E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.83754E-02
 Average contact pair depth                   0.11100    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.27751E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 114899 and target element 114860.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 257 and contact element type 257 has been set up.  The     
 companion pair has real constant set ID 258.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12801E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23447E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.39078E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.78156E-01
 Average contact pair depth                   0.23447E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.58617E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 115135 and target element 115304.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 258 and contact element type 257 has been set up.  The     
 companion pair has real constant set ID 257.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12801E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.32811E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.54684E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10937    
 Average contact pair depth                   0.32811E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.82027E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 7.6E-03 was detected between contact element  
 115193 and target element 114986.                                       
 You may move entire target surface by : x= 7.6E-03, y=                  
 -6.453458065E-17, z= -3.543835954E-17,to reduce initial penetration.    
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 259 and contact element type 259 has been set up.  The     
 companion pair has real constant set ID 260.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.26830E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14967E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10820E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.21641E-01
 Average contact pair depth                   0.14967E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37418E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 0 was detected between contact element 115389 
 and target element 115429.                                              
  
 Max.  Geometric gap 2.507126131E-03 has been detected between contact   
 element 115382 and target element 115427.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 260 and contact element type 259 has been set up.  The     
 companion pair has real constant set ID 259.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.26830E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15654E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.66356E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13271    
 Average contact pair depth                   0.15654    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39135E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 115424 and target element 115340.                               
  
 Max.  Geometric gap 2.340511227E-03 has been detected between contact   
 element 115421 and target element 115325.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 261 and contact element type 261 has been set up.  The     
 companion pair has real constant set ID 262.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.15400E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23622E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.39370E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.78740E-01
 Average contact pair depth                   0.23622E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.59055E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 3.552713679E-15 was detected between contact  
 element 115574 and target element 115797.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 262 and contact element type 261 has been set up.  The     
 companion pair has real constant set ID 261.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.15400E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27272E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.45454E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.90907E-01
 Average contact pair depth                   0.27272E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.68180E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Max.  Initial penetration 7.6E-03 was detected between contact element  
 115756 and target element 115540.                                       
 You may move entire target surface by : x= 7.6E-03, y= 5.772459315E-17, 
 z= -7.505767071E-17,to reduce initial penetration.                      
 *WARNING*: The detected penetration is larger than the pair based       
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.906   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 263 and contact element type 263 has been set up.  The     
 companion pair has real constant set ID 264.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28794E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15000E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11183E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22366E-01
 Average contact pair depth                   0.15000E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37499E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 115916 and target element 115963.                               
  
 Max.  Geometric gap 2.253430249E-03 has been detected between contact   
 element 115949 and target element 115962.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 264 and contact element type 263 has been set up.  The     
 companion pair has real constant set ID 263.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28794E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14586E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.66411E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13282    
 Average contact pair depth                   0.14586    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36466E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 115955 and target element 115861.                               
  
 Max.  Geometric gap 2.159995441E-03 has been detected between contact   
 element 115956 and target element 115903.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 265 and contact element type 265 has been set up.  The     
 companion pair has real constant set ID 266.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11833E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35494E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.30208E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.60417E-01
 Average contact pair depth                   0.35494E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88735E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 266 and contact element type 265 has been set up.  The     
 companion pair has real constant set ID 265.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11833E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.31171E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51952E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10390    
 Average contact pair depth                   0.31171E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77927E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 267 and contact element type 267 has been set up.  The     
 companion pair has real constant set ID 268.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.38357E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10950E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.29236E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.58472E-01
 Average contact pair depth                   0.10950    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.27375E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Min.  Initial gap 1.1E-02 was detected between contact element 115986   
 and target element 115992.                                              
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 268 and contact element type 267 has been set up.  The     
 companion pair has real constant set ID 267.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.38357E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.31171E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51952E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10390    
 Average contact pair depth                   0.31171E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77927E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 269 and contact element type 269 has been set up.  The     
 companion pair has real constant set ID 270.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.57934E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.72496E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.29722E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.59444E-01
 Average contact pair depth                   0.72496E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18124E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 116011 and target element 116052.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 270 and contact element type 269 has been set up.  The     
 companion pair has real constant set ID 269.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.57934E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30564E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.50598E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10120    
 Average contact pair depth                   0.30564E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.76410E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Min.  Initial gap 2.910475675E-03 was detected between contact element  
 116029 and target element 115999.                                       
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 3.652822432E-03 has been detected between contact   
 element 116036 and target element 115995.                               
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 271 and contact element type 271 has been set up.  The     
 companion pair has real constant set ID 272.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30851E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51418E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10284    
 Average contact pair depth                   0.30851E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77126E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 272 and contact element type 271 has been set up.  The     
 companion pair has real constant set ID 271.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.25656E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.42456E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.84913E-01
 Average contact pair depth                   0.25656E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.64140E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 116091 and target element 116072.                               
  
 Max.  Geometric gap 7.627606316E-03 has been detected between contact   
 element 116101 and target element 116075.                               
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 273 and contact element type 273 has been set up.  The     
 companion pair has real constant set ID 274.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30851E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51418E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10284    
 Average contact pair depth                   0.30851E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77126E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 274 and contact element type 273 has been set up.  The     
 companion pair has real constant set ID 273.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27235E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.45391E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.90782E-01
 Average contact pair depth                   0.27235E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.68087E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 116139 and target element 116129.                               
  
 Max.  Geometric gap 7.5E-03 has been detected between contact element   
 116141 and target element 116129.                                       
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Deformable-deformable contact pair identified by real constant set 275  
 and contact element type 275 has been set up.                           
 Node-surface contact pair is defined
 Contact force based contact model
 Contact algorithm: Augmented Lagrange method
 Contact detection at: nodal point (normal to target surface)
 *WARNING*: Smoothing on certain contact/target nodes (for example       
 160291) may have an accuracy issue.  You may switch contact and target  
 surfaces, or split the current pair into multiple pairs, or use Gauss   
 detection.                                                              
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21404E+14
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.50962E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25481E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50962E-01
 Average contact pair depth                   0.50962E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12740E-01
 Default target edge extension factor TOLS     10.000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      10.922   TIME= 11:41:19
 Max.  Initial penetration 9.795602115E-17 was detected between contact  
 element 116296 and target element 116544.                               
 ****************************************
  
  
  

  
  
     D I S T R I B U T E D   D O M A I N   D E C O M P O S E R
  
  ...Number of elements: 125689
  ...Number of nodes:    176706
  ...Decompose to 2 CPU domains
  ...Element load balance ratio =     1.011


                      L O A D   S T E P   O P T I O N S

   LOAD STEP NUMBER. . . . . . . . . . . . . . . .     1
   TIME AT END OF THE LOAD STEP. . . . . . . . . .  1.0000    
   AUTOMATIC TIME STEPPING . . . . . . . . . . . .    ON
      INITIAL NUMBER OF SUBSTEPS . . . . . . . . .     1
      MAXIMUM NUMBER OF SUBSTEPS . . . . . . . . .     1
      MINIMUM NUMBER OF SUBSTEPS . . . . . . . . .     1
   MAXIMUM NUMBER OF EQUILIBRIUM ITERATIONS. . . .     1
   STEP CHANGE BOUNDARY CONDITIONS . . . . . . . .    NO
   TERMINATE ANALYSIS IF NOT CONVERGED . . . . . .YES (EXIT)  
   CONVERGENCE CONTROLS. . . . . . . . . . . . . .USE DEFAULTS
   PRINT OUTPUT CONTROLS . . . . . . . . . . . . .NO PRINTOUT
   DATABASE OUTPUT CONTROLS
      ITEM     FREQUENCY   COMPONENT
       ALL       NONE               
      NSOL        ALL               
      RSOL        ALL               
      STRS        ALL               
      EPEL        ALL               
      EPPL        ALL               
      EPTH        ALL               


 SOLUTION MONITORING INFO IS WRITTEN TO FILE= file.mntr                                                                                                                                                                                                                                                           
 *WARNING*: Some target elements on target surface specified by real     
 constant set 275 belong to symmetric contact (e.g.  242 and 275), some  
 do not.                                                                 

 *** NOTE ***                            CP =      15.266   TIME= 11:41:22
 Smoothing on certain target nodes (e.g.160291) for pair ID 275 may      
 have accuracy issue.  Please verify element normal of connected target  
 elements (e.g.116533 & 116576).                                         

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 57 and contact element type 57 has been set up.  The       
 companion pair has real constant set ID 58.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11164E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43825E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 82789 and target element 83023.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= 4.162816645E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 58 and contact element type 57 has been set up.  The       
 companion pair has real constant set ID 57.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11164E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37623E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32394E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64788E-01
 Average contact pair depth                   0.37623E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94056E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 82899 and target element 82609.                                 
 You may move entire target surface by : x= -5.23630289E-18, y=          
 -8.993364942E-05, z= -4.100852339E-17,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 59 and contact element type 59 has been set up.  The       
 companion pair has real constant set ID 60.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11036E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17223E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21919E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43837E-01
 Average contact pair depth                   0.17223E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43058E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 83396 and target element 83660.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= 4.162816038E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 60 and contact element type 59 has been set up.  The       
 companion pair has real constant set ID 59.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11036E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38059E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32373E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64747E-01
 Average contact pair depth                   0.38059E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95146E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 83598 and target element 83308.                                 
 You may move entire target surface by : x= -1.450546119E-18, y=         
 8.993356416E-05, z= 9.676711305E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 63 and contact element type 63 has been set up.  The       
 companion pair has real constant set ID 64.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11099E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17436E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21900E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43800E-01
 Average contact pair depth                   0.17436E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43590E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 84613 and target element 84848.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162819039E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 64 and contact element type 63 has been set up.  The       
 companion pair has real constant set ID 63.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11099E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37840E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32389E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64777E-01
 Average contact pair depth                   0.37840E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94600E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 84806 and target element 84524.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 69 and contact element type 69 has been set up.  The       
 companion pair has real constant set ID 70.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11498E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21925E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43849E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 86462 and target element 86696.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814821E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 70 and contact element type 69 has been set up.  The       
 companion pair has real constant set ID 69.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11498E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36527E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31208E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62417E-01
 Average contact pair depth                   0.36527E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91317E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993352533E-05 was detected between contact  
 element 86654 and target element 86372.                                 
 You may move entire target surface by : x= 5.866560076E-19, y=          
 8.993352533E-05, z= 9.676707127E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 75 and contact element type 75 has been set up.  The       
 companion pair has real constant set ID 76.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11236E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17320E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43824E-01
 Average contact pair depth                   0.17320E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43300E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 88286 and target element 88507.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814826E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 76 and contact element type 75 has been set up.  The       
 companion pair has real constant set ID 75.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11236E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37380E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33959E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.67918E-01
 Average contact pair depth                   0.37380E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93449E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 88466 and target element 88196.                                 
 You may move entire target surface by : x= -5.903321888E-19, y=         
 8.993356416E-05, z= 4.787035643E-18,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 81 and contact element type 81 has been set up.  The       
 companion pair has real constant set ID 82.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15953E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19573E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.39146E-01
 Average contact pair depth                   0.15953E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39883E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 89953 and target element 90038.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814853E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 82 and contact element type 81 has been set up.  The       
 companion pair has real constant set ID 81.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11985E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35045E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25853E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51706E-01
 Average contact pair depth                   0.35045E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.87613E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 89974 and target element 89869.                                 
 You may move entire target surface by : x= -1.501698361E-19, y=         
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 85 and contact element type 85 has been set up.  The       
 companion pair has real constant set ID 86.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11467E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18599E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.23072E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.46145E-01
 Average contact pair depth                   0.18599E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.46498E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 90607 and target element 90823.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162817686E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 86 and contact element type 85 has been set up.  The       
 companion pair has real constant set ID 85.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11467E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36627E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31105E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62211E-01
 Average contact pair depth                   0.36627E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91568E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 90761 and target element 90523.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 87 and contact element type 87 has been set up.  The       
 companion pair has real constant set ID 88.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10768E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17417E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21912E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43825E-01
 Average contact pair depth                   0.17417E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43542E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 91192 and target element 91447.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.16281477E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 88 and contact element type 87 has been set up.  The       
 companion pair has real constant set ID 87.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10768E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.39004E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32393E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64786E-01
 Average contact pair depth                   0.39004E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.97511E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 91323 and target element 91012.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 89 and contact element type 89 has been set up.  The       
 companion pair has real constant set ID 90.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12184E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17402E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21942E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43883E-01
 Average contact pair depth                   0.17402E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43505E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 91799 and target element 92067.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818998E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 90 and contact element type 89 has been set up.  The       
 companion pair has real constant set ID 89.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12184E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34470E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28938E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57877E-01
 Average contact pair depth                   0.34470E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.86176E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 91931 and target element 91619.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 91 and contact element type 91 has been set up.  The       
 companion pair has real constant set ID 92.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11728E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17354E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17354E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43385E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 92432 and target element 92665.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= 4.162819053E-11,to reduce initial penetration.      
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 92 and contact element type 91 has been set up.  The       
 companion pair has real constant set ID 91.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11728E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35811E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62436E-01
 Average contact pair depth                   0.35811E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.89529E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 92541 and target element 92252.                                 
 You may move entire target surface by : x= -5.23630289E-18, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 95 and contact element type 95 has been set up.  The       
 companion pair has real constant set ID 96.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11602E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17373E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21942E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43883E-01
 Average contact pair depth                   0.17373E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43432E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 93647 and target element 93905.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818942E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 96 and contact element type 95 has been set up.  The       
 companion pair has real constant set ID 95.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11602E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36202E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.31218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.62436E-01
 Average contact pair depth                   0.36202E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90505E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 93781 and target element 93467.                                 
 You may move entire target surface by : x= -3.978804542E-18, y=         
 -8.993364942E-05, z= -7.133067212E-19,to reduce initial penetration.    
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 99 and contact element type 99 has been set up.  The       
 companion pair has real constant set ID 100.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11861E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17391E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21929E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43858E-01
 Average contact pair depth                   0.17391E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43479E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 94839 and target element 95074.                                 
 You may move entire target surface by : x= 1.122907136E-06, y=          
 8.558277778E-05, z= -4.162818982E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 100 and contact element type 99 has been set up.  The      
 companion pair has real constant set ID 99.  Both pairs should have     
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11861E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35409E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32383E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64767E-01
 Average contact pair depth                   0.35409E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88522E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993356416E-05 was detected between contact  
 element 95032 and target element 94748.                                 
 You may move entire target surface by : x= -1.007796978E-18, y=         
 8.993356416E-05, z= -2.804077897E-18,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 103 and contact element type 103 has been set up.  The     
 companion pair has real constant set ID 104.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11418E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17489E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17489E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43723E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 96056 and target element 96312.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814874E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 104 and contact element type 103 has been set up.  The     
 companion pair has real constant set ID 103.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11418E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36783E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.32383E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.64767E-01
 Average contact pair depth                   0.36783E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91957E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 96188 and target element 95876.                                 
 You may move entire target surface by : x= -1.501698361E-19, y=         
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.562   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 107 and contact element type 107 has been set up.  The     
 companion pair has real constant set ID 108.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11253E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17436E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.43812E-01
 Average contact pair depth                   0.17436E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43590E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.559014413E-05 was detected between contact  
 element 97272 and target element 97539.                                 
 You may move entire target surface by : x= -1.122907136E-06, y=         
 8.558277778E-05, z= -4.162814891E-11,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 108 and contact element type 107 has been set up.  The     
 companion pair has real constant set ID 107.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11253E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37322E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.29035E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.58070E-01
 Average contact pair depth                   0.37322E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93306E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.993364942E-05 was detected between contact  
 element 97403 and target element 97092.                                 
 You may move entire target surface by : x= -1.50169836E-19, y=          
 -8.993364942E-05, z= 1.889932157E-17,to reduce initial penetration.     
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 111 and contact element type 111 has been set up.  The     
 companion pair has real constant set ID 112.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11928E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.27156E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.15502E-01
 Average contact pair depth                   0.27156E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.67891E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 97991 and target element 98027.                                 
  
 Max.  Geometric gap 5.516840776E-04 has been detected between contact   
 element 98000 and target element 98027.                                 
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 112 and contact element type 111 has been set up.  The     
 companion pair has real constant set ID 111.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11928E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35212E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.11737    
 Average contact pair depth                   0.35212E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88030E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Min.  Initial gap 5.728620916E-03 was detected between contact element  
 98021 and target element 97982.                                         
 The gap is closed due to initial settings.                              
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 113 and contact element type 113 has been set up.  The     
 companion pair has real constant set ID 114.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10034E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.67178E-03
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.22342E-01
 Average contact pair depth                   0.67178E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.16795E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 98198 and target element 98333.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 98308 and target element 98333.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 114 and contact element type 113 has been set up.  The     
 companion pair has real constant set ID 113.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10034E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.39866E-02
 Default opening contact stiffness OPSF will be used.
 Frictionless contact pair is defined
 Update contact stiffness at each iteration
 Average contact surface length               0.12931    
 Average contact pair depth                   0.39866E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.99664E-02
 Initial penetration/gap is excluded.
 No-separation contact (always)               is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.1072301E-03 was detected between contact    
 element 98317 and target element 98156.                                 
 You may move entire target surface by : x= 1.574184064E-19, y=          
 -8.1072301E-03, z= 3.816341428E-08,to reduce initial penetration.       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 119 and contact element type 119 has been set up.  The     
 companion pair has real constant set ID 120.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13779E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.29029E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.76545E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15309E-01
 Average contact pair depth                   0.29029E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.72573E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.33226763E-15 was detected between contact   
 element 98724 and target element 98765.                                 
  
 Max.  Geometric gap 5.516841203E-04 has been detected between contact   
 element 98733 and target element 98771.                                 
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 120 and contact element type 119 has been set up.  The     
 companion pair has real constant set ID 119.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13779E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.29450E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.49083E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.98167E-01
 Average contact pair depth                   0.29450E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.73625E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 121 and contact element type 121 has been set up.  The     
 companion pair has real constant set ID 122.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10383E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.74241E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12342E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24683E-01
 Average contact pair depth                   0.74241E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18560E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 98905 and target element 99032.                                 
  
 Max.  Geometric gap 2.E-03 has been detected between contact element    
 99001 and target element 99044.                                         
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 122 and contact element type 121 has been set up.  The     
 companion pair has real constant set ID 121.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10383E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38524E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.58789E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11758    
 Average contact pair depth                   0.38524E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96309E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.1071713E-03 was detected between contact    
 element 99006 and target element 98785.                                 
 You may move entire target surface by : x= 1.33033867E-18, y=           
 -8.1071713E-03, z= -3.816313684E-08,to reduce initial penetration.      
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 129 and contact element type 129 has been set up.  The     
 companion pair has real constant set ID 130.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10944E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36549E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51906E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10381    
 Average contact pair depth                   0.36549E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.91374E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Min.  Initial gap 9.804903E-03 was detected between contact element     
 100659 and target element 100773.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The detected gap is larger than the pair based pinball.      
 Please verify the pinball radius carefully.                             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 130 and contact element type 129 has been set up.  The     
 companion pair has real constant set ID 129.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10944E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37608E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.33403E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.66806E-01
 Average contact pair depth                   0.37608E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.94021E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Min.  Initial gap 9.804903E-03 was detected between contact element     
 100714 and target element 100630.                                       
 The gap is closed due to initial settings.                              
 *WARNING*: The detected gap is larger than the pair based pinball.      
 Please verify the pinball radius carefully.                             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 *WARNING*: The initial penetration/gap is relatively large.  Bonded/no  
 separation option may cause an accuracy issue.  Switch to MPC           
 algorithm or you may use the CNCHECK,ADJUST/MORPH command to move the   
 contact nodes towards the target surface.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 133 and contact element type 133 has been set up.  The     
 companion pair has real constant set ID 134.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36272E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11579E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22340E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.44679E-01
 Average contact pair depth                   0.11579    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.28948E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 101370 and target element 101396.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 134 and contact element type 133 has been set up.  The     
 companion pair has real constant set ID 133.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.36272E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15437E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25220E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50439E-01
 Average contact pair depth                   0.15437E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38593E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 101384 
 and target element 101359.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 135 and contact element type 135 has been set up.  The     
 companion pair has real constant set ID 136.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28622E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14674E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.22943E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.45887E-01
 Average contact pair depth                   0.14674    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36686E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 101411 and target element 101450.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 136 and contact element type 135 has been set up.  The     
 companion pair has real constant set ID 135.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28622E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15444E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25328E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50656E-01
 Average contact pair depth                   0.15444E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38610E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 101432 
 and target element 101406.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 137 and contact element type 137 has been set up.  The     
 companion pair has real constant set ID 138.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.52769E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.79592E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13265E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.26531    
 Average contact pair depth                   0.79592E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19898E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 4.E-03 was detected between contact element   
 101465 and target element 101553.                                       
 You may move entire target surface by : x= 1.088634287E-17, y=          
 1.657933389E-17, z= 4.E-03,to reduce initial penetration.               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 138 and contact element type 137 has been set up.  The     
 companion pair has real constant set ID 137.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.52769E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14771E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14040E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28079E-01
 Average contact pair depth                   0.14771E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36928E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 101476 and target element 101452.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 139 and contact element type 139 has been set up.  The     
 companion pair has real constant set ID 140.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.70574E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.59512E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.99186E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.19837    
 Average contact pair depth                   0.59512E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.14878E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 140 and contact element type 139 has been set up.  The     
 companion pair has real constant set ID 139.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.70574E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.58176E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.16959E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.33917E-01
 Average contact pair depth                   0.58176E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.14544E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 101574 and target element 101563.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 141 and contact element type 141 has been set up.  The     
 companion pair has real constant set ID 142.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.53293E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.88822E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17764    
 Average contact pair depth                   0.53293E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13323E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 142 and contact element type 141 has been set up.  The     
 companion pair has real constant set ID 141.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60242E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69719E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24773E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49547E-01
 Average contact pair depth                   0.69719E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17430E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 101601 and target element 101595.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 145 and contact element type 145 has been set up.  The     
 companion pair has real constant set ID 146.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11815E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35547E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.59245E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.11849    
 Average contact pair depth                   0.35547E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88868E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.E-03 was detected between contact element   
 102180 and target element 102519.                                       
 You may move entire target surface by : x= -1.329399072E-17, y=         
 -8.E-03, z= -2.223577107E-19,to reduce initial penetration.             
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 146 and contact element type 145 has been set up.  The     
 companion pair has real constant set ID 145.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11815E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17456E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27904E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.55809E-01
 Average contact pair depth                   0.17456E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.43640E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 102207 and target element 102074.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 147 and contact element type 147 has been set up.  The     
 companion pair has real constant set ID 148.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79862E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.49517E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.26832E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.53665E-02
 Average contact pair depth                   0.49517E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12379E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 5.551115123E-17 was detected between contact  
 element 102577 and target element 102592.                               
  
 Max.  Geometric gap 2.02697948E-03 has been detected between contact    
 element 102570 and target element 102588.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 148 and contact element type 147 has been set up.  The     
 companion pair has real constant set ID 147.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79862E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.52591E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.87651E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17530    
 Average contact pair depth                   0.52591E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13148E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 157 and contact element type 157 has been set up.  The     
 companion pair has real constant set ID 158.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11284E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12806E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.15224E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.30447E-01
 Average contact pair depth                   0.12806E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.32016E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 105284 and target element 105397.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 158 and contact element type 157 has been set up.  The     
 companion pair has real constant set ID 157.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11284E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37220E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.87203E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17441E-01
 Average contact pair depth                   0.37220E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.93050E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.33226763E-15 was detected between contact   
 element 105344 and target element 105255.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 159 and contact element type 159 has been set up.  The     
 companion pair has real constant set ID 160.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15619E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25600E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51201E-01
 Average contact pair depth                   0.15619E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.39046E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 160 and contact element type 159 has been set up.  The     
 companion pair has real constant set ID 159.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13714E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11694E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23388E-01
 Average contact pair depth                   0.30625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.76563E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 105443 and target element 105427.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.578   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 161 and contact element type 161 has been set up.  The     
 companion pair has real constant set ID 162.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.27941E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15281E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24923E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49846E-01
 Average contact pair depth                   0.15281E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38202E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105522 and target element 105583.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 162 and contact element type 161 has been set up.  The     
 companion pair has real constant set ID 161.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.27941E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15032E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11186E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22372E-01
 Average contact pair depth                   0.15032    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37579E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 105557 and target element 105479.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 175 and contact element type 175 has been set up.  The     
 companion pair has real constant set ID 176.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11601E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.12702E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.15559E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.31117E-01
 Average contact pair depth                   0.12702E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.31755E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 106394 and target element 106434.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 176 and contact element type 175 has been set up.  The     
 companion pair has real constant set ID 175.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11601E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.36204E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10598E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.21196E-01
 Average contact pair depth                   0.36204E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.90510E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 106406 and target element 106345.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 179 and contact element type 179 has been set up.  The     
 companion pair has real constant set ID 180.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11309E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11714E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11764E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23528E-01
 Average contact pair depth                   0.11714E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29286E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106560 and target element 106598.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 180 and contact element type 179 has been set up.  The     
 companion pair has real constant set ID 179.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11309E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37138E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12111E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24221E-01
 Average contact pair depth                   0.37138E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.92845E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106575 and target element 106550.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 181 and contact element type 181 has been set up.  The     
 companion pair has real constant set ID 182.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41485E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15360E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25018E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50036E-01
 Average contact pair depth                   0.15360E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38400E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 106624 
 and target element 106643.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 182 and contact element type 181 has been set up.  The     
 companion pair has real constant set ID 181.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.41485E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10124E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24274E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48547E-01
 Average contact pair depth                   0.10124    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.25310E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106635 and target element 106613.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 183 and contact element type 183 has been set up.  The     
 companion pair has real constant set ID 184.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13872E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19315E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38631E-01
 Average contact pair depth                   0.13872E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.34681E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 106692 and target element 106737.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 184 and contact element type 183 has been set up.  The     
 companion pair has real constant set ID 183.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13669E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.27338E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 106724 and target element 106653.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 185 and contact element type 185 has been set up.  The     
 companion pair has real constant set ID 186.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.16182E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14318E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20889E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.41778E-01
 Average contact pair depth                   0.14318E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35796E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 3.330669074E-16 was detected between contact  
 element 106849 and target element 106900.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 186 and contact element type 185 has been set up.  The     
 companion pair has real constant set ID 185.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.16182E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.25955E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19382E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38764E-01
 Average contact pair depth                   0.25955E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.64888E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 106866 and target element 106783.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 187 and contact element type 187 has been set up.  The     
 companion pair has real constant set ID 188.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12193E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11651E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12118E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24236E-01
 Average contact pair depth                   0.11651E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29129E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106937 and target element 106960.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 188 and contact element type 187 has been set up.  The     
 companion pair has real constant set ID 187.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12193E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34447E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11642E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.23283E-01
 Average contact pair depth                   0.34447E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.86118E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 106949 and target element 106906.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 191 and contact element type 191 has been set up.  The     
 companion pair has real constant set ID 192.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14230E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.20299E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.40597E-01
 Average contact pair depth                   0.14230E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.35575E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 107051 and target element 107106.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 192 and contact element type 191 has been set up.  The     
 companion pair has real constant set ID 191.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21436E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19593E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.13669E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.27338E-01
 Average contact pair depth                   0.19593    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48983E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107095 and target element 107033.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 193 and contact element type 193 has been set up.  The     
 companion pair has real constant set ID 194.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18083E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14485E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.21413E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.42826E-01
 Average contact pair depth                   0.14485E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36213E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 107204 and target element 107272.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 194 and contact element type 193 has been set up.  The     
 companion pair has real constant set ID 193.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.18083E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23226E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.19103E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.38207E-01
 Average contact pair depth                   0.23226E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.58064E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 107244 and target element 107151.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 199 and contact element type 199 has been set up.  The     
 companion pair has real constant set ID 200.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79719E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15360E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25018E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50036E-01
 Average contact pair depth                   0.15360E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.38400E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 107666 
 and target element 107676.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 200 and contact element type 199 has been set up.  The     
 companion pair has real constant set ID 199.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.79719E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.52685E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.37798E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.75596E-01
 Average contact pair depth                   0.52685E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13171E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 107672 and target element 107650.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 203 and contact element type 203 has been set up.  The     
 companion pair has real constant set ID 204.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11875E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11813E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12077E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.24154E-01
 Average contact pair depth                   0.11813E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.29531E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 1.387778781E-17 was detected between contact  
 element 107937 and target element 108046.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 204 and contact element type 203 has been set up.  The     
 companion pair has real constant set ID 203.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11875E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35367E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.88277E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.17655E-01
 Average contact pair depth                   0.35367E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88418E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 107989 and target element 107901.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 207 and contact element type 207 has been set up.  The     
 companion pair has real constant set ID 208.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.81529E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.51515E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24285E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48571E-01
 Average contact pair depth                   0.51515E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12879E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 4.303286342E-04 was detected between contact  
 element 108183 and target element 108326.                               
 You may move entire target surface by : x= -2.320328472E-04, y=         
 -3.616434518E-04, z= -2.361154317E-05,to reduce initial penetration.    
  
 Max.  Geometric gap 9.E-03 has been detected between contact element    
 108156 and target element 108288.                                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 208 and contact element type 207 has been set up.  The     
 companion pair has real constant set ID 207.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.81529E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16450E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25670E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.51340E-01
 Average contact pair depth                   0.16450E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.41125E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 3.615199155E-04 was detected between contact  
 element 108267 and target element 108120.                               
 You may move entire target surface by : x= 2.227331075E-04, y=          
 2.847570598E-04, z= 1.702904744E-07,to reduce initial penetration.      
  
 Max.  Geometric gap 3.184938432E-03 has been detected between contact   
 element 108259 and target element 108144.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 209 and contact element type 209 has been set up.  The     
 companion pair has real constant set ID 210.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.66576E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.63085E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24828E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.49655E-01
 Average contact pair depth                   0.63085E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.15771E-01

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 One of the contact searching regions contains at least 55 target        
 elements.  You may reduce the pinball radius.                           
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 4.491127571E-04 was detected between contact  
 element 108425 and target element 108556.                               
 You may move entire target surface by : x= -2.208559608E-04, y=         
 3.907190955E-04, z= -1.623273335E-05,to reduce initial penetration.     
  
 Max.  Geometric gap 9.E-03 has been detected between contact element    
 108405 and target element 108542.                                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 210 and contact element type 209 has been set up.  The     
 companion pair has real constant set ID 209.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.66576E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16415E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25436E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50872E-01
 Average contact pair depth                   0.16415E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.41039E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 3.997438332E-04 was detected between contact  
 element 108494 and target element 108360.                               
 You may move entire target surface by : x= 2.462826662E-04, y=          
 -3.148649632E-04, z= 1.882939812E-07,to reduce initial penetration.     
  
 Max.  Geometric gap 3.176739077E-03 has been detected between contact   
 element 108509 and target element 108390.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 211 and contact element type 211 has been set up.  The     
 companion pair has real constant set ID 212.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.78817E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.37162E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.60085E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12017    
 Average contact pair depth                   0.37162E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.92905E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 108674 
 and target element 108971.                                              
  
 Max.  Geometric gap 7.349455406E-04 has been detected between contact   
 element 108700 and target element 108921.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.594   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 212 and contact element type 211 has been set up.  The     
 companion pair has real constant set ID 211.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.78817E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.53288E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14483E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28966E-01
 Average contact pair depth                   0.53288E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.13322E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 5.551115123E-17 was detected between contact  
 element 108746 and target element 108617.                               
  
 Max.  Geometric gap 9.748335779E-04 has been detected between contact   
 element 108872 and target element 108646.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 215 and contact element type 215 has been set up.  The     
 companion pair has real constant set ID 216.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.86566E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14428E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28855E-01
 Average contact pair depth                   0.86566E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.21641E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 216 and contact element type 215 has been set up.  The     
 companion pair has real constant set ID 215.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16331E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54436E-01
 Average contact pair depth                   0.16331E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.40827E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 219 and contact element type 219 has been set up.  The     
 companion pair has real constant set ID 220.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68228E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.61558E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10260E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.20519    
 Average contact pair depth                   0.61558E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.15390E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 109209 
 and target element 109407.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 220 and contact element type 219 has been set up.  The     
 companion pair has real constant set ID 219.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.68228E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.28146E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.46911E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.93821E-01
 Average contact pair depth                   0.28146E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.70366E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 5.E-03 was detected between contact element   
 109331 and target element 109172.                                       
 You may move entire target surface by : x= -2.010731742E-17, y=         
 2.902074441E-18, z= 5.E-03,to reduce initial penetration.               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 223 and contact element type 223 has been set up.  The     
 companion pair has real constant set ID 224.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55205E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.68625E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.24168E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.48335E-01
 Average contact pair depth                   0.68625E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17156E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 109495 and target element 109505.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 224 and contact element type 223 has been set up.  The     
 companion pair has real constant set ID 223.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55205E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.76080E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12680E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25360    
 Average contact pair depth                   0.76080E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19020E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 225 and contact element type 225 has been set up.  The     
 companion pair has real constant set ID 226.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.90930E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.46190E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.76983E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.15397    
 Average contact pair depth                   0.46190E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.11547E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Min.  Initial gap 3.550953997E-04 was detected between contact element  
 109515 and target element 109553.                                       
 The gap is closed due to initial settings.                              
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 226 and contact element type 225 has been set up.  The     
 companion pair has real constant set ID 225.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.90930E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.34008E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.65113E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13023E-01
 Average contact pair depth                   0.34008E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.85020E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 109524 and target element 109508.                               
  
 Max.  Geometric gap 8.36518718E-04 has been detected between contact    
 element 109525 and target element 109507.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 235 and contact element type 235 has been set up.  The     
 companion pair has real constant set ID 236.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.86566E-03
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.14428E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.28855E-01
 Average contact pair depth                   0.86566E-02
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.21641E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 236 and contact element type 235 has been set up.  The     
 companion pair has real constant set ID 235.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.25718E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.16331E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27218E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54436E-01
 Average contact pair depth                   0.16331E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.40827E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 237 and contact element type 237 has been set up.  The     
 companion pair has real constant set ID 238.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10291E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40813E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.68022E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13604    
 Average contact pair depth                   0.40813E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10203E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.E-03 was detected between contact element   
 110521 and target element 110818.                                       
 You may move entire target surface by : x= 2.240400286E-17, y= 8.E-03,  
 z= -2.473432853E-17,to reduce initial penetration.                      
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 238 and contact element type 237 has been set up.  The     
 companion pair has real constant set ID 237.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10291E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.19225E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28954E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.57908E-01
 Average contact pair depth                   0.19225E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.48061E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 110556 and target element 110413.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 239 and contact element type 239 has been set up.  The     
 companion pair has real constant set ID 240.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10456E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40167E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.66945E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13389    
 Average contact pair depth                   0.40167E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10042E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.E-03 was detected between contact element   
 110933 and target element 111240.                                       
 You may move entire target surface by : x= -1.486686244E-16, y= 8.E-03, 
 z= 2.628680716E-18,to reduce initial penetration.                       
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 240 and contact element type 239 has been set up.  The     
 companion pair has real constant set ID 239.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10456E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.17806E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.28393E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.56787E-01
 Average contact pair depth                   0.17806E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.44516E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 111078 and target element 110901.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 241 and contact element type 241 has been set up.  The     
 companion pair has real constant set ID 242.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness       5299.0    
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.13546E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.27145E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.54290E-01
 Average contact pair depth                   0.13546    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.33866E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 111501 and target element 111743.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 242 and contact element type 241 has been set up.  The     
 companion pair has real constant set ID 241.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness       5299.0    
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.79261E+09
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.10631E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.21263    
 Average contact pair depth                   0.79261E+10
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.19815E+10
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 111697 and target element 111366.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 243 and contact element type 243 has been set up.  The     
 companion pair has real constant set ID 244.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55389E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.75828E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.12638E-02
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.25276    
 Average contact pair depth                   0.75828E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18957E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 5.E-03 was detected between contact element   
 111840 and target element 113431.                                       
 You may move entire target surface by : x= 2.604679454E-18, y=          
 -2.290348148E-17, z= -5.E-03,to reduce initial penetration.             
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 244 and contact element type 243 has been set up.  The     
 companion pair has real constant set ID 243.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.55389E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.10604E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.17673E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.35346E-01
 Average contact pair depth                   0.10604E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.26510E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 112571 and target element 111824.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 247 and contact element type 247 has been set up.  The     
 companion pair has real constant set ID 248.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38012E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.63353E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12671    
 Average contact pair depth                   0.38012E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.95030E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 2.220446049E-16 was detected between contact  
 element 114393 and target element 114456.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 248 and contact element type 247 has been set up.  The     
 companion pair has real constant set ID 247.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69901E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48996E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97993E-01
 Average contact pair depth                   0.69901E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17475E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 114417 and target element 114246.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 251 and contact element type 251 has been set up.  The     
 companion pair has real constant set ID 252.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10347E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38920E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.54853E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10971E-01
 Average contact pair depth                   0.38920E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.97299E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 114581 and target element 114625.                               
  
 Max.  Geometric gap 1.70535368E-04 has been detected between contact    
 element 114588 and target element 114623.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 252 and contact element type 251 has been set up.  The     
 companion pair has real constant set ID 251.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.10347E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.40591E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48531E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97063E-01
 Average contact pair depth                   0.40591E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.10148E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 114618 
 and target element 114573.                                              
  
 Max.  Geometric gap 1.952835099E-05 has been detected between contact   
 element 114613 and target element 114556.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 253 and contact element type 253 has been set up.  The     
 companion pair has real constant set ID 254.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.38536E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.64226E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.12845    
 Average contact pair depth                   0.38536E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.96340E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 4.440892099E-16 was detected between contact  
 element 114736 and target element 114844.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 254 and contact element type 253 has been set up.  The     
 companion pair has real constant set ID 253.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.60085E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.69901E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.48996E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.97993E-01
 Average contact pair depth                   0.69901E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.17475E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 114820 and target element 114708.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 255 and contact element type 255 has been set up.  The     
 companion pair has real constant set ID 256.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37836E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.18170E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.30283E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.60566E-01
 Average contact pair depth                   0.18170E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.45424E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 0 was detected between contact element 114868 
 and target element 114934.                                              
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 256 and contact element type 255 has been set up.  The     
 companion pair has real constant set ID 255.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.37836E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.11100E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.41877E-04
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.83754E-02
 Average contact pair depth                   0.11100    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.27751E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 114899 and target element 114860.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 257 and contact element type 257 has been set up.  The     
 companion pair has real constant set ID 258.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12801E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.23447E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.39078E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.78156E-01
 Average contact pair depth                   0.23447E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.58617E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 115135 and target element 115304.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 258 and contact element type 257 has been set up.  The     
 companion pair has real constant set ID 257.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.12801E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.32811E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.54684E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10937    
 Average contact pair depth                   0.32811E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.82027E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 7.6E-03 was detected between contact element  
 115193 and target element 114986.                                       
 You may move entire target surface by : x= 7.6E-03, y=                  
 -6.453458065E-17, z= -3.543835954E-17,to reduce initial penetration.    
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 263 and contact element type 263 has been set up.  The     
 companion pair has real constant set ID 264.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28794E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.15000E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.11183E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.22366E-01
 Average contact pair depth                   0.15000E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.37499E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.609   TIME= 11:41:22
 Max.  Initial penetration 2.775557562E-17 was detected between contact  
 element 115916 and target element 115963.                               
  
 Max.  Geometric gap 2.253430249E-03 has been detected between contact   
 element 115949 and target element 115962.                               
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 264 and contact element type 263 has been set up.  The     
 companion pair has real constant set ID 263.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.28794E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.14586E-01
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.66411E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.13282    
 Average contact pair depth                   0.14586    
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.36466E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Max.  Initial penetration 1.776356839E-15 was detected between contact  
 element 115955 and target element 115861.                               
  
 Max.  Geometric gap 2.159995441E-03 has been detected between contact   
 element 115956 and target element 115903.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 265 and contact element type 265 has been set up.  The     
 companion pair has real constant set ID 266.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11833E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.35494E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.30208E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.60417E-01
 Average contact pair depth                   0.35494E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.88735E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 266 and contact element type 265 has been set up.  The     
 companion pair has real constant set ID 265.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.11833E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.31171E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51952E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10390    
 Average contact pair depth                   0.31171E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77927E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 269 and contact element type 269 has been set up.  The     
 companion pair has real constant set ID 270.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.57934E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.72496E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.29722E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.59444E-01
 Average contact pair depth                   0.72496E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.18124E-01
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Max.  Initial penetration 1.110223025E-16 was detected between contact  
 element 116011 and target element 116052.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 270 and contact element type 269 has been set up.  The     
 companion pair has real constant set ID 269.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.57934E+15
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30564E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.50598E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10120    
 Average contact pair depth                   0.30564E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.76410E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Min.  Initial gap 2.910475675E-03 was detected between contact element  
 116029 and target element 115999.                                       
 The gap is closed due to initial settings.                              
  
 Max.  Geometric gap 3.652822432E-03 has been detected between contact   
 element 116036 and target element 115995.                               
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 271 and contact element type 271 has been set up.  The     
 companion pair has real constant set ID 272.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will deactivate the current pair and keep its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.30851E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.51418E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.10284    
 Average contact pair depth                   0.30851E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.77126E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 No contact was detected for this contact pair.                          
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Symmetric Deformable- deformable contact pair identified by real        
 constant set 272 and contact element type 271 has been set up.  The     
 companion pair has real constant set ID 271.  Both pairs should have    
 the same behavior.                                                      
 ANSYS will keep the current pair and deactivate its companion pair,     
 resulting in asymmetric contact.                                        
 Contact algorithm: Augmented Lagrange method
 Contact detection at: Gauss integration point
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.13614E+16
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.25656E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.42456E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.84913E-01
 Average contact pair depth                   0.25656E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.64140E-02
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Max.  Initial penetration 8.881784197E-16 was detected between contact  
 element 116091 and target element 116072.                               
  
 Max.  Geometric gap 7.627606316E-03 has been detected between contact   
 element 116101 and target element 116075.                               
 *WARNING*: The geometric gap/penetration is larger than the pair based  
 pinball.  Please verify the pinball radius carefully.                   
 *WARNING*: The geometric gap/penetration may be too large.  Increase    
 pinball radius if it is a true geometric gap/penetration.  Decrease     
 pinball if it is a false one.                                           
 ****************************************
  

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Deformable-deformable contact pair identified by real constant set 275  
 and contact element type 275 has been set up.                           
 Node-surface contact pair is defined
 Contact force based contact model
 Contact algorithm: Augmented Lagrange method
 Contact detection at: nodal point (normal to target surface)
 *WARNING*: Smoothing on certain contact/target nodes (for example       
 160291) may have an accuracy issue.  You may switch contact and target  
 surfaces, or split the current pair into multiple pairs, or use Gauss   
 detection.                                                              
 Contact stiffness factor FKN                  10.000    
 The resulting initial contact stiffness      0.21404E+14
 Default penetration tolerance factor FTOLN   0.10000    
 The resulting penetration tolerance          0.50962E-02
 Default opening contact stiffness OPSF will be used.
 Default tangent stiffness factor FKT          1.0000    
 Default elastic slip factor SLTOL            0.50000E-02
 The resulting elastic slip                   0.25481E-03
 Update contact stiffness at each iteration
 Default Max. friction stress TAUMAX          0.10000E+21
 Average contact surface length               0.50962E-01
 Average contact pair depth                   0.50962E-01
 Default pinball region factor PINB           0.25000    
 The resulting pinball region                 0.12740E-01
 Default target edge extension factor TOLS     10.000    
 Initial penetration/gap is excluded.
 Bonded contact (always) is defined.

 *** NOTE ***                            CP =      15.625   TIME= 11:41:22
 Max.  Initial penetration 9.795602115E-17 was detected between contact  
 element 116296 and target element 116544.                               
 ****************************************
  

  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          57
 Max.  Penetration of -3.013353734E-16 has been detected between contact 
 element 82705 and target element 83010.                                 
  
 Max.  Geometrical gap of 3.935432276E-05 has been detected between      
 contact element 82789 and target element 83023.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 82789 and target element 83023.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.354229455E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -0.535335247.                                      
 Max.  Normal stiffness 1.116352961E+15.                                 
 Min.  Normal stiffness 1.116352961E+15.                                 
 Max.  Tangential stiffness 3.327482846E+14.                             
 Min.  Tangential stiffness 3.327482846E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          58

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          59
 Max.  Penetration of -4.990248657E-16 has been detected between contact 
 element 83313 and target element 83664.                                 
  
 Max.  Geometrical gap of 3.935421831E-05 has been detected between      
 contact element 83396 and target element 83660.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 83396 and target element 83660.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.305808202E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force 0.550705955.                                       
 Max.  Normal stiffness 1.103564157E+15.                                 
 Min.  Normal stiffness 1.103564157E+15.                                 
 Max.  Tangential stiffness 3.251865418E+14.                             
 Min.  Tangential stiffness 3.251865418E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          60

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          63
 Max.  Penetration of -4.440892099E-16 has been detected between contact 
 element 84531 and target element 84876.                                 
  
 Max.  Geometrical gap of 3.935401147E-05 has been detected between      
 contact element 84613 and target element 84848.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 84613 and target element 84848.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.358979173E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -0.6689248.                                        
 Max.  Normal stiffness 1.109934079E+15.                                 
 Min.  Normal stiffness 1.109934079E+15.                                 
 Max.  Tangential stiffness 3.313834625E+14.                             
 Min.  Tangential stiffness 3.313834625E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          64

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          69
 Max.  Penetration of -8.890221292E-16 has been detected between contact 
 element 86463 and target element 86763.                                 
  
 Max.  Geometrical gap of 3.935432276E-05 has been detected between      
 contact element 86462 and target element 86696.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 86462 and target element 86696.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.354230608E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force 1.02223216.                                        
 Max.  Normal stiffness 1.14983882E+15.                                  
 Min.  Normal stiffness 1.14983882E+15.                                  
 Max.  Tangential stiffness 3.425372789E+14.                             
 Min.  Tangential stiffness 3.425372789E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          70

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          75
 Max.  Penetration of -8.882548662E-16 has been detected between contact 
 element 88286 and target element 88506.                                 
  
 Max.  Geometrical gap of 3.935432276E-05 has been detected between      
 contact element 88286 and target element 88507.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 88286 and target element 88507.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.330033244E-03.                                 
 One of the contact searching regions contains at least 40 target        
 elements.                                                               
 Max.  Pressure/force -1.13690994.                                       
 Max.  Normal stiffness 1.123603612E+15.                                 
 Min.  Normal stiffness 1.123603612E+15.                                 
 Max.  Tangential stiffness 3.330538025E+14.                             
 Min.  Tangential stiffness 3.330538025E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          76

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          81
 Max.  Penetration of -1.778044145E-15 has been detected between contact 
 element 89874 and target element 90046.                                 
  
 Max.  Geometrical gap of 3.935418995E-05 has been detected between      
 contact element 89953 and target element 90038.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 89953 and target element 90038.                 
 For total 84 contact elements, there are 84 elements are in contact.    
 There are 84 elements are in sticking.                                  
 Contacting area 4.019344632E-03.                                        
 Max.  Pinball distance 3.988273546E-03.                                 
 One of the contact searching regions contains at least 34 target        
 elements.                                                               
 Max.  Pressure/force 2.13090033.                                        
 Max.  Normal stiffness 1.198451867E+15.                                 
 Min.  Normal stiffness 1.198451867E+15.                                 
 Max.  Tangential stiffness 3.663044286E+14.                             
 Min.  Tangential stiffness 3.663044286E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          82

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          85
 Max.  Penetration of -8.990842126E-16 has been detected between contact 
 element 90682 and target element 90924.                                 
  
 Max.  Geometrical gap of 3.935401147E-05 has been detected between      
 contact element 90607 and target element 90823.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 90607 and target element 90823.                 
 For total 156 contact elements, there are 156 elements are in contact.  
 There are 156 elements are in sticking.                                 
 Contacting area 8.798689266E-03.                                        
 Max.  Pinball distance 4.649784252E-03.                                 
 One of the contact searching regions contains at least 40 target        
 elements.                                                               
 Max.  Pressure/force -1.38214869.                                       
 Max.  Normal stiffness 1.146686395E+15.                                 
 Min.  Normal stiffness 1.146686395E+15.                                 
 Max.  Tangential stiffness 3.466374155E+14.                             
 Min.  Tangential stiffness 3.466374155E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          86

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          87
 Max.  Penetration of -1.332382157E-15 has been detected between contact 
 element 91112 and target element 91454.                                 
  
 Max.  Geometrical gap of 3.935418995E-05 has been detected between      
 contact element 91192 and target element 91447.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 91192 and target element 91447.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.354229281E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force 1.43471373.                                        
 Max.  Normal stiffness 1.076803471E+15.                                 
 Min.  Normal stiffness 1.076803471E+15.                                 
 Max.  Tangential stiffness 3.209598682E+14.                             
 Min.  Tangential stiffness 3.209598682E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          88

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          89
 Max.  Penetration of -1.011844967E-15 has been detected between contact 
 element 91796 and target element 92132.                                 
  
 Max.  Geometrical gap of 3.935418995E-05 has been detected between      
 contact element 91799 and target element 92067.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 91799 and target element 92067.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.350547637E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -1.46862983.                                       
 Max.  Normal stiffness 1.21844262E+15.                                  
 Min.  Normal stiffness 1.21844262E+15.                                  
 Max.  Tangential stiffness 3.623853204E+14.                             
 Min.  Tangential stiffness 3.623853204E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          90

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          91
 Max.  Penetration of -1.332382302E-15 has been detected between contact 
 element 92432 and target element 92665.                                 
  
 Max.  Geometrical gap of 3.935432276E-05 has been detected between      
 contact element 92432 and target element 92665.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 92432 and target element 92665.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.338524696E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -2.37340012.                                       
 Max.  Normal stiffness 1.172808009E+15.                                 
 Min.  Normal stiffness 1.172808009E+15.                                 
 Max.  Tangential stiffness 3.484153917E+14.                             
 Min.  Tangential stiffness 3.484153917E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          92

 *** NOTE ***                            CP =      23.578   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          95
 Max.  Penetration of -8.990842358E-16 has been detected between contact 
 element 93566 and target element 93913.                                 
  
 Max.  Geometrical gap of 3.935401974E-05 has been detected between      
 contact element 93647 and target element 93905.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 93647 and target element 93905.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.343229469E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -2.79676361.                                       
 Max.  Normal stiffness 1.160154042E+15.                                 
 Min.  Normal stiffness 1.160154042E+15.                                 
 Max.  Tangential stiffness 3.4446859E+14.                               
 Min.  Tangential stiffness 3.4446859E+14.                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          96

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET          99
 Max.  Penetration of -1.798168472E-15 has been detected between contact 
 element 94758 and target element 95070.                                 
  
 Max.  Geometrical gap of 3.93540855E-05 has been detected between       
 contact element 94839 and target element 95074.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 94839 and target element 95074.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.34786923E-03.                                  
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -2.40038966.                                       
 Max.  Normal stiffness 1.186147824E+15.                                 
 Min.  Normal stiffness 1.186147824E+15.                                 
 Max.  Tangential stiffness 3.527639968E+14.                             
 Min.  Tangential stiffness 3.527639968E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         100

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         103
 Max.  Penetration of -1.01184512E-15 has been detected between contact  
 element 96052 and target element 96364.                                 
  
 Max.  Geometrical gap of 3.935418995E-05 has been detected between      
 contact element 96056 and target element 96312.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 96056 and target element 96312.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.372335697E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force -1.37629083.                                       
 Max.  Normal stiffness 1.141833958E+15.                                 
 Min.  Normal stiffness 1.141833958E+15.                                 
 Max.  Tangential stiffness 3.418589883E+14.                             
 Min.  Tangential stiffness 3.418589883E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         104

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         107
 Max.  Penetration of -1.01184512E-15 has been detected between contact  
 element 97268 and target element 97604.                                 
  
 Max.  Geometrical gap of 3.935418995E-05 has been detected between      
 contact element 97272 and target element 97539.                         
  
 Max.  Geometrical penetration of -8.559014413E-05 has been detected     
 between contact element 97272 and target element 97539.                 
 For total 180 contact elements, there are 180 elements are in contact.  
 There are 180 elements are in sticking.                                 
 Contacting area 9.558689266E-03.                                        
 Max.  Pinball distance 4.358977824E-03.                                 
 One of the contact searching regions contains at least 44 target        
 elements.                                                               
 Max.  Pressure/force 1.13866041.                                        
 Max.  Normal stiffness 1.125330727E+15.                                 
 Min.  Normal stiffness 1.125330727E+15.                                 
 Max.  Tangential stiffness 3.35886982E+14.                              
 Min.  Tangential stiffness 3.35886982E+14.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         108

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         111
 Max.  Penetration of 0 has been detected between contact element 97991  
 and target element 98027.                                               
  
 Max.  Geometrical gap of 6.457667724E-03 has been detected between      
 contact element 98010 and target element 98026.                         
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -4.440892099E-16 has been detected     
 between contact element 98010 and target element 98026.                 
 For total 28 contact elements, there are 20 elements are in contact.    
 Contacting area 3.341035265E-04.                                        
 Max.  Pinball distance 6.789072301E-03.                                 
 One of the contact searching regions contains at least 4 target         
 elements.                                                               
 Max.  Pressure/force -0.664685253.                                      
 Max.  Normal stiffness 1.192780887E+15.                                 
 Min.  Normal stiffness 1.192780887E+15.                                 
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         112

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         113
 Max.  Penetration of 0 has been detected between contact element 98182  
 and target element 98333.                                               
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 98182 and target element 98333.                         
  
 Max.  Geometrical penetration of -2.220446049E-16 has been detected     
 between contact element 98182 and target element 98333.                 
 For total 140 contact elements, there are 86 elements are in contact.   
 Contacting area 1.182822331E-02.                                        
 Max.  Pinball distance 1.679450636E-03.                                 
 One of the contact searching regions contains at least 10 target        
 elements.                                                               
 Max.  Pressure/force 1.991083063E-02.                                   
 Max.  Normal stiffness 1.003373722E+15.                                 
 Min.  Normal stiffness 1.003373722E+15.                                 
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         114

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         119
 Max.  Penetration of -5.896368893E-16 has been detected between contact 
 element 98729 and target element 98770.                                 
  
 Max.  Geometrical gap of 6.457666592E-03 has been detected between      
 contact element 98732 and target element 98770.                         
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -1.33226763E-15 has been detected      
 between contact element 98732 and target element 98770.                 
 For total 28 contact elements, there are 20 elements are in contact.    
 There are 20 elements are in sticking.                                  
 Contacting area 3.341035264E-04.                                        
 Max.  Pinball distance 7.257339268E-03.                                 
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force -1.21870328.                                       
 Max.  Normal stiffness 1.377915463E+15.                                 
 Min.  Normal stiffness 1.377915463E+15.                                 
 Max.  Tangential stiffness 1.959625543E+15.                             
 Min.  Tangential stiffness 1.959625543E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         120

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         121
 Max.  Penetration of 0 has been detected between contact element 98902  
 and target element 99036.                                               
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 98923 and target element 99032.                         
  
 Max.  Geometrical penetration of -2.220446049E-16 has been detected     
 between contact element 98923 and target element 99032.                 
 For total 116 contact elements, there are 62 elements are in contact.   
 There are 62 elements are in sticking.                                  
 Contacting area 1.182822332E-02.                                        
 Max.  Pinball distance 1.856017786E-03.                                 
 One of the contact searching regions contains at least 11 target        
 elements.                                                               
 Max.  Pressure/force 2.276338908E-02.                                   
 Max.  Normal stiffness 1.03832316E+15.                                  
 Min.  Normal stiffness 1.03832316E+15.                                  
 Max.  Tangential stiffness 2.342242008E+14.                             
 Min.  Tangential stiffness 2.342242008E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         122

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         129

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         130

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 No contact was detected.                                                
 Max.  Pinball distance 9.402064911E-03.                                 
 One of the contact searching regions contains at least 13 target        
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         133
 Max.  Penetration of 0 has been detected between contact element 101363 
 and target element 101402.                                              
  
 Max.  Geometrical gap of 1.776356839E-15 has been detected between      
 contact element 101364 and target element 101398.                       
  
 Max.  Geometrical penetration of -1.776356839E-15 has been detected     
 between contact element 101364 and target element 101398.               
 For total 8 contact elements, there are 8 elements are in contact.      
 There are 8 elements are in sticking.                                   
 Contacting area 6.84E-04.                                               
 Max.  Pinball distance 2.894783497E-02.                                 
 One of the contact searching regions contains at least 16 target        
 elements.                                                               
 Max.  Pressure/force 1.439395128E-02.                                   
 Max.  Normal stiffness 3.627214267E+14.                                 
 Min.  Normal stiffness 3.627214267E+14.                                 
 Max.  Tangential stiffness 7.050240842E+14.                             
 Min.  Tangential stiffness 7.050240842E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         134

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         135
 Max.  Penetration of 0 has been detected between contact element 101411 
 and target element 101448.                                              
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 101412 and target element 101447.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 101412 and target element 101447.               
 For total 8 contact elements, there are 8 elements are in contact.      
 There are 8 elements are in sticking.                                   
 Contacting area 6.84E-04.                                               
 Max.  Pinball distance 3.668552925E-02.                                 
 One of the contact searching regions contains at least 16 target        
 elements.                                                               
 Max.  Pressure/force 1.166498126E-02.                                   
 Max.  Normal stiffness 2.862163969E+14.                                 
 Min.  Normal stiffness 2.862163969E+14.                                 
 Max.  Tangential stiffness 6.864694831E+14.                             
 Min.  Tangential stiffness 6.864694831E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         136

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         137

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         138
 Max.  Penetration of 0 has been detected between contact element 101467 
 and target element 101452.                                              
  
 Max.  Geometrical gap of 4.440892099E-16 has been detected between      
 contact element 101476 and target element 101452.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 101476 and target element 101452.               
 For total 48 contact elements, there are 32 elements are in contact.    
 There are 32 elements are in sticking.                                  
 Contacting area 1.372E-02.                                              
 Max.  Pinball distance 3.692763474E-03.                                 
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 Max.  Pressure/force 1.316020191E-02.                                   
 Max.  Normal stiffness 5.276905037E+14.                                 
 Min.  Normal stiffness 5.276905037E+14.                                 
 Max.  Tangential stiffness 2.081943638E+14.                             
 Min.  Tangential stiffness 2.081943638E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         139

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         140
 Max.  Penetration of 0 has been detected between contact element 101569 
 and target element 101563.                                              
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 101569 and target element 101563.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 101569 and target element 101563.               
 For total 12 contact elements, there are 12 elements are in contact.    
 There are 12 elements are in sticking.                                  
 Contacting area 7.740000015E-04.                                        
 Max.  Pinball distance 1.454401493E-02.                                 
 One of the contact searching regions contains at least 3 target         
 elements.                                                               
 Max.  Pressure/force 2.126025503E-02.                                   
 Max.  Normal stiffness 7.057422967E+14.                                 
 Min.  Normal stiffness 7.057422967E+14.                                 
 Max.  Tangential stiffness 9.078824189E+14.                             
 Min.  Tangential stiffness 9.078824189E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         141

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         142
 Max.  Penetration of 0 has been detected between contact element 101599 
 and target element 101595.                                              
  
 Max.  Geometrical gap of 1.110223025E-16 has been detected between      
 contact element 101601 and target element 101595.                       
  
 Max.  Geometrical penetration of -2.220446049E-16 has been detected     
 between contact element 101601 and target element 101595.               
 For total 8 contact elements, there are 8 elements are in contact.      
 There are 8 elements are in sticking.                                   
 Contacting area 9.8E-04.                                                
 Max.  Pinball distance 1.742968684E-02.                                 
 One of the contact searching regions contains at least 3 target         
 elements.                                                               
 Max.  Pressure/force 2.651024389E-02.                                   
 Max.  Normal stiffness 6.02420462E+14.                                  
 Min.  Normal stiffness 6.02420462E+14.                                  
 Max.  Tangential stiffness 6.357652147E+14.                             
 Min.  Tangential stiffness 6.357652147E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         145

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         146
 Max.  Penetration of 0 has been detected between contact element 102203 
 and target element 102076.                                              
  
 Max.  Geometrical gap of 4.440892099E-16 has been detected between      
 contact element 102207 and target element 102074.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 102207 and target element 102074.               
 For total 174 contact elements, there are 92 elements are in contact.   
 There are 92 elements are in sticking.                                  
 Contacting area 5.11151706E-02.                                         
 Max.  Pinball distance 4.364036245E-03.                                 
 One of the contact searching regions contains at least 22 target        
 elements.                                                               
 Max.  Pressure/force 5.856624749E-02.                                   
 Max.  Normal stiffness 1.181528329E+15.                                 
 Min.  Normal stiffness 1.181528329E+15.                                 
 Max.  Tangential stiffness 2.77172858E+14.                              
 Min.  Tangential stiffness 2.77172858E+14.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         147
 Max.  Penetration of 0 has been detected between contact element 102567 
 and target element 102588.                                              
  
 Max.  Geometrical gap of 2.02697948E-03 has been detected between       
 contact element 102570 and target element 102588.                       
  
 Max.  Geometrical penetration of -5.551115123E-17 has been detected     
 between contact element 102570 and target element 102588.               
 For total 16 contact elements, there are 16 elements are in contact.    
 There are 16 elements are in sticking.                                  
 Contacting area 1.000000018E-04.                                        
 Max.  Pinball distance 1.237937164E-02.                                 
 One of the contact searching regions contains at least 3 target         
 elements.                                                               
 Max.  Pressure/force -2.216624211E-02.                                  
 Max.  Normal stiffness 7.986230376E+14.                                 
 Min.  Normal stiffness 7.986230376E+14.                                 
 Max.  Tangential stiffness 5.526761068E+15.                             
 Min.  Tangential stiffness 5.526761068E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         148

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         157

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         158
 Max.  Penetration of 0 has been detected between contact element 105323 
 and target element 105259.                                              
  
 Max.  Geometrical gap of 8.881784197E-16 has been detected between      
 contact element 105344 and target element 105255.                       
  
 Max.  Geometrical penetration of -1.33226763E-15 has been detected      
 between contact element 105344 and target element 105255.               
 For total 47 contact elements, there are 41 elements are in contact.    
 There are 41 elements are in sticking.                                  
 Contacting area 2.585342326E-03.                                        
 Max.  Pinball distance 9.304975223E-03.                                 
 One of the contact searching regions contains at least 11 target        
 elements.                                                               
 Max.  Pressure/force 1.747986065E-02.                                   
 Max.  Normal stiffness 1.128428582E+15.                                 
 Min.  Normal stiffness 1.128428582E+15.                                 
 Max.  Tangential stiffness 1.806121167E+15.                             
 Min.  Tangential stiffness 1.806121167E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         159

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         160
 Max.  Penetration of 0 has been detected between contact element 105443 
 and target element 105427.                                              
  
 Max.  Geometrical penetration of -1.776356839E-15 has been detected     
 between contact element 105443 and target element 105427.               
 For total 2 contact elements, there are 2 elements are in contact.      
 There are 2 elements are in sticking.                                   
 Contacting area 5.4E-05.                                                
 Max.  Pinball distance 7.65625E-03.                                     
 One of the contact searching regions contains at least 13 target        
 elements.                                                               
 Max.  Pressure/force 2.848833535E-02.                                   
 Max.  Normal stiffness 1.371428571E+15.                                 
 Min.  Normal stiffness 1.371428571E+15.                                 
 Max.  Tangential stiffness 1.346842743E+15.                             
 Min.  Tangential stiffness 1.346842743E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         161

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         162
 Max.  Penetration of 0 has been detected between contact element 105533 
 and target element 105463.                                              
  
 Max.  Geometrical gap of 1.776356839E-15 has been detected between      
 contact element 105558 and target element 105479.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 105558 and target element 105479.               
 For total 26 contact elements, there are 26 elements are in contact.    
 There are 26 elements are in sticking.                                  
 Contacting area 1.863354652E-03.                                        
 Max.  Pinball distance 3.757887484E-02.                                 
 One of the contact searching regions contains at least 21 target        
 elements.                                                               
 Max.  Pressure/force 5.551960877E-03.                                   
 Max.  Normal stiffness 2.79412304E+14.                                  
 Min.  Normal stiffness 2.79412304E+14.                                  
 Max.  Tangential stiffness 1.408023489E+15.                             
 Min.  Tangential stiffness 1.408023489E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         175

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         176
 Max.  Penetration of 0 has been detected between contact element 106401 
 and target element 106353.                                              
  
 Max.  Geometrical gap of 1.110223025E-16 has been detected between      
 contact element 106406 and target element 106345.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 106406 and target element 106345.               
 For total 18 contact elements, there are 18 elements are in contact.    
 There are 18 elements are in sticking.                                  
 Contacting area 1.366252326E-03.                                        
 Max.  Pinball distance 9.051036043E-03.                                 
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 Max.  Pressure/force 2.183952046E-02.                                   
 Max.  Normal stiffness 1.160088188E+15.                                 
 Min.  Normal stiffness 1.160088188E+15.                                 
 Max.  Tangential stiffness 1.486136419E+15.                             
 Min.  Tangential stiffness 1.486136419E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         179

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         180
 Max.  Penetration of 0 has been detected between contact element 106573 
 and target element 106547.                                              
  
 Max.  Geometrical gap of 2.775557562E-17 has been detected between      
 contact element 106580 and target element 106534.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 106580 and target element 106534.               
 For total 14 contact elements, there are 14 elements are in contact.    
 There are 14 elements are in sticking.                                  
 Contacting area 1.192252328E-03.                                        
 Max.  Pinball distance 9.284549458E-03.                                 
 One of the contact searching regions contains at least 7 target         
 elements.                                                               
 Max.  Pressure/force 2.432885647E-02.                                   
 Max.  Normal stiffness 1.130911096E+15.                                 
 Min.  Normal stiffness 1.130911096E+15.                                 
 Max.  Tangential stiffness 1.300521509E+15.                             
 Min.  Tangential stiffness 1.300521509E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         181

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         182
 Max.  Penetration of 0 has been detected between contact element 106629 
 and target element 106609.                                              
  
 Max.  Geometrical gap of 1.110223025E-16 has been detected between      
 contact element 106632 and target element 106612.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 106632 and target element 106612.               
 For total 8 contact elements, there are 8 elements are in contact.      
 There are 8 elements are in sticking.                                   
 Contacting area 6.854369444E-04.                                        
 Max.  Pinball distance 2.531010883E-02.                                 
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force 1.788789492E-02.                                   
 Max.  Normal stiffness 4.148540044E+14.                                 
 Min.  Normal stiffness 4.148540044E+14.                                 
 Max.  Tangential stiffness 6.488537548E+14.                             
 Min.  Tangential stiffness 6.488537548E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         183

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         184
 Max.  Penetration of 0 has been detected between contact element 106721 
 and target element 106646.                                              
  
 Max.  Geometrical gap of 5.551115123E-17 has been detected between      
 contact element 106722 and target element 106658.                       
  
 Max.  Geometrical penetration of -1.387778781E-17 has been detected     
 between contact element 106722 and target element 106658.               
 For total 9 contact elements, there are 9 elements are in contact.      
 There are 9 elements are in sticking.                                   
 Contacting area 1.62E-03.                                               
 Max.  Pinball distance 4.898254653E-02.                                 
 One of the contact searching regions contains at least 31 target        
 elements.                                                               
 Max.  Pressure/force 5.204909512E-03.                                   
 Max.  Normal stiffness 2.143620686E+14.                                 
 Min.  Normal stiffness 2.143620686E+14.                                 
 Max.  Tangential stiffness 1.152246842E+15.                             
 Min.  Tangential stiffness 1.152246842E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         185

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         186
 Max.  Penetration of 0 has been detected between contact element 106859 
 and target element 106755.                                              
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 106870 and target element 106789.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 106870 and target element 106789.               
 For total 22 contact elements, there are 22 elements are in contact.    
 There are 22 elements are in sticking.                                  
 Contacting area 5.751809704E-03.                                        
 Max.  Pinball distance 6.488756721E-03.                                 
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 5.571371381E-02.                                   
 Max.  Normal stiffness 1.618183645E+15.                                 
 Min.  Normal stiffness 1.618183645E+15.                                 
 Max.  Tangential stiffness 8.12599347E+14.                              
 Min.  Tangential stiffness 8.12599347E+14.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         187

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         188
 Max.  Penetration of 0 has been detected between contact element 106945 
 and target element 106919.                                              
  
 Max.  Geometrical gap of 1.387778781E-17 has been detected between      
 contact element 106949 and target element 106906.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 106949 and target element 106906.               
 For total 14 contact elements, there are 14 elements are in contact.    
 There are 14 elements are in sticking.                                  
 Contacting area 1.192252326E-03.                                        
 Max.  Pinball distance 8.611811563E-03.                                 
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 Max.  Pressure/force 2.521381274E-02.                                   
 Max.  Normal stiffness 1.219255661E+15.                                 
 Min.  Normal stiffness 1.219255661E+15.                                 
 Max.  Tangential stiffness 1.352904147E+15.                             
 Min.  Tangential stiffness 1.352904147E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         191

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         192
 Max.  Penetration of 0 has been detected between contact element 107089 
 and target element 107033.                                              
  
 Max.  Geometrical gap of 1.387778781E-17 has been detected between      
 contact element 107095 and target element 107033.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 107095 and target element 107033.               
 For total 9 contact elements, there are 9 elements are in contact.      
 There are 9 elements are in sticking.                                   
 Contacting area 1.62E-03.                                               
 Max.  Pinball distance 4.898254552E-02.                                 
 One of the contact searching regions contains at least 31 target        
 elements.                                                               
 Max.  Pressure/force 5.204842733E-03.                                   
 Max.  Normal stiffness 2.14362073E+14.                                  
 Min.  Normal stiffness 2.14362073E+14.                                  
 Max.  Tangential stiffness 1.152261649E+15.                             
 Min.  Tangential stiffness 1.152261649E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         193

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         194
 Max.  Penetration of 0 has been detected between contact element 107227 
 and target element 107107.                                              
  
 Max.  Geometrical gap of 1.387778781E-17 has been detected between      
 contact element 107244 and target element 107151.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 107244 and target element 107151.               
 For total 23 contact elements, there are 23 elements are in contact.    
 There are 23 elements are in sticking.                                  
 Contacting area 5.751809704E-03.                                        
 Max.  Pinball distance 5.806402032E-03.                                 
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 6.136523435E-02.                                   
 Max.  Normal stiffness 1.808348775E+15.                                 
 Min.  Normal stiffness 1.808348775E+15.                                 
 Max.  Tangential stiffness 8.244618599E+14.                             
 Min.  Tangential stiffness 8.244618599E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         199

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         200
 Max.  Penetration of 0 has been detected between contact element 107671 
 and target element 107656.                                              
  
 Max.  Geometrical penetration of -1.776356839E-15 has been detected     
 between contact element 107672 and target element 107650.               
 For total 5 contact elements, there are 5 elements are in contact.      
 There are 5 elements are in sticking.                                   
 Contacting area 6.058602827E-04.                                        
 Max.  Pinball distance 1.317123374E-02.                                 
 One of the contact searching regions contains at least 13 target        
 elements.                                                               
 Max.  Pressure/force 5.352531744E-02.                                   
 Max.  Normal stiffness 7.971918353E+14.                                 
 Min.  Normal stiffness 7.971918353E+14.                                 
 Max.  Tangential stiffness 4.166912309E+14.                             
 Min.  Tangential stiffness 4.166912309E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         203

 *** NOTE ***                            CP =      23.594   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         204
 Max.  Penetration of 0 has been detected between contact element 107967 
 and target element 107918.                                              
  
 Max.  Geometrical gap of 4.163336342E-17 has been detected between      
 contact element 107967 and target element 107918.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 107967 and target element 107918.               
 For total 41 contact elements, there are 35 elements are in contact.    
 There are 35 elements are in sticking.                                  
 Contacting area 2.386936705E-03.                                        
 Max.  Pinball distance 8.841827513E-03.                                 
 One of the contact searching regions contains at least 7 target         
 elements.                                                               
 Max.  Pressure/force 1.862184411E-02.                                   
 Max.  Normal stiffness 1.187537303E+15.                                 
 Min.  Normal stiffness 1.187537303E+15.                                 
 Max.  Tangential stiffness 1.784166352E+15.                             
 Min.  Tangential stiffness 1.784166352E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         207
 Max.  Penetration of -3.081415487E-15 has been detected between contact 
 element 108164 and target element 108309.                               
  
 Max.  Geometrical gap of 9.E-03 has been detected between contact       
 element 108156 and target element 108288.                               
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -4.303286342E-04 has been detected     
 between contact element 108156 and target element 108288.               
 For total 63 contact elements, there are 54 elements are in contact.    
 There are 54 elements are in sticking.                                  
 Contacting area 6.999746221E-03.                                        
 Max.  Pinball distance 1.287878114E-02.                                 
 One of the contact searching regions contains at least 38 target        
 elements.                                                               
 Max.  Pressure/force 2.51226124.                                        
 Max.  Normal stiffness 8.152945445E+14.                                 
 Min.  Normal stiffness 8.152945445E+14.                                 
 Max.  Tangential stiffness 6.485382045E+14.                             
 Min.  Tangential stiffness 6.485382045E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         208

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         209
 Max.  Penetration of -2.054277572E-15 has been detected between contact 
 element 108443 and target element 108575.                               
  
 Max.  Geometrical gap of 9.E-03 has been detected between contact       
 element 108405 and target element 108542.                               
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -4.491127571E-04 has been detected     
 between contact element 108405 and target element 108542.               
 For total 65 contact elements, there are 53 elements are in contact.    
 There are 53 elements are in sticking.                                  
 Contacting area 6.485707267E-03.                                        
 Max.  Pinball distance 1.577136294E-02.                                 
 One of the contact searching regions contains at least 43 target        
 elements.                                                               
 Max.  Pressure/force -1.48391754.                                       
 Max.  Normal stiffness 6.6576364E+14.                                   
 Min.  Normal stiffness 6.6576364E+14.                                   
 Max.  Tangential stiffness 6.343736896E+14.                             
 Min.  Tangential stiffness 6.343736896E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         210

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         211

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         212
 Max.  Penetration of 0 has been detected between contact element 108743 
 and target element 108609.                                              
  
 Max.  Geometrical gap of 9.748335779E-04 has been detected between      
 contact element 108872 and target element 108646.                       
  
 Max.  Geometrical penetration of -5.551115123E-17 has been detected     
 between contact element 108872 and target element 108646.               
 For total 144 contact elements, there are 144 elements are in contact.  
 There are 144 elements are in sticking.                                 
 Contacting area 4.061416304E-03.                                        
 Max.  Pinball distance 1.332201279E-02.                                 
 One of the contact searching regions contains at least 18 target        
 elements.                                                               
 Max.  Pressure/force -6.562826847E-02.                                  
 Max.  Normal stiffness 7.881691878E+14.                                 
 Min.  Normal stiffness 7.881691878E+14.                                 
 Max.  Tangential stiffness 1.087475685E+15.                             
 Min.  Tangential stiffness 1.087475685E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         215

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 No contact was detected.                                                
 Max.  Pinball distance 2.16414514E-03.                                  
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         216

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         219

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         220
 Max.  Penetration of -4.440892099E-16 has been detected between contact 
 element 109340 and target element 109172.                               
  
 Max.  Geometrical gap of 1.776356839E-15 has been detected between      
 contact element 109331 and target element 109172.                       
  
 Max.  Geometrical penetration of -5.E-03 has been detected between      
 contact element 109331 and target element 109172.                       
 *WARNING*: The geometrical penetration may be too large.  Increase      
 pinball if it is a true geometrical penetration.  Decrease pinball if   
 it is a false one.                                                      
 For total 88 contact elements, there are 72 elements are in contact.    
 There are 72 elements are in sticking.                                  
 Contacting area 0.103141891.                                            
 Max.  Pinball distance 7.036612366E-03.                                 
 One of the contact searching regions contains at least 16 target        
 elements.                                                               
 Max.  Pressure/force 0.302992769.                                       
 Max.  Normal stiffness 6.822790616E+14.                                 
 Min.  Normal stiffness 6.822790616E+14.                                 
 Max.  Tangential stiffness 1.53512795E+14.                              
 Min.  Tangential stiffness 1.53512795E+14.                              
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         223
 Max.  Penetration of 0 has been detected between contact element 109495 
 and target element 109505.                                              
  
 Max.  Geometrical penetration of -4.440892099E-16 has been detected     
 between contact element 109495 and target element 109505.               
 For total 8 contact elements, there are 8 elements are in contact.      
 There are 8 elements are in sticking.                                   
 Contacting area 9.8E-04.                                                
 Max.  Pinball distance 1.715634787E-02.                                 
 One of the contact searching regions contains at least 2 target         
 elements.                                                               
 Max.  Pressure/force 2.369981119E-02.                                   
 Max.  Normal stiffness 5.520512792E+14.                                 
 Min.  Normal stiffness 5.520512792E+14.                                 
 Max.  Tangential stiffness 5.878415372E+14.                             
 Min.  Tangential stiffness 5.878415372E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         224

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         225

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         226
 Max.  Penetration of 0 has been detected between contact element 109524 
 and target element 109508.                                              
  
 Max.  Geometrical gap of 8.36518718E-04 has been detected between       
 contact element 109525 and target element 109507.                       
  
 Max.  Geometrical penetration of -4.440892099E-16 has been detected     
 between contact element 109525 and target element 109507.               
 For total 21 contact elements, there are 11 elements are in contact.    
 There are 11 elements are in sticking.                                  
 Contacting area 3.231160339E-04.                                        
 Max.  Pinball distance 8.502006764E-03.                                 
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 Max.  Pressure/force 1.051724151E-02.                                   
 Max.  Normal stiffness 9.092974694E+14.                                 
 Min.  Normal stiffness 9.092974694E+14.                                 
 Max.  Tangential stiffness 1.780955367E+15.                             
 Min.  Tangential stiffness 1.780955367E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         235

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 No contact was detected.                                                
 Max.  Pinball distance 2.16414514E-03.                                  
 One of the contact searching regions contains at least 6 target         
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         236

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         237

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         238
 Max.  Penetration of 0 has been detected between contact element 110539 
 and target element 110416.                                              
  
 Max.  Geometrical gap of 4.440892099E-16 has been detected between      
 contact element 110556 and target element 110413.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 110556 and target element 110413.               
 For total 160 contact elements, there are 84 elements are in contact.   
 There are 84 elements are in sticking.                                  
 Contacting area 5.161804186E-02.                                        
 Max.  Pinball distance 4.806133667E-03.                                 
 One of the contact searching regions contains at least 20 target        
 elements.                                                               
 Max.  Pressure/force 5.292796595E-02.                                   
 Max.  Normal stiffness 1.029071961E+15.                                 
 Min.  Normal stiffness 1.029071961E+15.                                 
 Max.  Tangential stiffness 2.562262397E+14.                             
 Min.  Tangential stiffness 2.562262397E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         239

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         240
 Max.  Penetration of 0 has been detected between contact element 110987 
 and target element 110866.                                              
  
 Max.  Geometrical gap of 4.440892099E-16 has been detected between      
 contact element 111078 and target element 110901.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 111078 and target element 110901.               
 For total 171 contact elements, there are 87 elements are in contact.   
 There are 87 elements are in sticking.                                  
 Contacting area 5.107396698E-02.                                        
 Max.  Pinball distance 4.451613033E-03.                                 
 One of the contact searching regions contains at least 20 target        
 elements.                                                               
 Max.  Pressure/force 5.273861351E-02.                                   
 Max.  Normal stiffness 1.045636822E+15.                                 
 Min.  Normal stiffness 1.045636822E+15.                                 
 Max.  Tangential stiffness 2.459075741E+14.                             
 Min.  Tangential stiffness 2.459075741E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         241
 Max.  Penetration of 0 has been detected between contact element 111501 
 and target element 111743.                                              
  
 Max.  Geometrical gap of 8.326672685E-17 has been detected between      
 contact element 111641 and target element 111745.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 111641 and target element 111745.               
 For total 172 contact elements, there are 172 elements are in contact.  
 There are 172 elements are in sticking.                                 
 Contacting area 1.187234237E-02.                                        
 Max.  Pinball distance 3.386569083E-02.                                 
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force 2.555115035E-13.                                   
 Max.  Normal stiffness 5298.97341.                                      
 Min.  Normal stiffness 5298.97341.                                      
 Max.  Tangential stiffness 9916.40908.                                  
 Min.  Tangential stiffness 9916.40908.                                  
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         242

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         243

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         244
 Max.  Penetration of 0 has been detected between contact element 112470 
 and target element 111829.                                              
  
 Max.  Geometrical gap of 1.776356839E-15 has been detected between      
 contact element 113001 and target element 111808.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 113001 and target element 111808.               
 For total 1125 contact elements, there are 508 elements are in contact. 
 There are 508 elements are in sticking.                                 
 Contacting area 0.126131075.                                            
 Max.  Pinball distance 2.650963928E-03.                                 
 One of the contact searching regions contains at least 16 target        
 elements.                                                               
 Max.  Pressure/force 1.738862371E-02.                                   
 Max.  Normal stiffness 5.538886363E+14.                                 
 Min.  Normal stiffness 5.538886363E+14.                                 
 Max.  Tangential stiffness 1.246249481E+14.                             
 Min.  Tangential stiffness 1.246249481E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         247

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         248
 Max.  Penetration of 0 has been detected between contact element 114413 
 and target element 114290.                                              
  
 Max.  Geometrical gap of 2.220446049E-16 has been detected between      
 contact element 114422 and target element 114264.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 114422 and target element 114264.               
 For total 24 contact elements, there are 24 elements are in contact.    
 There are 24 elements are in sticking.                                  
 Contacting area 1.4106E-02.                                             
 Max.  Pinball distance 1.747535686E-02.                                 
 One of the contact searching regions contains at least 24 target        
 elements.                                                               
 Max.  Pressure/force 5.229468416E-02.                                   
 Max.  Normal stiffness 6.008460991E+14.                                 
 Min.  Normal stiffness 6.008460991E+14.                                 
 Max.  Tangential stiffness 3.214522516E+14.                             
 Min.  Tangential stiffness 3.214522516E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         251
 Max.  Penetration of 0 has been detected between contact element 114581 
 and target element 114625.                                              
  
 Max.  Geometrical gap of 1.70535368E-04 has been detected between       
 contact element 114588 and target element 114623.                       
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 114588 and target element 114623.               
 For total 32 contact elements, there are 26 elements are in contact.    
 There are 26 elements are in sticking.                                  
 Contacting area 8.697592992E-04.                                        
 Max.  Pinball distance 9.729925934E-03.                                 
 One of the contact searching regions contains at least 8 target         
 elements.                                                               
 Max.  Pressure/force 1.008196856E-02.                                   
 Max.  Normal stiffness 1.034700408E+15.                                 
 Min.  Normal stiffness 1.034700408E+15.                                 
 Max.  Tangential stiffness 2.753055127E+15.                             
 Min.  Tangential stiffness 2.753055127E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         252

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         253

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         254
 Max.  Penetration of 0 has been detected between contact element 114801 
 and target element 114635.                                              
  
 Max.  Geometrical gap of 8.881784197E-16 has been detected between      
 contact element 114821 and target element 114654.                       
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 114821 and target element 114654.               
 For total 24 contact elements, there are 24 elements are in contact.    
 There are 24 elements are in sticking.                                  
 Contacting area 1.4106E-02.                                             
 Max.  Pinball distance 1.747537382E-02.                                 
 One of the contact searching regions contains at least 24 target        
 elements.                                                               
 Max.  Pressure/force 5.229463341E-02.                                   
 Max.  Normal stiffness 6.00845516E+14.                                  
 Min.  Normal stiffness 6.00845516E+14.                                  
 Max.  Tangential stiffness 3.214522516E+14.                             
 Min.  Tangential stiffness 3.214522516E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         255

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         256
 Max.  Penetration of 0 has been detected between contact element 114885 
 and target element 114851.                                              
  
 Max.  Geometrical gap of 8.881784197E-16 has been detected between      
 contact element 114899 and target element 114860.                       
  
 Max.  Geometrical penetration of -1.776356839E-15 has been detected     
 between contact element 114899 and target element 114860.               
 For total 26 contact elements, there are 18 elements are in contact.    
 There are 18 elements are in sticking.                                  
 Contacting area 3.036232073E-04.                                        
 Max.  Pinball distance 2.775119048E-02.                                 
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 2.814570011E-03.                                   
 Max.  Normal stiffness 3.783621466E+14.                                 
 Min.  Normal stiffness 3.783621466E+14.                                 
 Max.  Tangential stiffness 3.761026516E+15.                             
 Min.  Tangential stiffness 3.761026516E+15.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         257
 Max.  Penetration of 0 has been detected between contact element 115107 
 and target element 115294.                                              
  
 Max.  Geometrical penetration of -1.776356839E-15 has been detected     
 between contact element 115135 and target element 115304.               
 For total 114 contact elements, there are 28 elements are in contact.   
 There are 28 elements are in sticking.                                  
 Contacting area 3.421193983E-02.                                        
 Max.  Pinball distance 5.861668915E-03.                                 
 One of the contact searching regions contains at least 28 target        
 elements.                                                               
 Max.  Pressure/force 8.885759205E-02.                                   
 Max.  Normal stiffness 1.280071768E+15.                                 
 Min.  Normal stiffness 1.280071768E+15.                                 
 Max.  Tangential stiffness 2.880161593E+14.                             
 Min.  Tangential stiffness 2.880161593E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         258

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         263
 Max.  Penetration of 0 has been detected between contact element 115907 
 and target element 115961.                                              
  
 Max.  Geometrical gap of 2.253430249E-03 has been detected between      
 contact element 115949 and target element 115962.                       
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -2.775557562E-17 has been detected     
 between contact element 115949 and target element 115962.               
 For total 46 contact elements, there are 15 elements are in contact.    
 There are 15 elements are in sticking.                                  
 Contacting area 5.865446433E-04.                                        
 Max.  Pinball distance 3.749881797E-03.                                 
 One of the contact searching regions contains at least 6 target         
 elements.                                                               
 Max.  Pressure/force -0.255741975.                                      
 Max.  Normal stiffness 2.879398653E+14.                                 
 Min.  Normal stiffness 2.879398653E+14.                                 
 Max.  Tangential stiffness 1.448303037E+14.                             
 Min.  Tangential stiffness 1.448303037E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         264

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         265

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 No contact was detected.                                                
 Max.  Pinball distance 8.873475022E-03.                                 
 One of the contact searching regions contains at least 1 target         
 elements.                                                               
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         266

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         269
 Max.  Penetration of 0 has been detected between contact element 116007 
 and target element 116055.                                              
  
 Max.  Geometrical gap of 1.110223025E-16 has been detected between      
 contact element 116007 and target element 116055.                       
  
 Max.  Geometrical penetration of -1.110223025E-16 has been detected     
 between contact element 116007 and target element 116055.               
 For total 12 contact elements, there are 2 elements are in contact.     
 There are 2 elements are in sticking.                                   
 Contacting area 4.635E-04.                                              
 Max.  Pinball distance 1.812407689E-02.                                 
 One of the contact searching regions contains at least 14 target        
 elements.                                                               
 Max.  Pressure/force 3.058756189E-02.                                   
 Max.  Normal stiffness 5.793398509E+14.                                 
 Min.  Normal stiffness 5.793398509E+14.                                 
 Max.  Tangential stiffness 5.299065804E+14.                             
 Min.  Tangential stiffness 5.299065804E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         270

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         271

 *** NOTE ***                            CP =      23.609   TIME= 11:41:30
 Contact pair is inactive.                                               
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         272
 Max.  Penetration of 0 has been detected between contact element 116081 
 and target element 116071.                                              
  
 Max.  Geometrical gap of 6.181509964E-03 has been detected between      
 contact element 116083 and target element 116071.                       
 *WARNING*: The geometrical gap may be too large.  Increase pinball if   
 it is a true geometrical gap.  Decrease pinball if it is a false one.   
  
 Max.  Geometrical penetration of -8.881784197E-16 has been detected     
 between contact element 116083 and target element 116071.               
 For total 24 contact elements, there are 7 elements are in contact.     
 There are 7 elements are in sticking.                                   
 Contacting area 1.059564491E-03.                                        
 Max.  Pinball distance 6.413960482E-03.                                 
 One of the contact searching regions contains at least 4 target         
 elements.                                                               
 Max.  Pressure/force -0.302535318.                                      
 Max.  Normal stiffness 1.361401712E+15.                                 
 Min.  Normal stiffness 1.361401712E+15.                                 
 Max.  Tangential stiffness 3.085036764E+14.                             
 Min.  Tangential stiffness 3.085036764E+14.                             
 *************************************************
  
 *************************************************
  SUMMARY FOR CONTACT PAIR IDENTIFIED BY REAL CONSTANT SET         275
 Max.  Penetration of 0 has been detected between contact element 116185 
 and target element 116571.                                              
  
 Max.  Geometrical gap of 7.69059529E-17 has been detected between       
 contact element 116296 and target element 116544.                       
  
 Max.  Geometrical penetration of -9.795602115E-17 has been detected     
 between contact element 116296 and target element 116544.               
 For total 348 contact elements, there are 348 elements are in contact.  
 There are 348 elements are in sticking.                                 
 Contacting area 348.                                                    
 Max.  Pinball distance 1.274037563E-02.                                 
 One of the contact searching regions contains at least 12 target        
 elements.                                                               
 Max.  Pressure/force 9.6879961E-04.                                     
 Max.  Normal stiffness 2.140383106E+13.                                 
 Min.  Normal stiffness 2.140383106E+13.                                 
 Max.  Tangential stiffness 1.60528733E+13.                              
 Min.  Tangential stiffness 1.60528733E+13.                              
 *************************************************


                         ***********  PRECISE MASS SUMMARY  ***********

   TOTAL RIGID BODY MASS MATRIX ABOUT ORIGIN
               Translational mass               |   Coupled translational/rotational mass
         1551.2        0.0000        0.0000     |     0.0000        1940.0       -2856.4    
         0.0000        1551.2        0.0000     |    -1940.0        0.0000        5691.7    
         0.0000        0.0000        1551.2     |     2856.4       -5691.7        0.0000    
     ------------------------------------------ | ------------------------------------------
                                                |         Rotational mass (inertia)
                                                |     10887.       -10476.       -7214.3    
                                                |    -10476.        32436.       -3583.6    
                                                |    -7214.3       -3583.6        35069.    

   TOTAL MASS =  1551.2    
     The mass principal axes coincide with the global Cartesian axes

   CENTER OF MASS (X,Y,Z)=    3.6691        1.8414        1.2506    

   TOTAL INERTIA ABOUT CENTER OF MASS
         3201.2        4.0552       -96.158    
         4.0552        9126.8       -11.332    
        -96.158       -11.332        8926.2    

   PRINCIPAL INERTIAS =    3199.6        9127.4        8927.1    
   ORIENTATION VECTORS OF THE INERTIA PRINCIPAL AXES IN GLOBAL CARTESIAN
     ( 1.000,-0.001, 0.017) ( 0.002, 0.998,-0.057) (-0.017, 0.057, 0.998) 


  *** MASS SUMMARY BY ELEMENT TYPE ***

  TYPE      MASS
     1   4.26463    
     2   4.26566    
     3   4.26269    
     4   4.26423    
     5   4.26423    
     6   4.26423    
     7   4.26462    
     8   4.26422    
     9   4.26708    
    10   4.26422    
    11   4.26668    
    12   4.13934    
    13   1.77462    
    14   1.77643    
    15   3.91057    
    16   4.26708    
    17   4.26914    
    18   4.26216    
    19   4.26423    
    20   4.26708    
    21   4.26708    
    22   4.26422    
    23   4.26422    
    24   4.26422    
    25   4.26668    
    26   4.26668    
    27   4.41262    
    28   4.41262    
    29   4.41262    
    30   4.41262    
    31   140.748    
    32   32.4247    
    33   9.74404    
    34   9.74404    
    35   9.74404    
    36   9.74404    
    37   10.4587    
    38   10.4587    
    39   10.4587    
    40   10.4587    
    41   23.8947    
    42  0.103855    
    43   44.1082    
    44   47.2978    
    45  0.103855    
    46   251.205    
    47   37.2454    
    48   37.2455    
    49   54.9183    
    50   54.9183    
    51   73.7433    
    52   371.252    
    53   29.8977    
    54   29.8977    
    55   32.4227    
    56   85.9195    

 Range of element maximum matrix coefficients in global coordinates
 Maximum = 2.411919594E+13 at element 56612.                             
 Minimum = 1.856556941E-02 at element 111573.                            

 *** WARNING ***                         CP =      23.625   TIME= 11:41:30
 Coefficient ratio exceeds 1.0e8 - Check results.                        

   *** ELEMENT MATRIX FORMULATION TIMES
  TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

     1       727  SOLID187      0.078   0.000107
     2       740  SOLID187      0.078   0.000106
     3       748  SOLID187      0.078   0.000104
     4       719  SOLID187      0.109   0.000152
     5       739  SOLID187      0.125   0.000169
     6       718  SOLID187      0.078   0.000109
     7       717  SOLID187      0.094   0.000131
     8       733  SOLID187      0.094   0.000128
     9       725  SOLID187      0.094   0.000129
    10       724  SOLID187      0.109   0.000151
    11       727  SOLID187      0.094   0.000129
    12       702  SOLID187      0.078   0.000111
    13       477  SOLID187      0.078   0.000164
    14       473  SOLID187      0.078   0.000165
    15       632  SOLID187      0.094   0.000148
    16       726  SOLID187      0.078   0.000108
    17       737  SOLID187      0.062   0.000085
    18       718  SOLID187      0.109   0.000152
    19       728  SOLID187      0.078   0.000107
    20       717  SOLID187      0.094   0.000131
    21       733  SOLID187      0.062   0.000085
    22       723  SOLID187      0.094   0.000130
    23       718  SOLID187      0.062   0.000087
    24       722  SOLID187      0.109   0.000151
    25       734  SOLID187      0.062   0.000085
    26       734  SOLID187      0.078   0.000106
    27       685  SOLID187      0.078   0.000114
    28       777  SOLID187      0.078   0.000101
    29       656  SOLID187      0.031   0.000048
    30       798  SOLID187      0.094   0.000117
    31      3363  SOLID187      0.375   0.000112
    32      1477  SOLID187      0.172   0.000116
    33       811  SOLID187      0.125   0.000154
    34       796  SOLID187      0.078   0.000098
    35       798  SOLID187      0.094   0.000117
    36       801  SOLID187      0.078   0.000098
    37       716  SOLID187      0.078   0.000109
    38       731  SOLID187      0.156   0.000214
    39       735  SOLID187      0.078   0.000106
    40       743  SOLID187      0.094   0.000126
    41      1664  SOLID187      0.219   0.000131
    42        16  SOLID186      0.000   0.000000
    43      2316  SOLID187      0.250   0.000108
    44       915  SOLID187      0.109   0.000120
    45        16  SOLID186      0.000   0.000000
    46      8705  SOLID187      1.000   0.000115
    47      2150  SOLID187      0.203   0.000094
    48      2170  SOLID187      0.250   0.000115
    49      3398  SOLID187      0.391   0.000115
    50      3311  SOLID187      0.328   0.000099
    51      3831  SOLID187      0.438   0.000114
    52      9784  SOLID187      1.172   0.000120
    53       108  SOLID186      0.062   0.000579
    54       108  SOLID186      0.016   0.000145
    55      2164  SOLID187      0.312   0.000144
    56      9690  SOLID187      0.953   0.000098
    57       304  CONTA174      0.062   0.000206
    58       304  TARGE170      0.000   0.000000
    59       304  CONTA174      0.047   0.000154
    60       304  TARGE170      0.000   0.000000
    61       304  CONTA174      0.031   0.000103
    62       304  TARGE170      0.000   0.000000
    63       304  CONTA174      0.047   0.000154
    64       304  TARGE170      0.000   0.000000
    65       304  CONTA174      0.031   0.000103
    66       304  TARGE170      0.000   0.000000
    67       316  CONTA174      0.031   0.000099
    68       316  TARGE170      0.016   0.000049
    69       304  CONTA174      0.031   0.000103
    70       304  TARGE170      0.000   0.000000
    71       304  CONTA174      0.016   0.000051
    72       304  TARGE170      0.016   0.000051
    73       304  CONTA174      0.047   0.000154
    74       304  TARGE170      0.000   0.000000
    75       292  CONTA174      0.047   0.000161
    76       292  TARGE170      0.000   0.000000
    77       304  CONTA174      0.000   0.000000
    78       304  TARGE170      0.000   0.000000
    79       288  CONTA174      0.062   0.000217
    80       288  TARGE170      0.000   0.000000
    81       148  CONTA174      0.016   0.000106
    82       148  TARGE170      0.000   0.000000
    83       147  CONTA174      0.000   0.000000
    84       147  TARGE170      0.000   0.000000
    85       274  CONTA174      0.016   0.000057
    86       274  TARGE170      0.000   0.000000
    87       304  CONTA174      0.031   0.000103
    88       304  TARGE170      0.000   0.000000
    89       316  CONTA174      0.031   0.000099
    90       316  TARGE170      0.000   0.000000
    91       304  CONTA174      0.031   0.000103
    92       304  TARGE170      0.000   0.000000
    93       304  CONTA174      0.016   0.000051
    94       304  TARGE170      0.000   0.000000
    95       304  CONTA174      0.031   0.000103
    96       304  TARGE170      0.000   0.000000
    97       292  CONTA174      0.031   0.000107
    98       292  TARGE170      0.000   0.000000
    99       304  CONTA174      0.031   0.000103
   100       304  TARGE170      0.000   0.000000
   101       304  CONTA174      0.016   0.000051
   102       304  TARGE170      0.016   0.000051
   103       304  CONTA174      0.047   0.000154
   104       304  TARGE170      0.000   0.000000
   105       304  CONTA174      0.078   0.000257
   106       304  TARGE170      0.000   0.000000
   107       316  CONTA174      0.031   0.000099
   108       316  TARGE170      0.000   0.000000
   109       162  CONTA174      0.000   0.000000
   110       162  TARGE170      0.016   0.000096
   111        33  CONTA174      0.000   0.000000
   112        33  TARGE170      0.000   0.000000
   113       158  CONTA174      0.031   0.000198
   114       158  TARGE170      0.000   0.000000
   115        35  CONTA174      0.000   0.000000
   116        35  TARGE170      0.016   0.000446
   117       138  CONTA174      0.000   0.000000
   118       138  TARGE170      0.000   0.000000
   119        41  CONTA174      0.000   0.000000
   120        41  TARGE170      0.000   0.000000
   121       138  CONTA174      0.031   0.000226
   122       138  TARGE170      0.000   0.000000
   123        34  CONTA174      0.000   0.000000
   124        34  TARGE170      0.000   0.000000
   125       625  CONTA174      0.062   0.000100
   126       625  TARGE170      0.016   0.000025
   127       116  CONTA174      0.016   0.000135
   128       116  TARGE170      0.000   0.000000
   129       105  CONTA174      0.000   0.000000
   130       105  TARGE170      0.000   0.000000
   131       273  CONTA174      0.031   0.000114
   132       273  TARGE170      0.000   0.000000
   133        24  CONTA174      0.000   0.000000
   134        24  TARGE170      0.000   0.000000
   135        24  CONTA174      0.000   0.000000
   136        24  TARGE170      0.000   0.000000
   137        56  CONTA174      0.000   0.000000
   138        56  TARGE170      0.000   0.000000
   139        15  CONTA174      0.000   0.000000
   140        15  TARGE170      0.000   0.000000
   141        11  CONTA174      0.016   0.001420
   142        11  TARGE170      0.000   0.000000
   143       228  CONTA174      0.031   0.000137
   144       228  TARGE170      0.000   0.000000
   145       240  CONTA174      0.016   0.000065
   146       240  TARGE170      0.000   0.000000
   147        21  CONTA174      0.000   0.000000
   148        21  TARGE170      0.000   0.000000
   149      1212  CONTA174      0.156   0.000129
   150      1212  TARGE170      0.031   0.000026
   151        69  CONTA174      0.000   0.000000
   152        69  TARGE170      0.000   0.000000
   153        15  CONTA174      0.000   0.000000
   154        15  TARGE170      0.000   0.000000
   155        24  CONTA174      0.000   0.000000
   156        24  TARGE170      0.000   0.000000
   157        92  CONTA174      0.000   0.000000
   158        92  TARGE170      0.016   0.000170
   159        15  CONTA174      0.000   0.000000
   160        15  TARGE170      0.000   0.000000
   161        69  CONTA174      0.000   0.000000
   162        69  TARGE170      0.000   0.000000
   163        93  CONTA174      0.000   0.000000
   164        93  TARGE170      0.000   0.000000
   165        83  CONTA174      0.031   0.000377
   166        83  TARGE170      0.000   0.000000
   167        48  CONTA174      0.000   0.000000
   168        48  TARGE170      0.000   0.000000
   169        47  CONTA174      0.000   0.000000
   170        47  TARGE170      0.000   0.000000
   171        83  CONTA174      0.000   0.000000
   172        83  TARGE170      0.000   0.000000
   173        24  CONTA174      0.000   0.000000
   174        24  TARGE170      0.000   0.000000
   175        48  CONTA174      0.016   0.000326
   176        48  TARGE170      0.000   0.000000
   177        47  CONTA174      0.016   0.000332
   178        47  TARGE170      0.000   0.000000
   179        35  CONTA174      0.000   0.000000
   180        35  TARGE170      0.016   0.000446
   181        22  CONTA174      0.000   0.000000
   182        22  TARGE170      0.000   0.000000
   183        47  CONTA174      0.000   0.000000
   184        47  TARGE170      0.000   0.000000
   185        82  CONTA174      0.016   0.000191
   186        82  TARGE170      0.000   0.000000
   187        35  CONTA174      0.000   0.000000
   188        35  TARGE170      0.000   0.000000
   189        20  CONTA174      0.000   0.000000
   190        20  TARGE170      0.000   0.000000
   191        47  CONTA174      0.000   0.000000
   192        47  TARGE170      0.000   0.000000
   193        83  CONTA174      0.000   0.000000
   194        83  TARGE170      0.000   0.000000
   195       110  CONTA174      0.000   0.000000
   196       110  TARGE170      0.000   0.000000
   197        75  CONTA174      0.016   0.000208
   198        75  TARGE170      0.000   0.000000
   199        19  CONTA174      0.000   0.000000
   200        19  TARGE170      0.000   0.000000
   201       109  CONTA174      0.016   0.000143
   202       109  TARGE170      0.000   0.000000
   203        75  CONTA174      0.016   0.000208
   204        75  TARGE170      0.000   0.000000
   205        21  CONTA174      0.000   0.000000
   206        21  TARGE170      0.000   0.000000
   207       123  CONTA174      0.031   0.000254
   208       123  TARGE170      0.000   0.000000
   209       126  CONTA174      0.016   0.000124
   210       126  TARGE170      0.000   0.000000
   211       221  CONTA174      0.016   0.000071
   212       221  TARGE170      0.000   0.000000
   213        16  CONTA174      0.000   0.000000
   214        16  TARGE170      0.000   0.000000
   215        16  CONTA174      0.000   0.000000
   216        16  TARGE170      0.000   0.000000
   217        14  CONTA174      0.000   0.000000
   218        14  TARGE170      0.000   0.000000
   219       166  CONTA174      0.031   0.000188
   220       166  TARGE170      0.000   0.000000
   221        16  CONTA174      0.000   0.000000
   222        16  TARGE170      0.000   0.000000
   223        10  CONTA174      0.000   0.000000
   224        10  TARGE170      0.000   0.000000
   225        29  CONTA174      0.000   0.000000
   226        29  TARGE170      0.000   0.000000
   227        29  CONTA174      0.000   0.000000
   228        29  TARGE170      0.000   0.000000
   229       170  CONTA174      0.031   0.000184
   230       170  TARGE170      0.000   0.000000
   231       152  CONTA174      0.031   0.000206
   232       152  TARGE170      0.000   0.000000
   233        56  CONTA174      0.016   0.000279
   234        56  TARGE170      0.000   0.000000
   235        16  CONTA174      0.000   0.000000
   236        16  TARGE170      0.000   0.000000
   237       224  CONTA174      0.016   0.000070
   238       224  TARGE170      0.000   0.000000
   239       235  CONTA174      0.016   0.000066
   240       235  TARGE170      0.000   0.000000
   241       216  CONTA174      0.000   0.000000
   242       216  TARGE170      0.000   0.000000
   243      1198  CONTA174      0.250   0.000209
   244      1198  TARGE170      0.016   0.000013
   245        39  CONTA174      0.000   0.000000
   246        39  TARGE170      0.000   0.000000
   247       113  CONTA174      0.000   0.000000
   248       113  TARGE170      0.000   0.000000
   249        44  CONTA174      0.016   0.000355
   250        44  TARGE170      0.000   0.000000
   251        40  CONTA174      0.000   0.000000
   252        40  TARGE170      0.000   0.000000
   253       110  CONTA174      0.016   0.000142
   254       110  TARGE170      0.000   0.000000
   255        44  CONTA174      0.016   0.000355
   256        44  TARGE170      0.000   0.000000
   257       194  CONTA174      0.016   0.000081
   258       194  TARGE170      0.000   0.000000
   259        54  CONTA174      0.016   0.000289
   260        54  TARGE170      0.000   0.000000
   261       214  CONTA174      0.016   0.000073
   262       214  TARGE170      0.000   0.000000
   263        52  CONTA174      0.016   0.000300
   264        52  TARGE170      0.000   0.000000
   265         7  CONTA174      0.000   0.000000
   266         7  TARGE170      0.000   0.000000
   267         7  CONTA174      0.000   0.000000
   268         7  TARGE170      0.000   0.000000
   269        39  CONTA174      0.000   0.000000
   270        39  TARGE170      0.000   0.000000
   271        29  CONTA174      0.000   0.000000
   272        29  TARGE170      0.000   0.000000
   273        28  CONTA174      0.000   0.000000
   274        28  TARGE170      0.000   0.000000
   275       348  CONTA175      0.031   0.000090
   276        44  TARGE170      0.000   0.000000
   277      9113  SURF154       0.484   0.000053
 Time at end of element matrix formulation CP = 23.625.                  
     FORCE CONVERGENCE VALUE  = 0.1587E+09  CRITERION= 0.8097E+06

 DISTRIBUTED SPARSE MATRIX DIRECT SOLVER.
  Number of equations =      528258,    Maximum wavefront =    642

 *** NOTE ***                            CP =      28.031   TIME= 11:41:35
 The initial memory allocation (-m) has been exceeded.                   
  Supplemental memory allocations are being used.                        

  Local memory allocated for solver              =   1069.599 MB
  Local memory required for in-core solution     =    952.903 MB
  Local memory required for out-of-core solution =    474.884 MB

  Total memory allocated for solver              =   2109.213 MB
  Total memory required for in-core solution     =   1874.561 MB
  Total memory required for out-of-core solution =    866.246 MB

 *** NOTE ***                            CP =      28.031   TIME= 11:41:35
 The Distributed Sparse Matrix Solver is currently running in the        
 in-core memory mode.  This memory mode uses the most amount of memory   
 in order to avoid using the hard drive as much as possible, which most  
 often results in the fastest solution time.  This mode is recommended   
 if enough physical memory is present to accommodate all of the solver   
 data.                                                                   
 curEqn= 181188  totEqn= 265584 Job CP sec=     33.047
      Factor Done=  50% Factor Wall sec=      2.511 rate=    8236.3 Mflops
 curEqn= 265584  totEqn= 265584 Job CP sec=     35.688
      Factor Done= 100% Factor Wall sec=      5.163 rate=    7994.9 Mflops
 Distributed sparse solver maximum pivot= 4.003916685E+13 at node 128810 
 UY.                                                                     
 Distributed sparse solver minimum pivot= 38203.899 at node 68164 UX.    
 Distributed sparse solver minimum pivot in absolute value= 38203.899 at 
 node 68164 UX.                                                          
     DISP CONVERGENCE VALUE   = 0.1647E-01  CRITERION= 0.8401E-03

 *** WARNING ***                         CP =      40.375   TIME= 11:41:47
 Contact element 98263 (real ID 113) status changes abruptly from        
 contact (with target element 98339) -> no-contact.                      

   *** ELEMENT RESULT CALCULATION TIMES
  TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

     1       727  SOLID187      0.078   0.000107
     2       740  SOLID187      0.078   0.000106
     3       748  SOLID187      0.062   0.000084
     4       719  SOLID187      0.078   0.000109
     5       739  SOLID187      0.016   0.000021
     6       718  SOLID187      0.062   0.000087
     7       717  SOLID187      0.078   0.000109
     8       733  SOLID187      0.094   0.000128
     9       725  SOLID187      0.062   0.000086
    10       724  SOLID187      0.094   0.000129
    11       727  SOLID187      0.078   0.000107
    12       702  SOLID187      0.109   0.000156
    13       477  SOLID187      0.016   0.000033
    14       473  SOLID187      0.062   0.000132
    15       632  SOLID187      0.094   0.000148
    16       726  SOLID187      0.094   0.000129
    17       737  SOLID187      0.094   0.000127
    18       718  SOLID187      0.047   0.000065
    19       728  SOLID187      0.094   0.000129
    20       717  SOLID187      0.047   0.000065
    21       733  SOLID187      0.078   0.000107
    22       723  SOLID187      0.094   0.000130
    23       718  SOLID187      0.062   0.000087
    24       722  SOLID187      0.031   0.000043
    25       734  SOLID187      0.031   0.000043
    26       734  SOLID187      0.047   0.000064
    27       685  SOLID187      0.062   0.000091
    28       777  SOLID187      0.109   0.000141
    29       656  SOLID187      0.078   0.000119
    30       798  SOLID187      0.047   0.000059
    31      3363  SOLID187      0.297   0.000088
    32      1477  SOLID187      0.094   0.000063
    33       811  SOLID187      0.031   0.000039
    34       796  SOLID187      0.062   0.000079
    35       798  SOLID187      0.062   0.000078
    36       801  SOLID187      0.062   0.000078
    37       716  SOLID187      0.062   0.000087
    38       731  SOLID187      0.062   0.000085
    39       735  SOLID187      0.094   0.000128
    40       743  SOLID187      0.094   0.000126
    41      1664  SOLID187      0.188   0.000113
    42        16  SOLID186      0.000   0.000000
    43      2316  SOLID187      0.234   0.000101
    44       915  SOLID187      0.062   0.000068
    45        16  SOLID186      0.000   0.000000
    46      8705  SOLID187      0.891   0.000102
    47      2150  SOLID187      0.125   0.000058
    48      2170  SOLID187      0.172   0.000079
    49      3398  SOLID187      0.328   0.000097
    50      3311  SOLID187      0.234   0.000071
    51      3831  SOLID187      0.375   0.000098
    52      9784  SOLID187      1.016   0.000104
    53       108  SOLID186      0.016   0.000145
    54       108  SOLID186      0.031   0.000289
    55      2164  SOLID187      0.219   0.000101
    56      9690  SOLID187      0.922   0.000095
    57       304  CONTA174      0.031   0.000103
    59       304  CONTA174      0.016   0.000051
    61       304  CONTA174      0.031   0.000103
    63       304  CONTA174      0.047   0.000154
    65       304  CONTA174      0.016   0.000051
    67       316  CONTA174      0.016   0.000049
    69       304  CONTA174      0.016   0.000051
    71       304  CONTA174      0.000   0.000000
    73       304  CONTA174      0.016   0.000051
    75       292  CONTA174      0.000   0.000000
    77       304  CONTA174      0.000   0.000000
    79       288  CONTA174      0.000   0.000000
    81       148  CONTA174      0.000   0.000000
    83       147  CONTA174      0.000   0.000000
    85       274  CONTA174      0.000   0.000000
    87       304  CONTA174      0.016   0.000051
    89       316  CONTA174      0.000   0.000000
    91       304  CONTA174      0.000   0.000000
    93       304  CONTA174      0.016   0.000051
    95       304  CONTA174      0.000   0.000000
    97       292  CONTA174      0.016   0.000054
    99       304  CONTA174      0.016   0.000051
   101       304  CONTA174      0.000   0.000000
   103       304  CONTA174      0.031   0.000103
   105       304  CONTA174      0.031   0.000103
   107       316  CONTA174      0.000   0.000000
   109       162  CONTA174      0.000   0.000000
   111        33  CONTA174      0.016   0.000473
   113       158  CONTA174      0.000   0.000000
   115        35  CONTA174      0.000   0.000000
   117       138  CONTA174      0.016   0.000113
   119        41  CONTA174      0.000   0.000000
   121       138  CONTA174      0.000   0.000000
   123        34  CONTA174      0.000   0.000000
   125       625  CONTA174      0.047   0.000075
   127       116  CONTA174      0.000   0.000000
   129       105  CONTA174      0.000   0.000000
   131       273  CONTA174      0.000   0.000000
   133        24  CONTA174      0.000   0.000000
   135        24  CONTA174      0.000   0.000000
   137        56  CONTA174      0.000   0.000000
   139        15  CONTA174      0.000   0.000000
   141        11  CONTA174      0.000   0.000000
   143       228  CONTA174      0.016   0.000069
   145       240  CONTA174      0.000   0.000000
   147        21  CONTA174      0.016   0.000744
   149      1212  CONTA174      0.094   0.000077
   151        69  CONTA174      0.000   0.000000
   153        15  CONTA174      0.000   0.000000
   155        24  CONTA174      0.000   0.000000
   157        92  CONTA174      0.016   0.000170
   159        15  CONTA174      0.000   0.000000
   161        69  CONTA174      0.000   0.000000
   163        93  CONTA174      0.000   0.000000
   165        83  CONTA174      0.000   0.000000
   167        48  CONTA174      0.000   0.000000
   169        47  CONTA174      0.016   0.000332
   171        83  CONTA174      0.000   0.000000
   173        24  CONTA174      0.000   0.000000
   175        48  CONTA174      0.000   0.000000
   177        47  CONTA174      0.000   0.000000
   179        35  CONTA174      0.000   0.000000
   181        22  CONTA174      0.000   0.000000
   183        47  CONTA174      0.000   0.000000
   185        82  CONTA174      0.016   0.000191
   187        35  CONTA174      0.000   0.000000
   189        20  CONTA174      0.000   0.000000
   191        47  CONTA174      0.000   0.000000
   193        83  CONTA174      0.031   0.000377
   195       110  CONTA174      0.016   0.000142
   197        75  CONTA174      0.000   0.000000
   199        19  CONTA174      0.000   0.000000
   201       109  CONTA174      0.016   0.000143
   203        75  CONTA174      0.000   0.000000
   205        21  CONTA174      0.000   0.000000
   207       123  CONTA174      0.000   0.000000
   209       126  CONTA174      0.016   0.000124
   211       221  CONTA174      0.000   0.000000
   213        16  CONTA174      0.000   0.000000
   215        16  CONTA174      0.000   0.000000
   217        14  CONTA174      0.000   0.000000
   219       166  CONTA174      0.016   0.000094
   221        16  CONTA174      0.000   0.000000
   223        10  CONTA174      0.000   0.000000
   225        29  CONTA174      0.000   0.000000
   227        29  CONTA174      0.016   0.000539
   229       170  CONTA174      0.016   0.000092
   231       152  CONTA174      0.016   0.000103
   233        56  CONTA174      0.000   0.000000
   235        16  CONTA174      0.000   0.000000
   237       224  CONTA174      0.031   0.000140
   239       235  CONTA174      0.000   0.000000
   241       216  CONTA174      0.031   0.000145
   243      1198  CONTA174      0.031   0.000026
   245        39  CONTA174      0.000   0.000000
   247       113  CONTA174      0.000   0.000000
   249        44  CONTA174      0.000   0.000000
   251        40  CONTA174      0.000   0.000000
   253       110  CONTA174      0.016   0.000142
   255        44  CONTA174      0.000   0.000000
   257       194  CONTA174      0.000   0.000000
   259        54  CONTA174      0.016   0.000289
   261       214  CONTA174      0.000   0.000000
   263        52  CONTA174      0.000   0.000000
   265         7  CONTA174      0.000   0.000000
   267         7  CONTA174      0.016   0.002232
   269        39  CONTA174      0.000   0.000000
   271        29  CONTA174      0.000   0.000000
   273        28  CONTA174      0.016   0.000558
   275       348  CONTA175      0.016   0.000045
   277      9113  SURF154       0.344   0.000038

   *** NODAL LOAD CALCULATION TIMES
  TYPE    NUMBER   ENAME      TOTAL CP  AVE CP

     1       727  SOLID187      0.000   0.000000
     2       740  SOLID187      0.000   0.000000
     3       748  SOLID187      0.000   0.000000
     4       719  SOLID187      0.000   0.000000
     5       739  SOLID187      0.000   0.000000
     6       718  SOLID187      0.000   0.000000
     7       717  SOLID187      0.000   0.000000
     8       733  SOLID187      0.000   0.000000
     9       725  SOLID187      0.016   0.000022
    10       724  SOLID187      0.000   0.000000
    11       727  SOLID187      0.000   0.000000
    12       702  SOLID187      0.000   0.000000
    13       477  SOLID187      0.000   0.000000
    14       473  SOLID187      0.000   0.000000
    15       632  SOLID187      0.000   0.000000
    16       726  SOLID187      0.000   0.000000
    17       737  SOLID187      0.016   0.000021
    18       718  SOLID187      0.000   0.000000
    19       728  SOLID187      0.000   0.000000
    20       717  SOLID187      0.000   0.000000
    21       733  SOLID187      0.000   0.000000
    22       723  SOLID187      0.000   0.000000
    23       718  SOLID187      0.000   0.000000
    24       722  SOLID187      0.000   0.000000
    25       734  SOLID187      0.000   0.000000
    26       734  SOLID187      0.000   0.000000
    27       685  SOLID187      0.000   0.000000
    28       777  SOLID187      0.000   0.000000
    29       656  SOLID187      0.016   0.000024
    30       798  SOLID187      0.000   0.000000
    31      3363  SOLID187      0.016   0.000005
    32      1477  SOLID187      0.000   0.000000
    33       811  SOLID187      0.000   0.000000
    34       796  SOLID187      0.000   0.000000
    35       798  SOLID187      0.000   0.000000
    36       801  SOLID187      0.016   0.000020
    37       716  SOLID187      0.000   0.000000
    38       731  SOLID187      0.000   0.000000
    39       735  SOLID187      0.000   0.000000
    40       743  SOLID187      0.000   0.000000
    41      1664  SOLID187      0.000   0.000000
    42        16  SOLID186      0.000   0.000000
    43      2316  SOLID187      0.000   0.000000
    44       915  SOLID187      0.000   0.000000
    45        16  SOLID186      0.000   0.000000
    46      8705  SOLID187      0.047   0.000005
    47      2150  SOLID187      0.031   0.000015
    48      2170  SOLID187      0.016   0.000007
    49      3398  SOLID187      0.047   0.000014
    50      3311  SOLID187      0.000   0.000000
    51      3831  SOLID187      0.000   0.000000
    52      9784  SOLID187      0.016   0.000002
    53       108  SOLID186      0.000   0.000000
    54       108  SOLID186      0.000   0.000000
    55      2164  SOLID187      0.000   0.000000
    56      9690  SOLID187      0.031   0.000003
    57       304  CONTA174      0.000   0.000000
    59       304  CONTA174      0.000   0.000000
    61       304  CONTA174      0.016   0.000051
    63       304  CONTA174      0.000   0.000000
    65       304  CONTA174      0.000   0.000000
    67       316  CONTA174      0.000   0.000000
    69       304  CONTA174      0.000   0.000000
    71       304  CONTA174      0.000   0.000000
    73       304  CONTA174      0.000   0.000000
    75       292  CONTA174      0.000   0.000000
    77       304  CONTA174      0.000   0.000000
    79       288  CONTA174      0.000   0.000000
    81       148  CONTA174      0.000   0.000000
    83       147  CONTA174      0.000   0.000000
    85       274  CONTA174      0.000   0.000000
    87       304  CONTA174      0.000   0.000000
    89       316  CONTA174      0.000   0.000000
    91       304  CONTA174      0.000   0.000000
    93       304  CONTA174      0.000   0.000000
    95       304  CONTA174      0.000   0.000000
    97       292  CONTA174      0.000   0.000000
    99       304  CONTA174      0.000   0.000000
   101       304  CONTA174      0.016   0.000051
   103       304  CONTA174      0.000   0.000000
   105       304  CONTA174      0.000   0.000000
   107       316  CONTA174      0.000   0.000000
   109       162  CONTA174      0.000   0.000000
   111        33  CONTA174      0.000   0.000000
   113       158  CONTA174      0.000   0.000000
   115        35  CONTA174      0.000   0.000000
   117       138  CONTA174      0.000   0.000000
   119        41  CONTA174      0.000   0.000000
   121       138  CONTA174      0.000   0.000000
   123        34  CONTA174      0.000   0.000000
   125       625  CONTA174      0.000   0.000000
   127       116  CONTA174      0.000   0.000000
   129       105  CONTA174      0.000   0.000000
   131       273  CONTA174      0.016   0.000057
   133        24  CONTA174      0.000   0.000000
   135        24  CONTA174      0.000   0.000000
   137        56  CONTA174      0.000   0.000000
   139        15  CONTA174      0.000   0.000000
   141        11  CONTA174      0.000   0.000000
   143       228  CONTA174      0.000   0.000000
   145       240  CONTA174      0.016   0.000065
   147        21  CONTA174      0.000   0.000000
   149      1212  CONTA174      0.016   0.000013
   151        69  CONTA174      0.000   0.000000
   153        15  CONTA174      0.000   0.000000
   155        24  CONTA174      0.000   0.000000
   157        92  CONTA174      0.000   0.000000
   159        15  CONTA174      0.000   0.000000
   161        69  CONTA174      0.000   0.000000
   163        93  CONTA174      0.000   0.000000
   165        83  CONTA174      0.000   0.000000
   167        48  CONTA174      0.000   0.000000
   169        47  CONTA174      0.000   0.000000
   171        83  CONTA174      0.000   0.000000
   173        24  CONTA174      0.000   0.000000
   175        48  CONTA174      0.000   0.000000
   177        47  CONTA174      0.000   0.000000
   179        35  CONTA174      0.000   0.000000
   181        22  CONTA174      0.000   0.000000
   183        47  CONTA174      0.000   0.000000
   185        82  CONTA174      0.000   0.000000
   187        35  CONTA174      0.000   0.000000
   189        20  CONTA174      0.000   0.000000
   191        47  CONTA174      0.000   0.000000
   193        83  CONTA174      0.000   0.000000
   195       110  CONTA174      0.000   0.000000
   197        75  CONTA174      0.000   0.000000
   199        19  CONTA174      0.000   0.000000
   201       109  CONTA174      0.000   0.000000
   203        75  CONTA174      0.000   0.000000
   205        21  CONTA174      0.000   0.000000
   207       123  CONTA174      0.000   0.000000
   209       126  CONTA174      0.000   0.000000
   211       221  CONTA174      0.000   0.000000
   213        16  CONTA174      0.000   0.000000
   215        16  CONTA174      0.000   0.000000
   217        14  CONTA174      0.000   0.000000
   219       166  CONTA174      0.000   0.000000
   221        16  CONTA174      0.000   0.000000
   223        10  CONTA174      0.000   0.000000
   225        29  CONTA174      0.000   0.000000
   227        29  CONTA174      0.000   0.000000
   229       170  CONTA174      0.000   0.000000
   231       152  CONTA174      0.000   0.000000
   233        56  CONTA174      0.000   0.000000
   235        16  CONTA174      0.000   0.000000
   237       224  CONTA174      0.000   0.000000
   239       235  CONTA174      0.000   0.000000
   241       216  CONTA174      0.000   0.000000
   243      1198  CONTA174      0.000   0.000000
   245        39  CONTA174      0.000   0.000000
   247       113  CONTA174      0.000   0.000000
   249        44  CONTA174      0.000   0.000000
   251        40  CONTA174      0.000   0.000000
   253       110  CONTA174      0.000   0.000000
   255        44  CONTA174      0.000   0.000000
   257       194  CONTA174      0.000   0.000000
   259        54  CONTA174      0.000   0.000000
   261       214  CONTA174      0.000   0.000000
   263        52  CONTA174      0.000   0.000000
   265         7  CONTA174      0.016   0.002232
   267         7  CONTA174      0.000   0.000000
   269        39  CONTA174      0.000   0.000000
   271        29  CONTA174      0.000   0.000000
   273        28  CONTA174      0.000   0.000000
   275       348  CONTA175      0.000   0.000000
   277      9113  SURF154       0.016   0.000002
 *** LOAD STEP     1   SUBSTEP     1  COMPLETED.    CUM ITER =      1
 *** TIME =   1.00000         TIME INC =   1.00000      NEW TRIANG MATRIX


 *** ANSYS BINARY FILE STATISTICS
  BUFFER SIZE USED= 16384
      186.938 MB WRITTEN ON ELEMENT SAVED DATA FILE: file0.esav
      143.250 MB WRITTEN ON ASSEMBLED MATRIX FILE: file0.full
       48.500 MB WRITTEN ON RESULTS FILE: file0.rst
 *************** Write FE CONNECTORS *********

 WRITE OUT CONSTRAINT EQUATIONS TO FILE= file.ce                                                                                                                                                                                                                                                             
 ****************************************************
 *************** FINISHED SOLVE FOR LS 1 *************

 PARAMETER _DS_PROGRESS  DELETED.

 *GET  _WALLASOL  FROM  ACTI  ITEM=TIME WALL  VALUE=  11.6972222    

 PRINTOUT RESUMED BY /GOP

 FINISH SOLUTION PROCESSING


 ***** ROUTINE COMPLETED *****  CP =        43.766



 *** ANSYS - ENGINEERING ANALYSIS SYSTEM  RELEASE Release 17.0     17.0     ***
 DISTRIBUTED ANSYS Multiphysics                                

 00000000  VERSION=WINDOWS x64   11:41:51  JUN 15, 2019 CP=     43.781

 unsaved_project--Static Structural (A5)                                       



          ***** ANSYS RESULTS INTERPRETATION (POST1) *****

 *** NOTE ***                            CP =      43.797   TIME= 11:41:51
 Reading results into the database (SET command) will update the current 
 displacement and force boundary conditions in the database with the     
 values from the results file for that load set.  Note that any          
 subsequent solutions will use these values unless action is taken to    
 either SAVE the current values or not overwrite them (/EXIT,NOSAVE).    

 Set Encoding of XML File to:ISO-8859-1

 Set Output of XML File to:
     PARM,     ,     ,     ,     ,     ,     ,     ,     ,     ,     ,     ,
         ,     ,     ,     ,     ,     ,     ,

 DATABASE WRITTEN ON FILE  parm.xml                                                                                                                                                                                                                                                            

 EXIT THE ANSYS POST1 DATABASE PROCESSOR


 ***** ROUTINE COMPLETED *****  CP =        43.797



 PRINTOUT RESUMED BY /GOP

 *GET  _WALLDONE  FROM  ACTI  ITEM=TIME WALL  VALUE=  11.6975000    

 PARAMETER _PREPTIME =     2.000000000    

 PARAMETER _SOLVTIME =     35.00000000    

 PARAMETER _POSTTIME =     1.000000000    

 PARAMETER _TOTALTIM =     38.00000000    

 EXIT ANSYS WITHOUT SAVING DATABASE


 NUMBER OF WARNING MESSAGES ENCOUNTERED=          5
 NUMBER OF ERROR   MESSAGES ENCOUNTERED=          0

+--------- D I S T R I B U T E D   A N S Y S   S T A T I S T I C S ------------+

Release: Release 17.0       Build: 17.0       Update: UP20151214   Platform: WINDOWS x64 
Date Run: 06/15/2019   Time: 11:41
Operating System: Windows 10  (Build: 17134)
Windows Process ID: 14960       

Processor Model: Intel(R) Core(TM) i7-6700HQ CPU @ 2.60GHz

Compiler: Intel(R) FORTRAN Compiler Version 15.0.2  (Build: 20150121)
          Intel(R) C/C++ Compiler Version 15.0.2  (Build: 20150121)
          Intel(R) Math Kernel Library Version 11.2.3 Product Build 20150413

Number of machines requested            :    1
Total number of cores available         :    8
Number of physical cores available      :    4
Number of processes requested           :    2
Number of threads per process requested :    1
Total number of cores requested         :    2 (Distributed Memory Parallel)               
MPI Type: INTELMPI
MPI Version: Intel(R) MPI Library 5.0 Update 3 for Windows* OS


GPU Acceleration: Not Requested

Job Name: file0
Input File: dummy.dat

  Core                Machine Name   Working Directory
  ----------------------------------------------------
     0                         MSI   C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScratch\Scr48FB
     1                         MSI   C:\Users\Eduardo\AppData\Local\Temp\WB_MSI_Eduardo_4224_2\_ProjectScratch\Scr48FB
 
Latency time from master to core    1 =    3.800 microseconds
 
Communication speed from master to core    1 =  3353.83 MB/sec

Total CPU time for main thread                    :       39.2 seconds
Total CPU time summed for all threads             :       43.8 seconds

Elapsed time spent pre-processing model (/PREP7)  :        2.6 seconds
Elapsed time spent solution - preprocessing       :        5.7 seconds
Elapsed time spent computing solution             :       27.4 seconds
Elapsed time spent solution - postprocessing      :        1.0 seconds
Elapsed time spent post-processing model (/POST1) :        0.0 seconds
 
Equation solver used                              :            Sparse (symmetric)
Equation solver computational rate                :    15881.9 Mflops
Equation solver effective I/O rate                :     8597.2 MB/sec

Maximum total memory used                         :     3678.0 MB
Maximum total memory allocated                    :     4884.0 MB
Maximum total memory available                    :         16 GB

+------ E N D   D I S T R I B U T E D   A N S Y S   S T A T I S T I C S -------+


 *---------------------------------------------------------------------------*
 |                                                                           |
 |                       DISTRIBUTED ANSYS RUN COMPLETED                     |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Ansys Release 17.0          Build 17.0         UP20151214     WINDOWS x64 |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 | Database Requested(-db)  1024 MB    Scratch Memory Requested      1024 MB |
 | Maximum Database Used     198 MB    Maximum Scratch Memory Used   1779 MB |
 |                                                                           |
 |---------------------------------------------------------------------------|
 |                                                                           |
 |        CP Time      (sec) =         43.828       Time  =  11:41:51        |
 |        Elapsed Time (sec) =         41.000       Date  =  06/15/2019      |
 |                                                                           |
 *---------------------------------------------------------------------------*
