/COM,ANSYS RELEASE Release 17.0      BUILD 17.0      UP20151214       11:41:11

 *** WARNING ***                         CP =       6.047   TIME= 11:41:15
 Using 1 iteration per substep may result in unconverged solutions for   
 nonlinear analysis and the program may not indicate divergence in this  
 case.  Check your results.                                              

 *** WARNING ***                         CP =       6.484   TIME= 11:41:16
 Element shape checking is currently inactive.  Issue SHPP,ON or         
 SHPP,WARN to reactivate, if desired.                                    

 *** WARNING ***                         CP =       7.422   TIME= 11:41:16
 Material number 277 (used by element 116577 ) should normally have at   
 least one MP or one TB type command associated with it.  Output of      
 energy by material may not be available.                                

 *** WARNING ***                         CP =      23.625   TIME= 11:41:30
 Coefficient ratio exceeds 1.0e8 - Check results.                        

 *** WARNING ***                         CP =      40.375   TIME= 11:41:47
 Contact element 98263 (real ID 113) status changes abruptly from        
 contact (with target element 98339) -> no-contact.                      
