Fitter report for Proyecto
Sat Jun 29 12:54:19 2013
Quartus II 32-bit Version 12.0 Build 263 08/02/2012 Service Pack 2 SJ Web Edition


---------------------
; Table of Contents ;
---------------------
  1. Legal Notice
  2. Fitter Summary
  3. Fitter Settings
  4. Parallel Compilation
  5. I/O Assignment Warnings
  6. Fitter Netlist Optimizations
  7. Incremental Compilation Preservation Summary
  8. Incremental Compilation Partition Settings
  9. Incremental Compilation Placement Preservation
 10. Pin-Out File
 11. Fitter Resource Usage Summary
 12. Fitter Partition Statistics
 13. Input Pins
 14. Output Pins
 15. Dual Purpose and Dedicated Pins
 16. I/O Bank Usage
 17. All Package Pins
 18. Fitter Resource Utilization by Entity
 19. Delay Chain Summary
 20. Pad To Core Delay Chain Fanout
 21. Control Signals
 22. Global & Other Fast Signals
 23. Non-Global High Fan-Out Signals
 24. Fitter DSP Block Usage Summary
 25. DSP Block Details
 26. Interconnect Usage Summary
 27. LAB Logic Elements
 28. LAB-wide Signals
 29. LAB Signals Sourced
 30. LAB Signals Sourced Out
 31. LAB Distinct Inputs
 32. I/O Rules Summary
 33. I/O Rules Details
 34. I/O Rules Matrix
 35. Fitter Device Options
 36. Operating Settings and Conditions
 37. Estimated Delay Added for Hold Timing Summary
 38. Estimated Delay Added for Hold Timing Details
 39. Fitter Messages



----------------
; Legal Notice ;
----------------
Copyright (C) 1991-2012 Altera Corporation
Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and its AMPP partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, Altera MegaCore Function License 
Agreement, or other applicable license agreement, including, 
without limitation, that your use is for the sole purpose of 
programming logic devices manufactured by Altera and sold by 
Altera or its authorized distributors.  Please refer to the 
applicable agreement for further details.



+------------------------------------------------------------------------------------+
; Fitter Summary                                                                     ;
+------------------------------------+-----------------------------------------------+
; Fitter Status                      ; Successful - Sat Jun 29 12:54:18 2013         ;
; Quartus II 32-bit Version          ; 12.0 Build 263 08/02/2012 SP 2 SJ Web Edition ;
; Revision Name                      ; Proyecto                                      ;
; Top-level Entity Name              ; proyecto                                      ;
; Family                             ; Cyclone IV E                                  ;
; Device                             ; EP4CE115F29C7                                 ;
; Timing Models                      ; Final                                         ;
; Total logic elements               ; 7,551 / 114,480 ( 7 % )                       ;
;     Total combinational functions  ; 6,856 / 114,480 ( 6 % )                       ;
;     Dedicated logic registers      ; 3,087 / 114,480 ( 3 % )                       ;
; Total registers                    ; 3087                                          ;
; Total pins                         ; 57 / 529 ( 11 % )                             ;
; Total virtual pins                 ; 0                                             ;
; Total memory bits                  ; 0 / 3,981,312 ( 0 % )                         ;
; Embedded Multiplier 9-bit elements ; 20 / 532 ( 4 % )                              ;
; Total PLLs                         ; 0 / 4 ( 0 % )                                 ;
+------------------------------------+-----------------------------------------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Settings                                                                                                                                            ;
+----------------------------------------------------------------------------+---------------------------------------+---------------------------------------+
; Option                                                                     ; Setting                               ; Default Value                         ;
+----------------------------------------------------------------------------+---------------------------------------+---------------------------------------+
; Device                                                                     ; EP4CE115F29C7                         ;                                       ;
; Nominal Core Supply Voltage                                                ; 1.2V                                  ;                                       ;
; Minimum Core Junction Temperature                                          ; 0                                     ;                                       ;
; Maximum Core Junction Temperature                                          ; 85                                    ;                                       ;
; Fit Attempts to Skip                                                       ; 0                                     ; 0.0                                   ;
; Device I/O Standard                                                        ; 2.5 V                                 ;                                       ;
; Use smart compilation                                                      ; Off                                   ; Off                                   ;
; Enable parallel Assembler and TimeQuest Timing Analyzer during compilation ; On                                    ; On                                    ;
; Enable compact report table                                                ; Off                                   ; Off                                   ;
; Auto Merge PLLs                                                            ; On                                    ; On                                    ;
; Router Timing Optimization Level                                           ; Normal                                ; Normal                                ;
; Perform Clocking Topology Analysis During Routing                          ; Off                                   ; Off                                   ;
; Placement Effort Multiplier                                                ; 1.0                                   ; 1.0                                   ;
; Router Effort Multiplier                                                   ; 1.0                                   ; 1.0                                   ;
; Optimize Hold Timing                                                       ; All Paths                             ; All Paths                             ;
; Optimize Multi-Corner Timing                                               ; On                                    ; On                                    ;
; PowerPlay Power Optimization                                               ; Normal compilation                    ; Normal compilation                    ;
; SSN Optimization                                                           ; Off                                   ; Off                                   ;
; Optimize Timing                                                            ; Normal compilation                    ; Normal compilation                    ;
; Optimize Timing for ECOs                                                   ; Off                                   ; Off                                   ;
; Regenerate full fit report during ECO compiles                             ; Off                                   ; Off                                   ;
; Optimize IOC Register Placement for Timing                                 ; Normal                                ; Normal                                ;
; Limit to One Fitting Attempt                                               ; Off                                   ; Off                                   ;
; Final Placement Optimizations                                              ; Automatically                         ; Automatically                         ;
; Fitter Aggressive Routability Optimizations                                ; Automatically                         ; Automatically                         ;
; Fitter Initial Placement Seed                                              ; 1                                     ; 1                                     ;
; PCI I/O                                                                    ; Off                                   ; Off                                   ;
; Weak Pull-Up Resistor                                                      ; Off                                   ; Off                                   ;
; Enable Bus-Hold Circuitry                                                  ; Off                                   ; Off                                   ;
; Auto Packed Registers                                                      ; Auto                                  ; Auto                                  ;
; Auto Delay Chains                                                          ; On                                    ; On                                    ;
; Allow Single-ended Buffer for Differential-XSTL Input                      ; Off                                   ; Off                                   ;
; Treat Bidirectional Pin as Output Pin                                      ; Off                                   ; Off                                   ;
; Perform Physical Synthesis for Combinational Logic for Fitting             ; Off                                   ; Off                                   ;
; Perform Physical Synthesis for Combinational Logic for Performance         ; Off                                   ; Off                                   ;
; Perform Register Duplication for Performance                               ; Off                                   ; Off                                   ;
; Perform Logic to Memory Mapping for Fitting                                ; Off                                   ; Off                                   ;
; Perform Register Retiming for Performance                                  ; Off                                   ; Off                                   ;
; Perform Asynchronous Signal Pipelining                                     ; Off                                   ; Off                                   ;
; Fitter Effort                                                              ; Auto Fit                              ; Auto Fit                              ;
; Physical Synthesis Effort Level                                            ; Normal                                ; Normal                                ;
; Logic Cell Insertion - Logic Duplication                                   ; Auto                                  ; Auto                                  ;
; Auto Register Duplication                                                  ; Auto                                  ; Auto                                  ;
; Auto Global Clock                                                          ; On                                    ; On                                    ;
; Auto Global Register Control Signals                                       ; On                                    ; On                                    ;
; Reserve all unused pins                                                    ; As input tri-stated with weak pull-up ; As input tri-stated with weak pull-up ;
; Synchronizer Identification                                                ; Off                                   ; Off                                   ;
; Enable Beneficial Skew Optimization                                        ; On                                    ; On                                    ;
; Optimize Design for Metastability                                          ; On                                    ; On                                    ;
; Force Fitter to Avoid Periphery Placement Warnings                         ; Off                                   ; Off                                   ;
; Enable input tri-state on active configuration pins in user mode           ; Off                                   ; Off                                   ;
+----------------------------------------------------------------------------+---------------------------------------+---------------------------------------+


Parallel compilation was disabled, but you have multiple processors available. Enable parallel compilation to reduce compilation time.
+-------------------------------------+
; Parallel Compilation                ;
+----------------------------+--------+
; Processors                 ; Number ;
+----------------------------+--------+
; Number detected on machine ; 2      ;
; Maximum allowed            ; 1      ;
+----------------------------+--------+


+------------------------------------------------------+
; I/O Assignment Warnings                              ;
+---------------+--------------------------------------+
; Pin Name      ; Reason                               ;
+---------------+--------------------------------------+
; LED_config[0] ; Missing drive strength and slew rate ;
; LED_config[1] ; Missing drive strength and slew rate ;
; LED_config[2] ; Missing drive strength and slew rate ;
; LED_modo      ; Missing drive strength and slew rate ;
; LED_inst[0]   ; Missing drive strength and slew rate ;
; LED_inst[1]   ; Missing drive strength and slew rate ;
; sal_LED[0]    ; Missing drive strength and slew rate ;
; sal_LED[1]    ; Missing drive strength and slew rate ;
; sal_LED[2]    ; Missing drive strength and slew rate ;
; sal_LED[3]    ; Missing drive strength and slew rate ;
; sal_LED[4]    ; Missing drive strength and slew rate ;
; sal_LED[5]    ; Missing drive strength and slew rate ;
; sal_LED[6]    ; Missing drive strength and slew rate ;
; sal_LED[7]    ; Missing drive strength and slew rate ;
; sal_LED[8]    ; Missing drive strength and slew rate ;
; sal_LED[9]    ; Missing drive strength and slew rate ;
; sal_LED[10]   ; Missing drive strength and slew rate ;
; sal_LED[11]   ; Missing drive strength and slew rate ;
; pulse_48KHz   ; Missing drive strength and slew rate ;
; AUD_MCLK      ; Missing drive strength and slew rate ;
; AUD_BCLK      ; Missing drive strength and slew rate ;
; AUD_DACDAT    ; Missing drive strength and slew rate ;
; AUD_DACLRCK   ; Missing drive strength and slew rate ;
; I2C_SDAT      ; Missing drive strength and slew rate ;
; I2C_SCLK      ; Missing drive strength and slew rate ;
+---------------+--------------------------------------+


+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Netlist Optimizations                                                                                                                                                                                    ;
+------------------+-----------------+------------------+---------------------+-----------+----------------+-----------------------------------------------------------+------------------+-----------------------+
; Node             ; Action          ; Operation        ; Reason              ; Node Port ; Node Port Name ; Destination Node                                          ; Destination Port ; Destination Port Name ;
+------------------+-----------------+------------------+---------------------+-----------+----------------+-----------------------------------------------------------+------------------+-----------------------+
; FF2:U17|B1_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B1_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B2_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B3_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B4_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B5_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B6_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B7_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B8_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|B9_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U17|Bf_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B1_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B2_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B3_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B4_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B5_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B6_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B7_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B8_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|B9_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[0] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[1] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[2] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[3] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[4] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[5] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[6] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
; FF2:U34|Bf_FF[7] ; Packed Register ; Register Packing ; Timing optimization ; Q         ;                ; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ; DATAA            ;                       ;
+------------------+-----------------+------------------+---------------------+-----------+----------------+-----------------------------------------------------------+------------------+-----------------------+


+----------------------------------------------+
; Incremental Compilation Preservation Summary ;
+---------------------+------------------------+
; Type                ; Value                  ;
+---------------------+------------------------+
; Placement (by node) ;                        ;
;     -- Requested    ; 0 / 10271 ( 0.00 % )   ;
;     -- Achieved     ; 0 / 10271 ( 0.00 % )   ;
;                     ;                        ;
; Routing (by net)    ;                        ;
;     -- Requested    ; 0 / 0 ( 0.00 % )       ;
;     -- Achieved     ; 0 / 0 ( 0.00 % )       ;
+---------------------+------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Incremental Compilation Partition Settings                                                                                                                                             ;
+--------------------------------+----------------+-------------------+-------------------------+------------------------+------------------------------+--------------------------------+
; Partition Name                 ; Partition Type ; Netlist Type Used ; Preservation Level Used ; Netlist Type Requested ; Preservation Level Requested ; Contents                       ;
+--------------------------------+----------------+-------------------+-------------------------+------------------------+------------------------------+--------------------------------+
; Top                            ; User-created   ; Source File       ; N/A                     ; Source File            ; N/A                          ;                                ;
; hard_block:auto_generated_inst ; Auto-generated ; Source File       ; N/A                     ; Source File            ; N/A                          ; hard_block:auto_generated_inst ;
+--------------------------------+----------------+-------------------+-------------------------+------------------------+------------------------------+--------------------------------+


+------------------------------------------------------------------------------------------------------------+
; Incremental Compilation Placement Preservation                                                             ;
+--------------------------------+---------+-------------------+-------------------------+-------------------+
; Partition Name                 ; # Nodes ; # Preserved Nodes ; Preservation Level Used ; Netlist Type Used ;
+--------------------------------+---------+-------------------+-------------------------+-------------------+
; Top                            ; 10261   ; 0                 ; N/A                     ; Source File       ;
; hard_block:auto_generated_inst ; 10      ; 0                 ; N/A                     ; Source File       ;
+--------------------------------+---------+-------------------+-------------------------+-------------------+


+--------------+
; Pin-Out File ;
+--------------+
The pin-out file can be found in C:/Documents and Settings/Usuario/Escritorio/arpa_bien/Proyecto_altera/Proyecto.pin.


+------------------------------------------------------------------------+
; Fitter Resource Usage Summary                                          ;
+---------------------------------------------+--------------------------+
; Resource                                    ; Usage                    ;
+---------------------------------------------+--------------------------+
; Total logic elements                        ; 7,551 / 114,480 ( 7 % )  ;
;     -- Combinational with no register       ; 4464                     ;
;     -- Register only                        ; 695                      ;
;     -- Combinational with a register        ; 2392                     ;
;                                             ;                          ;
; Logic element usage by number of LUT inputs ;                          ;
;     -- 4 input functions                    ; 2400                     ;
;     -- 3 input functions                    ; 3039                     ;
;     -- <=2 input functions                  ; 1417                     ;
;     -- Register only                        ; 695                      ;
;                                             ;                          ;
; Logic elements by mode                      ;                          ;
;     -- normal mode                          ; 3845                     ;
;     -- arithmetic mode                      ; 3011                     ;
;                                             ;                          ;
; Total registers*                            ; 3,087 / 117,053 ( 3 % )  ;
;     -- Dedicated logic registers            ; 3,087 / 114,480 ( 3 % )  ;
;     -- I/O registers                        ; 0 / 2,573 ( 0 % )        ;
;                                             ;                          ;
; Total LABs:  partially or completely used   ; 577 / 7,155 ( 8 % )      ;
; User inserted logic elements                ; 0                        ;
; Virtual pins                                ; 0                        ;
; I/O pins                                    ; 57 / 529 ( 11 % )        ;
;     -- Clock pins                           ; 1 / 7 ( 14 % )           ;
;     -- Dedicated input pins                 ; 0 / 9 ( 0 % )            ;
;                                             ;                          ;
; Global signals                              ; 4                        ;
; M9Ks                                        ; 0 / 432 ( 0 % )          ;
; Total block memory bits                     ; 0 / 3,981,312 ( 0 % )    ;
; Total block memory implementation bits      ; 0 / 3,981,312 ( 0 % )    ;
; Embedded Multiplier 9-bit elements          ; 20 / 532 ( 4 % )         ;
; PLLs                                        ; 0 / 4 ( 0 % )            ;
; Global clocks                               ; 4 / 20 ( 20 % )          ;
; JTAGs                                       ; 0 / 1 ( 0 % )            ;
; CRC blocks                                  ; 0 / 1 ( 0 % )            ;
; ASMI blocks                                 ; 0 / 1 ( 0 % )            ;
; Impedance control blocks                    ; 0 / 4 ( 0 % )            ;
; Average interconnect usage (total/H/V)      ; 2% / 2% / 2%             ;
; Peak interconnect usage (total/H/V)         ; 26% / 28% / 26%          ;
; Maximum fan-out node                        ; divisor1:U1|sint~clkctrl ;
; Maximum fan-out                             ; 2464                     ;
; Highest non-global fan-out signal           ; RST~input                ;
; Highest non-global fan-out                  ; 1123                     ;
; Total fan-out                               ; 31795                    ;
; Average fan-out                             ; 2.94                     ;
+---------------------------------------------+--------------------------+
*  Register count does not include registers inside RAM blocks or DSP blocks.



+------------------------------------------------------------------------------------------------------+
; Fitter Partition Statistics                                                                          ;
+---------------------------------------------+-----------------------+--------------------------------+
; Statistic                                   ; Top                   ; hard_block:auto_generated_inst ;
+---------------------------------------------+-----------------------+--------------------------------+
; Difficulty Clustering Region                ; Low                   ; Low                            ;
;                                             ;                       ;                                ;
; Total logic elements                        ; 7551 / 114480 ( 7 % ) ; 0 / 114480 ( 0 % )             ;
;     -- Combinational with no register       ; 4464                  ; 0                              ;
;     -- Register only                        ; 695                   ; 0                              ;
;     -- Combinational with a register        ; 2392                  ; 0                              ;
;                                             ;                       ;                                ;
; Logic element usage by number of LUT inputs ;                       ;                                ;
;     -- 4 input functions                    ; 2400                  ; 0                              ;
;     -- 3 input functions                    ; 3039                  ; 0                              ;
;     -- <=2 input functions                  ; 1417                  ; 0                              ;
;     -- Register only                        ; 695                   ; 0                              ;
;                                             ;                       ;                                ;
; Logic elements by mode                      ;                       ;                                ;
;     -- normal mode                          ; 3845                  ; 0                              ;
;     -- arithmetic mode                      ; 3011                  ; 0                              ;
;                                             ;                       ;                                ;
; Total registers                             ; 3087                  ; 0                              ;
;     -- Dedicated logic registers            ; 3087 / 114480 ( 3 % ) ; 0 / 114480 ( 0 % )             ;
;     -- I/O registers                        ; 0                     ; 0                              ;
;                                             ;                       ;                                ;
; Total LABs:  partially or completely used   ; 577 / 7155 ( 8 % )    ; 0 / 7155 ( 0 % )               ;
;                                             ;                       ;                                ;
; Virtual pins                                ; 0                     ; 0                              ;
; I/O pins                                    ; 57                    ; 0                              ;
; Embedded Multiplier 9-bit elements          ; 20 / 532 ( 4 % )      ; 0 / 532 ( 0 % )                ;
; Total memory bits                           ; 0                     ; 0                              ;
; Total RAM block bits                        ; 0                     ; 0                              ;
; Clock control block                         ; 4 / 24 ( 16 % )       ; 0 / 24 ( 0 % )                 ;
;                                             ;                       ;                                ;
; Connections                                 ;                       ;                                ;
;     -- Input Connections                    ; 0                     ; 0                              ;
;     -- Registered Input Connections         ; 0                     ; 0                              ;
;     -- Output Connections                   ; 0                     ; 0                              ;
;     -- Registered Output Connections        ; 0                     ; 0                              ;
;                                             ;                       ;                                ;
; Internal Connections                        ;                       ;                                ;
;     -- Total Connections                    ; 32130                 ; 5                              ;
;     -- Registered Connections               ; 12674                 ; 0                              ;
;                                             ;                       ;                                ;
; External Connections                        ;                       ;                                ;
;     -- Top                                  ; 0                     ; 0                              ;
;     -- hard_block:auto_generated_inst       ; 0                     ; 0                              ;
;                                             ;                       ;                                ;
; Partition Interface                         ;                       ;                                ;
;     -- Input Ports                          ; 32                    ; 0                              ;
;     -- Output Ports                         ; 25                    ; 0                              ;
;     -- Bidir Ports                          ; 0                     ; 0                              ;
;                                             ;                       ;                                ;
; Registered Ports                            ;                       ;                                ;
;     -- Registered Input Ports               ; 0                     ; 0                              ;
;     -- Registered Output Ports              ; 0                     ; 0                              ;
;                                             ;                       ;                                ;
; Port Connectivity                           ;                       ;                                ;
;     -- Input Ports driven by GND            ; 0                     ; 0                              ;
;     -- Output Ports driven by GND           ; 0                     ; 0                              ;
;     -- Input Ports driven by VCC            ; 0                     ; 0                              ;
;     -- Output Ports driven by VCC           ; 0                     ; 0                              ;
;     -- Input Ports with no Source           ; 0                     ; 0                              ;
;     -- Output Ports with no Source          ; 0                     ; 0                              ;
;     -- Input Ports with no Fanout           ; 0                     ; 0                              ;
;     -- Output Ports with no Fanout          ; 0                     ; 0                              ;
+---------------------------------------------+-----------------------+--------------------------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Input Pins                                                                                                                                                                                                                                                                         ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+---------------------------+----------------------+
; Name          ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Z coordinate ; Combinational Fan-Out ; Registered Fan-Out ; Global ; Input Register ; Power Up High ; PCI I/O Enabled ; Bus Hold ; Weak Pull Up ; I/O Standard ; Termination Control Block ; Location assigned by ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+---------------------------+----------------------+
; CLK           ; Y2    ; 2        ; 0            ; 36           ; 14           ; 27                    ; 0                  ; yes    ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; INIT          ; Y23   ; 5        ; 115          ; 14           ; 7            ; 4                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; RST           ; AA22  ; 5        ; 115          ; 6            ; 14           ; 1123                  ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; W_EN          ; Y24   ; 5        ; 115          ; 13           ; 0            ; 2                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; en            ; R24   ; 5        ; 115          ; 35           ; 21           ; 11                    ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[0]      ; AB22  ; 4        ; 107          ; 0            ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[10]     ; AF22  ; 4        ; 96           ; 0            ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[11]     ; AG25  ; 4        ; 91           ; 0            ; 21           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[1]      ; AB21  ; 4        ; 109          ; 0            ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[2]      ; AC21  ; 4        ; 102          ; 0            ; 21           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[3]      ; AD21  ; 4        ; 102          ; 0            ; 14           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[4]      ; AD15  ; 4        ; 60           ; 0            ; 14           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[5]      ; AC19  ; 4        ; 94           ; 0            ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[6]      ; AD19  ; 4        ; 94           ; 0            ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[7]      ; AF24  ; 4        ; 83           ; 0            ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[8]      ; AF25  ; 4        ; 83           ; 0            ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas[9]      ; AE22  ; 4        ; 96           ; 0            ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[0]  ; AB24  ; 5        ; 115          ; 5            ; 14           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[10] ; AC28  ; 5        ; 115          ; 14           ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[11] ; AB28  ; 5        ; 115          ; 17           ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[1]  ; AC24  ; 5        ; 115          ; 4            ; 14           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[2]  ; AB25  ; 5        ; 115          ; 16           ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[3]  ; AC25  ; 5        ; 115          ; 4            ; 21           ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[4]  ; AB26  ; 5        ; 115          ; 15           ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[5]  ; AD26  ; 5        ; 115          ; 10           ; 0            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[6]  ; AC26  ; 5        ; 115          ; 11           ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[7]  ; AB27  ; 5        ; 115          ; 18           ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[8]  ; AD27  ; 5        ; 115          ; 13           ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; notas_int[9]  ; AC27  ; 5        ; 115          ; 15           ; 7            ; 1                     ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; num_inst[0]   ; AB23  ; 5        ; 115          ; 7            ; 14           ; 544                   ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; num_inst[1]   ; AA24  ; 5        ; 115          ; 9            ; 21           ; 571                   ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
; sel           ; AA23  ; 5        ; 115          ; 10           ; 7            ; 13                    ; 0                  ; no     ; no             ; no            ; yes             ; no       ; Off          ; 2.5 V        ; --                        ; User                 ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------------+--------------------+--------+----------------+---------------+-----------------+----------+--------------+--------------+---------------------------+----------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Output Pins                                                                                                                                                                                                                                                                                                                                                                                                                                                    ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------+------------------------+---------------+-----------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-----------------------------------+---------------------------+----------------------------+-----------------------------+----------------------+----------------------+---------------------+
; Name          ; Pin # ; I/O Bank ; X coordinate ; Y coordinate ; Z coordinate ; Output Register ; Output Enable Register ; Power Up High ; Slew Rate ; PCI I/O Enabled ; Open Drain ; TRI Primitive ; Bus Hold ; Weak Pull Up ; I/O Standard ; Current Strength ; Termination                       ; Termination Control Block ; Output Buffer Pre-emphasis ; Voltage Output Differential ; Location assigned by ; Output Enable Source ; Output Enable Group ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------+------------------------+---------------+-----------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-----------------------------------+---------------------------+----------------------------+-----------------------------+----------------------+----------------------+---------------------+
; AUD_BCLK      ; F2    ; 1        ; 0            ; 60           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; AUD_DACDAT    ; D1    ; 1        ; 0            ; 68           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; AUD_DACLRCK   ; E3    ; 1        ; 0            ; 66           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; AUD_MCLK      ; E1    ; 1        ; 0            ; 61           ; 21           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; I2C_SCLK      ; B7    ; 8        ; 29           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; I2C_SDAT      ; A8    ; 8        ; 18           ; 73           ; 21           ; no              ; no                     ; no            ; 2         ; yes             ; no         ; yes           ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_config[0] ; G15   ; 7        ; 65           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_config[1] ; G16   ; 7        ; 67           ; 73           ; 0            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_config[2] ; H15   ; 7        ; 60           ; 73           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_inst[0]   ; J16   ; 7        ; 65           ; 73           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_inst[1]   ; H17   ; 7        ; 67           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; LED_modo      ; F15   ; 7        ; 58           ; 73           ; 0            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; pulse_48KHz   ; M7    ; 1        ; 0            ; 45           ; 21           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; Fitter               ; -                    ; -                   ;
; sal_LED[0]    ; H16   ; 7        ; 65           ; 73           ; 21           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[10]   ; F19   ; 7        ; 94           ; 73           ; 0            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[11]   ; G19   ; 7        ; 69           ; 73           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[1]    ; J15   ; 7        ; 60           ; 73           ; 21           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[2]    ; G17   ; 7        ; 83           ; 73           ; 21           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[3]    ; J17   ; 7        ; 69           ; 73           ; 0            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[4]    ; H19   ; 7        ; 72           ; 73           ; 0            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[5]    ; J19   ; 7        ; 72           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[6]    ; E18   ; 7        ; 87           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[7]    ; F18   ; 7        ; 87           ; 73           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[8]    ; F21   ; 7        ; 107          ; 73           ; 14           ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
; sal_LED[9]    ; E19   ; 7        ; 94           ; 73           ; 7            ; no              ; no                     ; no            ; 2         ; no              ; no         ; no            ; no       ; Off          ; 2.5 V        ; Default          ; Series 50 Ohm without Calibration ; --                        ; no                         ; no                          ; User                 ; -                    ; -                   ;
+---------------+-------+----------+--------------+--------------+--------------+-----------------+------------------------+---------------+-----------+-----------------+------------+---------------+----------+--------------+--------------+------------------+-----------------------------------+---------------------------+----------------------------+-----------------------------+----------------------+----------------------+---------------------+


+-------------------------------------------------------------------------------------------------------------------------+
; Dual Purpose and Dedicated Pins                                                                                         ;
+----------+-----------------------------+--------------------------+-------------------------+---------------------------+
; Location ; Pin Name                    ; Reserved As              ; User Signal Name        ; Pin Type                  ;
+----------+-----------------------------+--------------------------+-------------------------+---------------------------+
; F4       ; DIFFIO_L5n, DATA1, ASDO     ; As input tri-stated      ; ~ALTERA_ASDO_DATA1~     ; Dual Purpose Pin          ;
; E2       ; DIFFIO_L8p, FLASH_nCE, nCSO ; As input tri-stated      ; ~ALTERA_FLASH_nCE_nCSO~ ; Dual Purpose Pin          ;
; M6       ; nSTATUS                     ; -                        ; -                       ; Dedicated Programming Pin ;
; P3       ; DCLK                        ; As output driving ground ; ~ALTERA_DCLK~           ; Dual Purpose Pin          ;
; N7       ; DATA0                       ; As input tri-stated      ; ~ALTERA_DATA0~          ; Dual Purpose Pin          ;
; P4       ; nCONFIG                     ; -                        ; -                       ; Dedicated Programming Pin ;
; R8       ; nCE                         ; -                        ; -                       ; Dedicated Programming Pin ;
; P24      ; CONF_DONE                   ; -                        ; -                       ; Dedicated Programming Pin ;
; N22      ; MSEL0                       ; -                        ; -                       ; Dedicated Programming Pin ;
; P23      ; MSEL1                       ; -                        ; -                       ; Dedicated Programming Pin ;
; M22      ; MSEL2                       ; -                        ; -                       ; Dedicated Programming Pin ;
; P22      ; MSEL3                       ; -                        ; -                       ; Dedicated Programming Pin ;
; P28      ; DIFFIO_R23n, nCEO           ; Use as programming pin   ; ~ALTERA_nCEO~           ; Dual Purpose Pin          ;
; B7       ; DIFFIO_T18p, DATA5          ; Use as regular IO        ; I2C_SCLK                ; Dual Purpose Pin          ;
; A8       ; DIFFIO_T11n, DATA9          ; Use as regular IO        ; I2C_SDAT                ; Dual Purpose Pin          ;
+----------+-----------------------------+--------------------------+-------------------------+---------------------------+


+------------------------------------------------------------+
; I/O Bank Usage                                             ;
+----------+------------------+---------------+--------------+
; I/O Bank ; Usage            ; VCCIO Voltage ; VREF Voltage ;
+----------+------------------+---------------+--------------+
; 1        ; 9 / 56 ( 16 % )  ; 2.5V          ; --           ;
; 2        ; 1 / 63 ( 2 % )   ; 2.5V          ; --           ;
; 3        ; 0 / 73 ( 0 % )   ; 2.5V          ; --           ;
; 4        ; 12 / 71 ( 17 % ) ; 2.5V          ; --           ;
; 5        ; 19 / 65 ( 29 % ) ; 2.5V          ; --           ;
; 6        ; 1 / 58 ( 2 % )   ; 2.5V          ; --           ;
; 7        ; 18 / 72 ( 25 % ) ; 2.5V          ; --           ;
; 8        ; 2 / 71 ( 3 % )   ; 2.5V          ; --           ;
+----------+------------------+---------------+--------------+


+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; All Package Pins                                                                                                                                                                        ;
+----------+------------+----------+-----------------------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; Location ; Pad Number ; I/O Bank ; Pin Name/Usage                                            ; Dir.   ; I/O Standard ; Voltage ; I/O Type   ; User Assignment ; Bus Hold ; Weak Pull Up ;
+----------+------------+----------+-----------------------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
; A2       ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A3       ; 535        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A4       ; 532        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A5       ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A6       ; 504        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A7       ; 501        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A8       ; 517        ; 8        ; I2C_SDAT                                                  ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; A9       ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A10      ; 491        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A11      ; 487        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A12      ; 482        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A13      ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A14      ; 472        ; 8        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; A15      ; 470        ; 7        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; A16      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A17      ; 462        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A18      ; 442        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A19      ; 440        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A20      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A21      ; 425        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A22      ; 423        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A23      ; 412        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A24      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; A25      ; 405        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A26      ; 404        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; A27      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AA1      ;            ; 2        ; VCCIO2                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AA2      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA3      ; 102        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA4      ; 101        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA5      ; 119        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA6      ; 118        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA7      ; 120        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA8      ; 154        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA9      ;            ;          ; GNDA1                                                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA10     ; 155        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA11     ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AA12     ; 188        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA13     ; 190        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA14     ; 191        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA15     ; 213        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA16     ; 211        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA17     ; 241        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA18     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AA19     ; 264        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA20     ;            ;          ; GNDA4                                                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA21     ; 269        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AA22     ; 275        ; 5        ; RST                                                       ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AA23     ; 280        ; 5        ; sel                                                       ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AA24     ; 279        ; 5        ; num_inst[1]                                               ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AA25     ; 294        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA26     ; 293        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AA27     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AA28     ;            ; 5        ; VCCIO5                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AB1      ; 86         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB2      ; 85         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB3      ; 99         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB4      ; 121        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB5      ; 127        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB6      ; 126        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AB7      ; 152        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB8      ; 148        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB9      ; 147        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB10     ; 173        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB11     ; 164        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB12     ; 180        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB13     ; 181        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB14     ; 192        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB15     ; 214        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB16     ; 212        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB17     ; 242        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB18     ; 254        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB19     ; 253        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB20     ; 257        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AB21     ; 266        ; 4        ; notas[1]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AB22     ; 265        ; 4        ; notas[0]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AB23     ; 276        ; 5        ; num_inst[0]                                               ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AB24     ; 274        ; 5        ; notas_int[0]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AB25     ; 292        ; 5        ; notas_int[2]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AB26     ; 291        ; 5        ; notas_int[4]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AB27     ; 296        ; 5        ; notas_int[7]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AB28     ; 295        ; 5        ; notas_int[11]                                             ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AC1      ; 94         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AC2      ; 93         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AC3      ; 95         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AC4      ; 125        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AC5      ; 124        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AC6      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC7      ; 144        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC8      ; 153        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC9      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC10     ; 174        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC11     ; 185        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC12     ; 179        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC13     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC14     ; 195        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC15     ; 203        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC16     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC17     ; 221        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC18     ; 240        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC19     ; 247        ; 4        ; notas[5]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AC20     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC21     ; 258        ; 4        ; notas[2]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AC22     ; 267        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AC23     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AC24     ; 273        ; 5        ; notas_int[1]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AC25     ; 272        ; 5        ; notas_int[3]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AC26     ; 282        ; 5        ; notas_int[6]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AC27     ; 290        ; 5        ; notas_int[9]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AC28     ; 289        ; 5        ; notas_int[10]                                             ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AD1      ; 98         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AD2      ; 97         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AD3      ; 96         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AD4      ; 130        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD5      ; 128        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD6      ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD7      ; 134        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD8      ; 143        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD9      ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD10     ; 149        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD11     ; 186        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD12     ; 182        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD13     ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD14     ; 196        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD15     ; 204        ; 4        ; notas[4]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AD16     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD17     ; 222        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD18     ; 237        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD19     ; 248        ; 4        ; notas[6]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AD20     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD21     ; 259        ; 4        ; notas[3]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AD22     ; 268        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD23     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AD24     ; 260        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD25     ; 255        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AD26     ; 281        ; 5        ; notas_int[5]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AD27     ; 286        ; 5        ; notas_int[8]                                              ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; AD28     ; 285        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE1      ; 106        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE2      ; 105        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE3      ; 122        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE4      ; 132        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE5      ; 135        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE6      ; 129        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE7      ; 158        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE8      ; 161        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE9      ; 163        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE10     ; 165        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE11     ; 171        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE12     ; 169        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE13     ; 177        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE14     ; 183        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE15     ; 205        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE16     ; 209        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE17     ; 215        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE18     ; 225        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE19     ; 231        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE20     ; 235        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE21     ; 238        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE22     ; 251        ; 4        ; notas[9]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AE23     ; 261        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE24     ; 256        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE25     ; 243        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AE26     ; 278        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE27     ; 284        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AE28     ; 283        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AF1      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AF2      ; 123        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AF3      ; 138        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF4      ; 131        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF5      ; 136        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF6      ; 139        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF7      ; 159        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF8      ; 162        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF9      ; 160        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF10     ; 166        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF11     ; 172        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF12     ; 170        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF13     ; 178        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF14     ; 184        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF15     ; 206        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF16     ; 210        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF17     ; 216        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF18     ; 226        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF19     ; 232        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF20     ; 236        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF21     ; 239        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF22     ; 252        ; 4        ; notas[10]                                                 ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AF23     ; 262        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF24     ; 233        ; 4        ; notas[7]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AF25     ; 234        ; 4        ; notas[8]                                                  ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AF26     ; 244        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AF27     ; 277        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; AF28     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG1      ;            ; 2        ; VCCIO2                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AG2      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG3      ; 133        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG4      ; 141        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG5      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG6      ; 145        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG7      ; 150        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG8      ; 156        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG9      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG10     ; 167        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG11     ; 175        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG12     ; 193        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG13     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG14     ; 199        ; 3        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; AG15     ; 201        ; 4        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; AG16     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG17     ; 207        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG18     ; 217        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG19     ; 219        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG20     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG21     ; 223        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG22     ; 227        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG23     ; 229        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG24     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG25     ; 245        ; 4        ; notas[11]                                                 ; input  ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; AG26     ; 270        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AG27     ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; AG28     ;            ; 5        ; VCCIO5                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH2      ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH3      ; 137        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH4      ; 142        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH5      ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH6      ; 146        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH7      ; 151        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH8      ; 157        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH9      ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH10     ; 168        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH11     ; 176        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH12     ; 194        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH13     ;            ; 3        ; VCCIO3                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH14     ; 200        ; 3        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; AH15     ; 202        ; 4        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; AH16     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH17     ; 208        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH18     ; 218        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH19     ; 220        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH20     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH21     ; 224        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH22     ; 228        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH23     ; 230        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH24     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; AH25     ; 246        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH26     ; 271        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; AH27     ;            ; 4        ; VCCIO4                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; B1       ;            ; 1        ; VCCIO1                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; B2       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B3       ; 534        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B4       ; 533        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B5       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B6       ; 505        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B7       ; 502        ; 8        ; I2C_SCLK                                                  ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; B8       ; 518        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B10      ; 492        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B11      ; 488        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B14      ; 473        ; 8        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; B15      ; 471        ; 7        ; GND+                                                      ;        ;              ;         ; Column I/O ;                 ; --       ; --           ;
; B16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B17      ; 463        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B18      ; 443        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B19      ; 441        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B21      ; 426        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B22      ; 424        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B23      ; 413        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B24      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B25      ; 406        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B26      ; 401        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; B27      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; B28      ;            ; 6        ; VCCIO6                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; C1       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; C2       ; 1          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; C3       ; 543        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C4       ; 539        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C5       ; 538        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C6       ; 536        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C7       ; 521        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C8       ; 519        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C9       ; 510        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C10      ; 495        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C11      ; 508        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C12      ; 478        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C13      ; 474        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C14      ; 476        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C15      ; 468        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C16      ; 460        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C17      ; 438        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C18      ; 429        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C19      ; 435        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C20      ; 431        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C21      ; 422        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C22      ; 418        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C23      ; 415        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C24      ; 416        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C25      ; 411        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C26      ; 400        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; C27      ; 382        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; C28      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; D1       ; 3          ; 1        ; AUD_DACDAT                                                ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; D2       ; 2          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; D3       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; D4       ; 540        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D5       ; 537        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D6       ; 524        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D7       ; 522        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D8       ; 520        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D9       ; 511        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D10      ; 496        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D11      ; 509        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D12      ; 479        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D13      ; 475        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D14      ; 477        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D15      ; 469        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D16      ; 461        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D17      ; 439        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D18      ; 430        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D19      ; 436        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D20      ; 432        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D21      ; 419        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D22      ; 402        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D23      ; 414        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D24      ; 417        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D25      ; 410        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; D26      ; 383        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; D27      ; 381        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; D28      ; 380        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; E1       ; 17         ; 1        ; AUD_MCLK                                                  ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E2       ; 16         ; 1        ; ~ALTERA_FLASH_nCE_nCSO~ / RESERVED_INPUT_WITH_WEAK_PULLUP ; input  ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; On           ;
; E3       ; 7          ; 1        ; AUD_DACLRCK                                               ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; E4       ; 541        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E5       ; 542        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E6       ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E7       ; 523        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E8       ; 526        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E9       ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E10      ; 516        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E11      ; 499        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E12      ; 497        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E13      ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E14      ; 486        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E15      ; 467        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E16      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E17      ; 456        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E18      ; 427        ; 7        ; sal_LED[6]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; E19      ; 421        ; 7        ; sal_LED[9]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; E20      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E21      ; 407        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E22      ; 403        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E23      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; E24      ; 433        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E25      ; 434        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; E26      ; 378        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; E27      ; 375        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; E28      ; 374        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F1       ; 19         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F2       ; 18         ; 1        ; AUD_BCLK                                                  ; output ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; F3       ; 8          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F4       ; 10         ; 1        ; ~ALTERA_ASDO_DATA1~ / RESERVED_INPUT_WITH_WEAK_PULLUP     ; input  ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; On           ;
; F5       ; 9          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F6       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F7       ; 531        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F8       ; 527        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F10      ; 512        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F11      ; 500        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F12      ; 498        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F14      ; 485        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F15      ; 466        ; 7        ; LED_modo                                                  ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; F16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F17      ; 455        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F18      ; 428        ; 7        ; sal_LED[7]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; F19      ; 420        ; 7        ; sal_LED[10]                                               ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; F20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F21      ; 408        ; 7        ; sal_LED[8]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; F22      ; 409        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; F23      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; F24      ; 396        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F25      ; 395        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F26      ; 379        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F27      ; 373        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; F28      ; 372        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G1       ; 26         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G2       ; 25         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G3       ; 13         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G4       ; 12         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G5       ; 6          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G6       ; 5          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G7       ; 530        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G8       ; 528        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G9       ; 525        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G10      ; 513        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G11      ; 506        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G12      ; 503        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G13      ; 493        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G14      ; 484        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G15      ; 457        ; 7        ; LED_config[0]                                             ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; G16      ; 453        ; 7        ; LED_config[1]                                             ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; G17      ; 437        ; 7        ; sal_LED[2]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; G18      ; 452        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G19      ; 451        ; 7        ; sal_LED[11]                                               ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; G20      ; 444        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G21      ; 445        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G22      ; 449        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; G23      ; 398        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G24      ; 397        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G25      ; 393        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G26      ; 392        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G27      ; 367        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; G28      ; 366        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H1       ;            ; 1        ; VCCIO1                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; H2       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; H3       ; 15         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H4       ; 14         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H5       ; 20         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H6       ; 11         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H7       ; 4          ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H8       ; 529        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H9       ;            ;          ; GNDA3                                                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; H10      ; 514        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H11      ;            ; 8        ; VCCIO8                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; H12      ; 507        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H13      ; 494        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H14      ; 480        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H15      ; 464        ; 7        ; LED_config[2]                                             ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; H16      ; 459        ; 7        ; sal_LED[0]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; H17      ; 454        ; 7        ; LED_inst[1]                                               ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; H18      ;            ; 7        ; VCCIO7                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; H19      ; 446        ; 7        ; sal_LED[4]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; H20      ;            ;          ; GNDA2                                                     ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; H21      ; 448        ; 7        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; H22      ; 399        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H23      ; 391        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H24      ; 390        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H25      ; 377        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H26      ; 376        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; H27      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; H28      ;            ; 6        ; VCCIO6                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; J1       ; 64         ; 1        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; J2       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; J3       ; 23         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J4       ; 22         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J5       ; 36         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J6       ; 35         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J7       ; 37         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J8       ;            ; --       ; VCCA3                                                     ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; J9       ;            ;          ; VCCD_PLL3                                                 ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J10      ; 515        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; J11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; J12      ; 490        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; J13      ; 489        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; J14      ; 481        ; 8        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; J15      ; 465        ; 7        ; sal_LED[1]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; J16      ; 458        ; 7        ; LED_inst[0]                                               ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; J17      ; 450        ; 7        ; sal_LED[3]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; J18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; J19      ; 447        ; 7        ; sal_LED[5]                                                ; output ; 2.5 V        ;         ; Column I/O ; Y               ; no       ; Off          ;
; J20      ;            ;          ; VCCD_PLL2                                                 ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; J21      ;            ; --       ; VCCA2                                                     ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; J22      ; 394        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J23      ; 387        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J24      ; 386        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J25      ; 365        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J26      ; 364        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; J27      ; 338        ; 6        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; J28      ; 337        ; 6        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; K1       ; 28         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K2       ; 27         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K3       ; 30         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K4       ; 29         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K5       ;            ; 1        ; VCCIO1                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; K6       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K7       ; 38         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K8       ; 39         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K9       ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K10      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K11      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K13      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K14      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K15      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K17      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K19      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; K20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K21      ; 389        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K22      ; 388        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K23      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; K24      ;            ; 6        ; VCCIO6                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; K25      ; 371        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K26      ; 370        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K27      ; 362        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; K28      ; 361        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L1       ; 49         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L2       ; 48         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L3       ; 32         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L4       ; 31         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L5       ; 21         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L6       ; 43         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L7       ; 42         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L8       ; 40         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L10      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L12      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L14      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L15      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L16      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L17      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L18      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L19      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; L20      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; L21      ; 385        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L22      ; 384        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L23      ; 360        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L24      ; 359        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L25      ; 369        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L26      ; 363        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L27      ; 358        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; L28      ; 357        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M1       ; 51         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M2       ; 50         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M3       ; 34         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M4       ; 33         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M5       ; 41         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M6       ; 24         ; 1        ; ^nSTATUS                                                  ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M7       ; 47         ; 1        ; pulse_48KHz                                               ; output ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; Off          ;
; M8       ; 46         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M9       ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M10      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M11      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M13      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M14      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M15      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M17      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M19      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; M20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; M21      ; 368        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M22      ; 342        ; 6        ; ^MSEL2                                                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; M23      ; 344        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M24      ; 347        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M25      ; 356        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M26      ; 355        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M27      ; 354        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; M28      ; 353        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N1       ;            ; 1        ; VCCIO1                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; N2       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N3       ; 45         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N4       ; 44         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N5       ;            ; 1        ; VCCIO1                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; N6       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N7       ; 56         ; 1        ; ~ALTERA_DATA0~ / RESERVED_INPUT_WITH_WEAK_PULLUP          ; input  ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; On           ;
; N8       ; 54         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N10      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N12      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N14      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N15      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N16      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N17      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N18      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N19      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N20      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; N21      ; 348        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N22      ; 340        ; 6        ; ^MSEL0                                                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; N23      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N24      ;            ; 6        ; VCCIO6                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; N25      ; 352        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N26      ; 351        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; N27      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; N28      ;            ; 6        ; VCCIO6                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; P1       ; 53         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P2       ; 52         ; 1        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P3       ; 55         ; 1        ; ~ALTERA_DCLK~                                             ; output ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; On           ;
; P4       ; 57         ; 1        ; ^nCONFIG                                                  ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P5       ; 59         ; 1        ; #TCK                                                      ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; P6       ; 61         ; 1        ; #TDO                                                      ; output ;              ;         ; --         ;                 ; --       ; --           ;
; P7       ; 58         ; 1        ; #TDI                                                      ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; P8       ; 60         ; 1        ; #TMS                                                      ; input  ;              ;         ; --         ;                 ; --       ; --           ;
; P9       ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P10      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P11      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P13      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P14      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P15      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P17      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P19      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; P20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; P21      ; 334        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P22      ; 343        ; 6        ; ^MSEL3                                                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P23      ; 341        ; 6        ; ^MSEL1                                                    ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P24      ; 339        ; 6        ; ^CONF_DONE                                                ;        ;              ;         ; --         ;                 ; --       ; --           ;
; P25      ; 346        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P26      ; 345        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P27      ; 350        ; 6        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; P28      ; 349        ; 6        ; ~ALTERA_nCEO~ / RESERVED_OUTPUT_OPEN_DRAIN                ; output ; 2.5 V        ;         ; Row I/O    ; N               ; no       ; Off          ;
; R1       ; 68         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R2       ; 67         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R3       ; 73         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R4       ; 74         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R5       ; 77         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R6       ; 70         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R7       ; 69         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R8       ; 62         ; 1        ; ^nCE                                                      ;        ;              ;         ; --         ;                 ; --       ; --           ;
; R9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R10      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R12      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R14      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R15      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R16      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R17      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R18      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R19      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; R20      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; R21      ; 333        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R22      ; 332        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R23      ; 331        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R24      ; 330        ; 5        ; en                                                        ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; R25      ; 327        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R26      ; 326        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R27      ; 329        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; R28      ; 328        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T1       ;            ; 2        ; VCCIO2                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; T2       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T3       ; 76         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T4       ; 75         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T5       ;            ; 2        ; VCCIO2                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; T6       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T7       ; 78         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T8       ; 100        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T9       ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T10      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T11      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T13      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T14      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T15      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T17      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T19      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; T20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T21      ; 325        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T22      ; 324        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T23      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T24      ;            ; 5        ; VCCIO5                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; T25      ; 323        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T26      ; 322        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; T27      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; T28      ;            ; 5        ; VCCIO5                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; U1       ; 80         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U2       ; 79         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U3       ; 71         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U4       ; 72         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U5       ; 90         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U6       ; 89         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U7       ; 103        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U8       ; 104        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U10      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U12      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U14      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U15      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U16      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U17      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U18      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U19      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; U20      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; U21      ; 319        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U22      ; 313        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U23      ; 305        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U24      ; 316        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U25      ; 315        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U26      ; 314        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U27      ; 318        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; U28      ; 317        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V1       ; 84         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V2       ; 83         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V3       ; 82         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V4       ; 81         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V5       ; 108        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V6       ; 107        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V7       ; 110        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V8       ; 109        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V9       ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V10      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V11      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V12      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V13      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V14      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V15      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V16      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V17      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V19      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; V20      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; V21      ; 311        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V22      ; 312        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V23      ; 309        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V24      ; 308        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V25      ; 307        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V26      ; 306        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V27      ; 304        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; V28      ; 303        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W1       ; 88         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W2       ; 87         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W3       ; 112        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W4       ; 111        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W5       ;            ; 2        ; VCCIO2                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; W6       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W7       ; 115        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W8       ; 116        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W9       ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W10      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W12      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W13      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W14      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W15      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W16      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W17      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W18      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W19      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W20      ;            ;          ; VCCINT                                                    ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; W21      ; 310        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W22      ; 321        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W23      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; W24      ;            ; 5        ; VCCIO5                                                    ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; W25      ; 300        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W26      ; 299        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W27      ; 301        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; W28      ; 302        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y1       ; 66         ; 2        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; Y2       ; 65         ; 2        ; CLK                                                       ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; Y3       ; 92         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y4       ; 91         ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y5       ; 114        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y6       ; 113        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y7       ; 117        ; 2        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y8       ;            ; --       ; VCCA1                                                     ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; Y9       ;            ;          ; VCCD_PLL1                                                 ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; Y10      ; 140        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y11      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; Y12      ; 187        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y13      ; 189        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y14      ; 197        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y15      ; 198        ; 3        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y16      ; 250        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y17      ; 249        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y18      ;            ;          ; GND                                                       ; gnd    ;              ;         ; --         ;                 ; --       ; --           ;
; Y19      ; 263        ; 4        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Column I/O ;                 ; no       ; On           ;
; Y20      ;            ;          ; VCCD_PLL4                                                 ; power  ;              ; 1.2V    ; --         ;                 ; --       ; --           ;
; Y21      ;            ; --       ; VCCA4                                                     ; power  ;              ; 2.5V    ; --         ;                 ; --       ; --           ;
; Y22      ; 320        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y23      ; 288        ; 5        ; INIT                                                      ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; Y24      ; 287        ; 5        ; W_EN                                                      ; input  ; 2.5 V        ;         ; Row I/O    ; Y               ; no       ; Off          ;
; Y25      ; 298        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y26      ; 297        ; 5        ; RESERVED_INPUT_WITH_WEAK_PULLUP                           ;        ;              ;         ; Row I/O    ;                 ; no       ; On           ;
; Y27      ; 336        ; 5        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
; Y28      ; 335        ; 5        ; GND+                                                      ;        ;              ;         ; Row I/O    ;                 ; --       ; --           ;
+----------+------------+----------+-----------------------------------------------------------+--------+--------------+---------+------------+-----------------+----------+--------------+
Note: Pin directions (input, output or bidir) are based on device operating in user mode.


+---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Fitter Resource Utilization by Entity                                                                                                                                                                                                                                                                                                                                                                         ;
+---------------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+--------------------------------------------------------------------------------------------------------------------------------------------+--------------+
; Compilation Hierarchy Node                        ; Logic Cells ; Dedicated Logic Registers ; I/O Registers ; Memory Bits ; M9Ks ; DSP Elements ; DSP 9x9 ; DSP 18x18 ; Pins ; Virtual Pins ; LUT-Only LCs ; Register-Only LCs ; LUT/Register LCs ; Full Hierarchy Name                                                                                                                        ; Library Name ;
+---------------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+--------------------------------------------------------------------------------------------------------------------------------------------+--------------+
; |proyecto                                         ; 7551 (1)    ; 3087 (0)                  ; 0 (0)         ; 0           ; 0    ; 20           ; 20      ; 0         ; 57   ; 0            ; 4464 (1)     ; 695 (0)           ; 2392 (0)         ; |proyecto                                                                                                                                  ;              ;
;    |DMUX:U16|                                     ; 160 (160)   ; 160 (160)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 146 (146)         ; 14 (14)          ; |proyecto|DMUX:U16                                                                                                                         ;              ;
;    |DMUX:U33|                                     ; 160 (160)   ; 160 (160)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 138 (138)         ; 22 (22)          ; |proyecto|DMUX:U33                                                                                                                         ;              ;
;    |FF1:U13|                                      ; 219 (219)   ; 180 (180)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (18)      ; 11 (11)           ; 190 (190)        ; |proyecto|FF1:U13                                                                                                                          ;              ;
;    |FF1:U30|                                      ; 217 (217)   ; 180 (180)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 14 (14)      ; 9 (9)             ; 194 (194)        ; |proyecto|FF1:U30                                                                                                                          ;              ;
;    |FF2:U17|                                      ; 80 (80)     ; 80 (80)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 10 (10)           ; 70 (70)          ; |proyecto|FF2:U17                                                                                                                          ;              ;
;    |FF2:U34|                                      ; 112 (112)   ; 80 (80)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (28)      ; 8 (8)             ; 76 (76)          ; |proyecto|FF2:U34                                                                                                                          ;              ;
;    |LED3:U43|                                     ; 3 (3)       ; 3 (3)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 3 (3)            ; |proyecto|LED3:U43                                                                                                                         ;              ;
;    |acum:U11|                                     ; 342 (342)   ; 342 (342)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 342 (342)        ; |proyecto|acum:U11                                                                                                                         ;              ;
;    |acum:U28|                                     ; 342 (342)   ; 342 (342)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 342 (342)        ; |proyecto|acum:U28                                                                                                                         ;              ;
;    |amplitud:U25|                                 ; 322 (322)   ; 150 (150)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 172 (172)    ; 21 (21)           ; 129 (129)        ; |proyecto|amplitud:U25                                                                                                                     ;              ;
;    |amplitud:U7|                                  ; 321 (321)   ; 150 (150)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 171 (171)    ; 18 (18)           ; 132 (132)        ; |proyecto|amplitud:U7                                                                                                                      ;              ;
;    |arm:U10|                                      ; 281 (181)   ; 165 (165)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 116 (16)     ; 4 (4)             ; 161 (113)        ; |proyecto|arm:U10                                                                                                                          ;              ;
;       |lpm_mult:Mult0|                            ; 48 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 32 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult0                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 48 (19)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 32 (19)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 29 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 13 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_88h:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_2jh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_2jh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_dkh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_dkh:auto_generated   ;              ;
;       |lpm_mult:Mult1|                            ; 56 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult1                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 56 (27)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (27)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 29 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 13 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_88h:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_2jh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_2jh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_dkh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_dkh:auto_generated   ;              ;
;       |lpm_mult:Mult2|                            ; 44 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult2                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 44 (14)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (14)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 30 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 14 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 10 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_g9h:auto_generated|    ; 10 (10)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_g9h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_akh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_akh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_ekh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_ekh:auto_generated   ;              ;
;    |arm:U27|                                      ; 281 (181)   ; 165 (165)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 116 (16)     ; 4 (4)             ; 161 (113)        ; |proyecto|arm:U27                                                                                                                          ;              ;
;       |lpm_mult:Mult0|                            ; 60 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 44 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult0                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 60 (31)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 44 (31)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 29 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 13 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_88h:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_2jh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_2jh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_dkh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_dkh:auto_generated   ;              ;
;       |lpm_mult:Mult1|                            ; 44 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult1                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 44 (15)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (15)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 29 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 13 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_88h:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 5 (5)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_2jh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_2jh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_dkh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_dkh:auto_generated   ;              ;
;       |lpm_mult:Mult2|                            ; 44 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult2                                                                                                           ;              ;
;          |multcore:mult_core|                     ; 44 (14)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 28 (14)      ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core                                                                                        ;              ;
;             |mpar_add:padder|                     ; 30 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 14 (0)       ; 0 (0)             ; 16 (0)           ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder                                                                        ;              ;
;                |lpm_add_sub:adder[0]|             ; 10 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (0)        ; 0 (0)             ; 4 (0)            ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                   ;              ;
;                   |add_sub_g9h:auto_generated|    ; 10 (10)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 4 (4)            ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_g9h:auto_generated                        ;              ;
;                |lpm_add_sub:adder[1]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]                                                   ;              ;
;                   |add_sub_akh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[1]|add_sub_akh:auto_generated                        ;              ;
;                |mpar_add:sub_par_add|             ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                   ;              ;
;                   |lpm_add_sub:adder[0]|          ; 12 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (0)           ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                              ;              ;
;                      |add_sub_ekh:auto_generated| ; 12 (12)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_ekh:auto_generated   ;              ;
;    |arp:U22|                                      ; 11 (11)     ; 11 (11)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 11 (11)          ; |proyecto|arp:U22                                                                                                                          ;              ;
;    |calc_notas:U23|                               ; 86 (86)     ; 8 (8)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 70 (70)      ; 0 (0)             ; 16 (16)          ; |proyecto|calc_notas:U23                                                                                                                   ;              ;
;    |control:U8|                                   ; 6 (6)       ; 5 (5)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 1 (1)        ; 0 (0)             ; 5 (5)            ; |proyecto|control:U8                                                                                                                       ;              ;
;    |deteccion:U40|                                ; 11 (11)     ; 11 (11)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 11 (11)          ; |proyecto|deteccion:U40                                                                                                                    ;              ;
;    |divisor1:U1|                                  ; 18 (18)     ; 12 (12)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 12 (12)          ; |proyecto|divisor1:U1                                                                                                                      ;              ;
;    |divisor2:U2|                                  ; 1 (1)       ; 1 (1)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 1 (1)             ; 0 (0)            ; |proyecto|divisor2:U2                                                                                                                      ;              ;
;    |divisor3:U3|                                  ; 17 (17)     ; 11 (11)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 6 (6)        ; 0 (0)             ; 11 (11)          ; |proyecto|divisor3:U3                                                                                                                      ;              ;
;    |fase:U24|                                     ; 844 (844)   ; 342 (342)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 502 (502)    ; 147 (147)         ; 195 (195)        ; |proyecto|fase:U24                                                                                                                         ;              ;
;    |fase:U6|                                      ; 845 (845)   ; 342 (342)                 ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 503 (503)    ; 149 (149)         ; 193 (193)        ; |proyecto|fase:U6                                                                                                                          ;              ;
;    |g00_audio_interface:U4|                       ; 186 (186)   ; 93 (93)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 93 (93)      ; 2 (2)             ; 91 (91)          ; |proyecto|g00_audio_interface:U4                                                                                                           ;              ;
;    |incrementos:U26|                              ; 56 (56)     ; 26 (26)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 30 (30)      ; 14 (14)           ; 12 (12)          ; |proyecto|incrementos:U26                                                                                                                  ;              ;
;    |incrementos:U9|                               ; 55 (55)     ; 26 (26)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 29 (29)      ; 13 (13)           ; 13 (13)          ; |proyecto|incrementos:U9                                                                                                                   ;              ;
;    |invertir:U42|                                 ; 12 (12)     ; 12 (12)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 12 (12)          ; |proyecto|invertir:U42                                                                                                                     ;              ;
;    |mult:U18|                                     ; 343 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 10           ; 10      ; 0         ; 0    ; 0            ; 257 (0)      ; 0 (0)             ; 86 (0)           ; |proyecto|mult:U18                                                                                                                         ;              ;
;       |lpm_mult:Mult0|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult0                                                                                                          ;              ;
;          |mult_aat:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult0|mult_aat:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult10|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 38 (0)       ; 0 (0)             ; 12 (0)           ; |proyecto|mult:U18|lpm_mult:Mult10                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 38 (38)      ; 0 (0)             ; 12 (12)          ; |proyecto|mult:U18|lpm_mult:Mult10|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult11|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (0)       ; 0 (0)             ; 10 (0)           ; |proyecto|mult:U18|lpm_mult:Mult11                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (40)      ; 0 (0)             ; 10 (10)          ; |proyecto|mult:U18|lpm_mult:Mult11|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult12|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (0)       ; 0 (0)             ; 11 (0)           ; |proyecto|mult:U18|lpm_mult:Mult12                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (39)      ; 0 (0)             ; 11 (11)          ; |proyecto|mult:U18|lpm_mult:Mult12|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult13|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (0)       ; 0 (0)             ; 10 (0)           ; |proyecto|mult:U18|lpm_mult:Mult13                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (40)      ; 0 (0)             ; 10 (10)          ; |proyecto|mult:U18|lpm_mult:Mult13|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult14|                           ; 42 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 29 (0)       ; 0 (0)             ; 13 (0)           ; |proyecto|mult:U18|lpm_mult:Mult14                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 42 (24)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 29 (13)      ; 0 (0)             ; 13 (11)          ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 18 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 16 (0)       ; 0 (0)             ; 2 (0)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;                |mpar_add:sub_par_add|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 7 (0)        ; 0 (0)             ; 2 (0)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                 ;              ;
;                   |lpm_add_sub:adder[0]|          ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 7 (0)        ; 0 (0)             ; 2 (0)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                            ;              ;
;                      |add_sub_vch:auto_generated| ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 7 (7)        ; 0 (0)             ; 2 (2)            ; |proyecto|mult:U18|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_vch:auto_generated ;              ;
;       |lpm_mult:Mult15|                           ; 34 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 26 (0)       ; 0 (0)             ; 8 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 34 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 26 (9)       ; 0 (0)             ; 8 (7)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 18 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 17 (0)       ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 1 (1)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;                |mpar_add:sub_par_add|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                 ;              ;
;                   |lpm_add_sub:adder[0]|          ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                            ;              ;
;                      |add_sub_vch:auto_generated| ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_vch:auto_generated ;              ;
;       |lpm_mult:Mult16|                           ; 25 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 19 (0)       ; 0 (0)             ; 6 (0)            ; |proyecto|mult:U18|lpm_mult:Mult16                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 25 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 19 (10)      ; 0 (0)             ; 6 (6)            ; |proyecto|mult:U18|lpm_mult:Mult16|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult17|                           ; 25 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (0)       ; 0 (0)             ; 7 (0)            ; |proyecto|mult:U18|lpm_mult:Mult17                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 25 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (9)       ; 0 (0)             ; 7 (7)            ; |proyecto|mult:U18|lpm_mult:Mult17|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult19|                           ; 17 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 9 (0)            ; |proyecto|mult:U18|lpm_mult:Mult19                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 17 (8)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 9 (8)            ; |proyecto|mult:U18|lpm_mult:Mult19|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U18|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U18|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 1 (1)            ; |proyecto|mult:U18|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult1|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult1                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult1|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult2|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult2                                                                                                          ;              ;
;          |mult_aat:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult2|mult_aat:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult3|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult3                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult3|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult4|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult4                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult4|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult5|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult5                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult5|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult6|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult6                                                                                                          ;              ;
;          |mult_7at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult6|mult_7at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult7|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult7                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult7|mult_4at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult8|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult8                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult8|mult_4at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult9|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult9                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U18|lpm_mult:Mult9|mult_4at:auto_generated                                                                                  ;              ;
;    |mult:U35|                                     ; 342 (0)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 10           ; 10      ; 0         ; 0    ; 0            ; 262 (0)      ; 0 (0)             ; 80 (0)           ; |proyecto|mult:U35                                                                                                                         ;              ;
;       |lpm_mult:Mult0|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult0                                                                                                          ;              ;
;          |mult_aat:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult0|mult_aat:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult10|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (0)       ; 0 (0)             ; 10 (0)           ; |proyecto|mult:U35|lpm_mult:Mult10                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 40 (40)      ; 0 (0)             ; 10 (10)          ; |proyecto|mult:U35|lpm_mult:Mult10|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult11|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (0)       ; 0 (0)             ; 11 (0)           ; |proyecto|mult:U35|lpm_mult:Mult11                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (39)      ; 0 (0)             ; 11 (11)          ; |proyecto|mult:U35|lpm_mult:Mult11|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult12|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 38 (0)       ; 0 (0)             ; 12 (0)           ; |proyecto|mult:U35|lpm_mult:Mult12                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 38 (38)      ; 0 (0)             ; 12 (12)          ; |proyecto|mult:U35|lpm_mult:Mult12|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult13|                           ; 50 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (0)       ; 0 (0)             ; 11 (0)           ; |proyecto|mult:U35|lpm_mult:Mult13                                                                                                         ;              ;
;          |mult_2at:auto_generated|                ; 50 (50)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 39 (39)      ; 0 (0)             ; 11 (11)          ; |proyecto|mult:U35|lpm_mult:Mult13|mult_2at:auto_generated                                                                                 ;              ;
;       |lpm_mult:Mult14|                           ; 42 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 34 (0)       ; 0 (0)             ; 8 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 42 (24)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 34 (16)      ; 0 (0)             ; 8 (8)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 18 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (0)       ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;                |mpar_add:sub_par_add|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                 ;              ;
;                   |lpm_add_sub:adder[0]|          ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                            ;              ;
;                      |add_sub_vch:auto_generated| ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult14|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_vch:auto_generated ;              ;
;       |lpm_mult:Mult15|                           ; 34 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 25 (0)       ; 0 (0)             ; 9 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 34 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 25 (8)       ; 0 (0)             ; 9 (8)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 18 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 17 (0)       ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 1 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 1 (1)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;                |mpar_add:sub_par_add|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add                                                 ;              ;
;                   |lpm_add_sub:adder[0]|          ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]                            ;              ;
;                      |add_sub_vch:auto_generated| ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult15|multcore:mult_core|mpar_add:padder|mpar_add:sub_par_add|lpm_add_sub:adder[0]|add_sub_vch:auto_generated ;              ;
;       |lpm_mult:Mult16|                           ; 25 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (0)       ; 0 (0)             ; 7 (0)            ; |proyecto|mult:U35|lpm_mult:Mult16                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 25 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 18 (9)       ; 0 (0)             ; 7 (7)            ; |proyecto|mult:U35|lpm_mult:Mult16|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult16|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult17|                           ; 25 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 21 (0)       ; 0 (0)             ; 4 (0)            ; |proyecto|mult:U35|lpm_mult:Mult17                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 25 (16)     ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 21 (12)      ; 0 (0)             ; 4 (4)            ; |proyecto|mult:U35|lpm_mult:Mult17|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 9 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 9 (9)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 9 (9)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult17|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult19|                           ; 16 (0)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 8 (0)            ; |proyecto|mult:U35|lpm_mult:Mult19                                                                                                         ;              ;
;          |multcore:mult_core|                     ; 16 (8)      ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 8 (8)            ; |proyecto|mult:U35|lpm_mult:Mult19|multcore:mult_core                                                                                      ;              ;
;             |mpar_add:padder|                     ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder                                                                      ;              ;
;                |lpm_add_sub:adder[0]|             ; 8 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]                                                 ;              ;
;                   |add_sub_nbh:auto_generated|    ; 8 (8)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated                      ;              ;
;       |lpm_mult:Mult1|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult1                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult1|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult2|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult2                                                                                                          ;              ;
;          |mult_aat:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult2|mult_aat:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult3|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult3                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult3|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult4|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult4                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult4|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult5|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult5                                                                                                          ;              ;
;          |mult_8at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult5|mult_8at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult6|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult6                                                                                                          ;              ;
;          |mult_7at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult6|mult_7at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult7|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult7                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult7|mult_4at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult8|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult8                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult8|mult_4at:auto_generated                                                                                  ;              ;
;       |lpm_mult:Mult9|                            ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult9                                                                                                          ;              ;
;          |mult_4at:auto_generated|                ; 0 (0)       ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 1            ; 1       ; 0         ; 0    ; 0            ; 0 (0)        ; 0 (0)             ; 0 (0)            ; |proyecto|mult:U35|lpm_mult:Mult9|mult_4at:auto_generated                                                                                  ;              ;
;    |mux1:U14|                                     ; 117 (117)   ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 71 (71)      ; 0 (0)             ; 46 (46)          ; |proyecto|mux1:U14                                                                                                                         ;              ;
;    |mux1:U31|                                     ; 121 (121)   ; 9 (9)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 75 (75)      ; 0 (0)             ; 46 (46)          ; |proyecto|mux1:U31                                                                                                                         ;              ;
;    |offset:U19|                                   ; 423 (423)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 371 (371)    ; 0 (0)             ; 52 (52)          ; |proyecto|offset:U19                                                                                                                       ;              ;
;    |offset:U36|                                   ; 423 (423)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 376 (376)    ; 0 (0)             ; 47 (47)          ; |proyecto|offset:U36                                                                                                                       ;              ;
;    |seleccion:U41|                                ; 20 (20)     ; 12 (12)                   ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 8 (8)        ; 0 (0)             ; 12 (12)          ; |proyecto|seleccion:U41                                                                                                                    ;              ;
;    |sen:U15|                                      ; 265 (265)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 254 (254)    ; 0 (0)             ; 11 (11)          ; |proyecto|sen:U15                                                                                                                          ;              ;
;    |sen:U32|                                      ; 265 (265)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 254 (254)    ; 0 (0)             ; 11 (11)          ; |proyecto|sen:U32                                                                                                                          ;              ;
;    |suma:U20|                                     ; 330 (330)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 330 (330)    ; 0 (0)             ; 0 (0)            ; |proyecto|suma:U20                                                                                                                         ;              ;
;    |suma:U37|                                     ; 330 (330)   ; 0 (0)                     ; 0 (0)         ; 0           ; 0    ; 0            ; 0       ; 0         ; 0    ; 0            ; 330 (330)    ; 0 (0)             ; 0 (0)            ; |proyecto|suma:U37                                                                                                                         ;              ;
+---------------------------------------------------+-------------+---------------------------+---------------+-------------+------+--------------+---------+-----------+------+--------------+--------------+-------------------+------------------+--------------------------------------------------------------------------------------------------------------------------------------------+--------------+
Note: For table entries with two numbers listed, the numbers in parentheses indicate the number of resources of the given type used by the specific entity alone. The numbers listed outside of parentheses indicate the total resources of the given type used by the specific entity and all of its sub-entities in the hierarchy.


+-----------------------------------------------------------------------------------------------+
; Delay Chain Summary                                                                           ;
+---------------+----------+---------------+---------------+-----------------------+-----+------+
; Name          ; Pin Type ; Pad to Core 0 ; Pad to Core 1 ; Pad to Input Register ; TCO ; TCOE ;
+---------------+----------+---------------+---------------+-----------------------+-----+------+
; LED_config[0] ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; LED_config[1] ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; LED_config[2] ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; LED_modo      ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; LED_inst[0]   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; LED_inst[1]   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[0]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[1]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[2]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[3]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[4]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[5]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[6]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[7]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[8]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[9]    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[10]   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sal_LED[11]   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; pulse_48KHz   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; AUD_MCLK      ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; AUD_BCLK      ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; AUD_DACDAT    ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; AUD_DACLRCK   ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; I2C_SDAT      ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; I2C_SCLK      ; Output   ; --            ; --            ; --                    ; --  ; --   ;
; sel           ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; num_inst[0]   ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; num_inst[1]   ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; RST           ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; CLK           ; Input    ; (0) 0 ps      ; --            ; --                    ; --  ; --   ;
; W_EN          ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; INIT          ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[0]  ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[1]  ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas_int[2]  ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas_int[3]  ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas_int[4]  ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[5]  ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[6]  ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[7]  ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[8]  ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas_int[9]  ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas_int[10] ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas_int[11] ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[0]      ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; en            ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas[1]      ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas[2]      ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[3]      ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas[5]      ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[6]      ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[7]      ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas[8]      ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[9]      ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[10]     ; Input    ; (6) 1314 ps   ; --            ; --                    ; --  ; --   ;
; notas[11]     ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
; notas[4]      ; Input    ; --            ; (6) 1314 ps   ; --                    ; --  ; --   ;
+---------------+----------+---------------+---------------+-----------------------+-----+------+


+-----------------------------------------------------------------------------+
; Pad To Core Delay Chain Fanout                                              ;
+-----------------------------------------------+-------------------+---------+
; Source Pin / Fanout                           ; Pad To Core Index ; Setting ;
+-----------------------------------------------+-------------------+---------+
; sel                                           ;                   ;         ;
;      - seleccion:U41|inter~0                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~1                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~2                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~3                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~4                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~5                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~6                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~7                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~8                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~9                  ; 1                 ; 6       ;
;      - seleccion:U41|inter~10                 ; 1                 ; 6       ;
;      - seleccion:U41|inter~11                 ; 1                 ; 6       ;
;      - LED_modo~output                        ; 1                 ; 6       ;
; num_inst[0]                                   ;                   ;         ;
;      - fase:U24|fase12e[6]                    ; 0                 ; 6       ;
;      - fase:U24|fase15e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[8]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[0]                    ; 0                 ; 6       ;
;      - fase:U24|fase19e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase19e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase19e[0]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[5]                    ; 0                 ; 6       ;
;      - fase:U6|fase12e[6]                     ; 0                 ; 6       ;
;      - fase:U6|fase15e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase18e[8]                     ; 0                 ; 6       ;
;      - fase:U6|fase18e[0]                     ; 0                 ; 6       ;
;      - fase:U6|fase19e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase19e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase19e[0]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[5]                     ; 0                 ; 6       ;
;      - incrementos:U26|INCe[14]               ; 0                 ; 6       ;
;      - incrementos:U9|INCe[14]                ; 0                 ; 6       ;
;      - amplitud:U25|amp9e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp8e[0]                  ; 0                 ; 6       ;
;      - amplitud:U7|amp9e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp8e[0]                   ; 0                 ; 6       ;
;      - amplitud:U25|amp10e[0]~0               ; 0                 ; 6       ;
;      - amplitud:U25|amp1e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e[2]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e[3]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e[4]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e[5]                  ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[7]               ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[6]~1             ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[5]               ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[4]               ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[3]               ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde[2]               ; 0                 ; 6       ;
;      - amplitud:U25|amp3e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp3e[2]~2                ; 0                 ; 6       ;
;      - amplitud:U25|amp3e[3]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp2e[5]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp2e[4]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp2e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp6e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp6e[1]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp5e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp5e[1]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp5e[2]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp4e[0]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp4e[1]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp4e[2]                  ; 0                 ; 6       ;
;      - amplitud:U25|amp4e[3]                  ; 0                 ; 6       ;
;      - amplitud:U7|amp10e[0]~0                ; 0                 ; 6       ;
;      - amplitud:U7|amp1e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e[2]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e[3]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e[4]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e[5]                   ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[7]                ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[6]~1              ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[5]                ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[4]                ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[3]                ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde[2]                ; 0                 ; 6       ;
;      - amplitud:U7|amp3e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp3e[2]~2                 ; 0                 ; 6       ;
;      - amplitud:U7|amp3e[3]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp2e[5]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp2e[4]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp2e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp6e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp6e[1]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp5e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp5e[1]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp5e[2]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp4e[0]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp4e[1]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp4e[2]                   ; 0                 ; 6       ;
;      - amplitud:U7|amp4e[3]                   ; 0                 ; 6       ;
;      - fase:U24|fase9e[0]                     ; 0                 ; 6       ;
;      - fase:U24|fase1e[0]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[0]                    ; 0                 ; 6       ;
;      - fase:U24|fase6e[0]                     ; 0                 ; 6       ;
;      - fase:U24|fase4e[0]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[0]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[0]                    ; 0                 ; 6       ;
;      - fase:U24|fase10e[8]                    ; 0                 ; 6       ;
;      - fase:U24|fase3e[8]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[8]~1                  ; 0                 ; 6       ;
;      - fase:U24|fase12e[8]                    ; 0                 ; 6       ;
;      - fase:U24|fase13e[8]                    ; 0                 ; 6       ;
;      - fase:U24|fase8e[8]                     ; 0                 ; 6       ;
;      - fase:U24|fase1e[8]                     ; 0                 ; 6       ;
;      - fase:U24|fase9e[8]                     ; 0                 ; 6       ;
;      - fase:U24|fase7e[8]                     ; 0                 ; 6       ;
;      - fase:U24|fase16e[8]                    ; 0                 ; 6       ;
;      - fase:U24|fase6e[7]                     ; 0                 ; 6       ;
;      - fase:U24|fase2e[7]~1                   ; 0                 ; 6       ;
;      - fase:U24|fase14e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase1e[7]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase4e[7]                     ; 0                 ; 6       ;
;      - fase:U24|fase8e[7]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase15e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[7]                    ; 0                 ; 6       ;
;      - fase:U24|fase6e[4]~2                   ; 0                 ; 6       ;
;      - fase:U24|fase10e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase2e[4]                     ; 0                 ; 6       ;
;      - fase:U24|fase14e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase5e[4]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase11e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase7e[4]                     ; 0                 ; 6       ;
;      - fase:U24|fase3e[4]                     ; 0                 ; 6       ;
;      - fase:U24|fase15e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase16e[4]                    ; 0                 ; 6       ;
;      - fase:U24|fase10e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase3e[5]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase5e[5]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase1e[5]                     ; 0                 ; 6       ;
;      - fase:U24|fase9e[5]                     ; 0                 ; 6       ;
;      - fase:U24|fase14e[5]~2                  ; 0                 ; 6       ;
;      - fase:U24|fase7e[5]                     ; 0                 ; 6       ;
;      - fase:U24|fase6e[5]~3                   ; 0                 ; 6       ;
;      - fase:U24|fase18e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase16e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase19e[5]                    ; 0                 ; 6       ;
;      - fase:U24|fase3e[3]                     ; 0                 ; 6       ;
;      - fase:U24|fase7e[3]                     ; 0                 ; 6       ;
;      - fase:U24|fase9e[3]                     ; 0                 ; 6       ;
;      - fase:U24|fase8e[3]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase5e[3]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase14e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase10e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[3]                    ; 0                 ; 6       ;
;      - fase:U24|fase6e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase12e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase14e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase3e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase9e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase1e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase8e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase10e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase13e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase5e[2]                     ; 0                 ; 6       ;
;      - fase:U24|fase15e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase16e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase19e[2]                    ; 0                 ; 6       ;
;      - fase:U24|fase3e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase6e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase2e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase7e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase9e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase8e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase4e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase5e[6]                     ; 0                 ; 6       ;
;      - fase:U24|fase11e[6]~6                  ; 0                 ; 6       ;
;      - fase:U24|fase10e[6]                    ; 0                 ; 6       ;
;      - fase:U24|fase18e[6]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[6]                    ; 0                 ; 6       ;
;      - fase:U24|fase16e[6]                    ; 0                 ; 6       ;
;      - fase:U24|fase6e[1]                     ; 0                 ; 6       ;
;      - fase:U24|fase3e[1]                     ; 0                 ; 6       ;
;      - fase:U24|fase2e[1]~5                   ; 0                 ; 6       ;
;      - fase:U24|fase9e[1]                     ; 0                 ; 6       ;
;      - fase:U24|fase12e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase8e[1]                     ; 0                 ; 6       ;
;      - fase:U24|fase13e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase4e[1]                     ; 0                 ; 6       ;
;      - fase:U24|fase5e[1]~5                   ; 0                 ; 6       ;
;      - fase:U24|fase14e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase11e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase10e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase17e[1]                    ; 0                 ; 6       ;
;      - fase:U24|fase16e[1]                    ; 0                 ; 6       ;
;      - fase:U6|fase6e[0]                      ; 0                 ; 6       ;
;      - fase:U6|fase9e[0]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[0]                     ; 0                 ; 6       ;
;      - fase:U6|fase4e[0]                      ; 0                 ; 6       ;
;      - fase:U6|fase1e[0]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[0]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[0]                     ; 0                 ; 6       ;
;      - fase:U6|fase3e[8]                      ; 0                 ; 6       ;
;      - fase:U6|fase7e[8]                      ; 0                 ; 6       ;
;      - fase:U6|fase12e[8]                     ; 0                 ; 6       ;
;      - fase:U6|fase9e[8]                      ; 0                 ; 6       ;
;      - fase:U6|fase8e[8]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[8]                     ; 0                 ; 6       ;
;      - fase:U6|fase1e[8]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[8]~1                   ; 0                 ; 6       ;
;      - fase:U6|fase10e[8]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[8]                     ; 0                 ; 6       ;
;      - fase:U6|fase6e[7]                      ; 0                 ; 6       ;
;      - fase:U6|fase4e[7]                      ; 0                 ; 6       ;
;      - fase:U6|fase14e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase1e[7]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase2e[7]~1                    ; 0                 ; 6       ;
;      - fase:U6|fase8e[7]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase15e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase18e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[7]                     ; 0                 ; 6       ;
;      - fase:U6|fase3e[4]                      ; 0                 ; 6       ;
;      - fase:U6|fase6e[4]~2                    ; 0                 ; 6       ;
;      - fase:U6|fase2e[4]                      ; 0                 ; 6       ;
;      - fase:U6|fase7e[4]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase5e[4]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase14e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase10e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase15e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[4]                     ; 0                 ; 6       ;
;      - fase:U6|fase9e[5]                      ; 0                 ; 6       ;
;      - fase:U6|fase3e[5]                      ; 0                 ; 6       ;
;      - fase:U6|fase1e[5]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase6e[5]~3                    ; 0                 ; 6       ;
;      - fase:U6|fase14e[5]~2                   ; 0                 ; 6       ;
;      - fase:U6|fase10e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase13e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase7e[5]                      ; 0                 ; 6       ;
;      - fase:U6|fase5e[5]                      ; 0                 ; 6       ;
;      - fase:U6|fase18e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase19e[5]                     ; 0                 ; 6       ;
;      - fase:U6|fase14e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase3e[3]                      ; 0                 ; 6       ;
;      - fase:U6|fase9e[3]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase8e[3]                      ; 0                 ; 6       ;
;      - fase:U6|fase10e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase7e[3]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase5e[3]                      ; 0                 ; 6       ;
;      - fase:U6|fase18e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[3]                     ; 0                 ; 6       ;
;      - fase:U6|fase9e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase12e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase8e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase13e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase6e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase3e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase1e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase5e[2]                      ; 0                 ; 6       ;
;      - fase:U6|fase14e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase10e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase15e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase18e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase19e[2]                     ; 0                 ; 6       ;
;      - fase:U6|fase9e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase8e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase6e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase3e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase2e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase7e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase4e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase5e[6]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[6]~6                   ; 0                 ; 6       ;
;      - fase:U6|fase10e[6]                     ; 0                 ; 6       ;
;      - fase:U6|fase17e[6]                     ; 0                 ; 6       ;
;      - fase:U6|fase18e[6]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[6]                     ; 0                 ; 6       ;
;      - fase:U6|fase9e[1]                      ; 0                 ; 6       ;
;      - fase:U6|fase3e[1]                      ; 0                 ; 6       ;
;      - fase:U6|fase11e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase6e[1]                      ; 0                 ; 6       ;
;      - fase:U6|fase12e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase4e[1]                      ; 0                 ; 6       ;
;      - fase:U6|fase14e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase2e[1]~5                    ; 0                 ; 6       ;
;      - fase:U6|fase8e[1]                      ; 0                 ; 6       ;
;      - fase:U6|fase10e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase13e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase5e[1]~5                    ; 0                 ; 6       ;
;      - fase:U6|fase17e[1]                     ; 0                 ; 6       ;
;      - fase:U6|fase16e[1]                     ; 0                 ; 6       ;
;      - incrementos:U26|INCe[9]                ; 0                 ; 6       ;
;      - incrementos:U26|INCe[10]               ; 0                 ; 6       ;
;      - incrementos:U26|INCe[8]                ; 0                 ; 6       ;
;      - incrementos:U26|INCe[3]                ; 0                 ; 6       ;
;      - incrementos:U26|INCe[6]                ; 0                 ; 6       ;
;      - incrementos:U26|INCe[7]                ; 0                 ; 6       ;
;      - incrementos:U26|INCe[11]               ; 0                 ; 6       ;
;      - incrementos:U26|INCe[12]               ; 0                 ; 6       ;
;      - incrementos:U9|INCe[9]                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe[8]                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe[10]                ; 0                 ; 6       ;
;      - incrementos:U9|INCe[11]                ; 0                 ; 6       ;
;      - incrementos:U9|INCe[3]                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe[6]                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe[7]                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe[12]                ; 0                 ; 6       ;
;      - amplitud:U7|Equal1~0                   ; 0                 ; 6       ;
;      - amplitud:U25|amp12e~5                  ; 0                 ; 6       ;
;      - amplitud:U25|amp10e~9                  ; 0                 ; 6       ;
;      - amplitud:U7|amp10e~9                   ; 0                 ; 6       ;
;      - amplitud:U25|amp15e~0                  ; 0                 ; 6       ;
;      - amplitud:U25|amp15e~1                  ; 0                 ; 6       ;
;      - amplitud:U25|amp12e~8                  ; 0                 ; 6       ;
;      - amplitud:U25|amp11e~4                  ; 0                 ; 6       ;
;      - fase:U24|fase15e[6]~7                  ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde~14               ; 0                 ; 6       ;
;      - amplitud:U25|ampfunde~19               ; 0                 ; 6       ;
;      - amplitud:U25|amp3e~8                   ; 0                 ; 6       ;
;      - amplitud:U25|amp2e~4                   ; 0                 ; 6       ;
;      - amplitud:U25|amp7e~2                   ; 0                 ; 6       ;
;      - amplitud:U25|Mux101~0                  ; 0                 ; 6       ;
;      - amplitud:U25|amp7e~6                   ; 0                 ; 6       ;
;      - amplitud:U25|amp8e~1                   ; 0                 ; 6       ;
;      - amplitud:U7|amp15e~0                   ; 0                 ; 6       ;
;      - amplitud:U7|amp15e~1                   ; 0                 ; 6       ;
;      - amplitud:U7|amp12e~7                   ; 0                 ; 6       ;
;      - amplitud:U7|amp11e~4                   ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde~14                ; 0                 ; 6       ;
;      - amplitud:U7|ampfunde~17                ; 0                 ; 6       ;
;      - amplitud:U7|amp3e~8                    ; 0                 ; 6       ;
;      - amplitud:U7|amp2e~4                    ; 0                 ; 6       ;
;      - amplitud:U7|amp2e~5                    ; 0                 ; 6       ;
;      - amplitud:U7|amp7e~2                    ; 0                 ; 6       ;
;      - amplitud:U7|Mux101~0                   ; 0                 ; 6       ;
;      - amplitud:U7|amp7e~6                    ; 0                 ; 6       ;
;      - amplitud:U7|amp8e~1                    ; 0                 ; 6       ;
;      - amplitud:U25|amp1e~18                  ; 0                 ; 6       ;
;      - amplitud:U25|amp12e~9                  ; 0                 ; 6       ;
;      - amplitud:U25|amp2e~15                  ; 0                 ; 6       ;
;      - amplitud:U25|amp2e~19                  ; 0                 ; 6       ;
;      - amplitud:U25|amp6e~13                  ; 0                 ; 6       ;
;      - amplitud:U25|amp7e~7                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e~18                   ; 0                 ; 6       ;
;      - amplitud:U7|amp12e~8                   ; 0                 ; 6       ;
;      - amplitud:U7|amp2e~15                   ; 0                 ; 6       ;
;      - amplitud:U7|amp2e~18                   ; 0                 ; 6       ;
;      - amplitud:U7|amp6e~14                   ; 0                 ; 6       ;
;      - amplitud:U7|amp7e~7                    ; 0                 ; 6       ;
;      - fase:U24|fase17e~11                    ; 0                 ; 6       ;
;      - fase:U24|fase17e~12                    ; 0                 ; 6       ;
;      - fase:U24|fase16e~10                    ; 0                 ; 6       ;
;      - fase:U24|fase16e~18                    ; 0                 ; 6       ;
;      - fase:U24|fase6e~24                     ; 0                 ; 6       ;
;      - fase:U24|fase10e~15                    ; 0                 ; 6       ;
;      - fase:U24|fase10e~31                    ; 0                 ; 6       ;
;      - fase:U24|fase2e~17                     ; 0                 ; 6       ;
;      - fase:U24|fase2e~24                     ; 0                 ; 6       ;
;      - fase:U24|fase2e~27                     ; 0                 ; 6       ;
;      - fase:U24|fase2e~28                     ; 0                 ; 6       ;
;      - fase:U24|fase14e~10                    ; 0                 ; 6       ;
;      - fase:U24|fase14e~11                    ; 0                 ; 6       ;
;      - fase:U24|fase9e~11                     ; 0                 ; 6       ;
;      - fase:U24|fase9e~14                     ; 0                 ; 6       ;
;      - fase:U24|fase9e~15                     ; 0                 ; 6       ;
;      - fase:U24|fase1e~18                     ; 0                 ; 6       ;
;      - fase:U24|fase1e~22                     ; 0                 ; 6       ;
;      - fase:U24|fase1e~23                     ; 0                 ; 6       ;
;      - fase:U24|fase1e~28                     ; 0                 ; 6       ;
;      - fase:U24|fase13e~11                    ; 0                 ; 6       ;
;      - fase:U24|fase4e~14                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~15                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~16                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~17                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~22                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~24                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~25                     ; 0                 ; 6       ;
;      - fase:U24|fase8e~22                     ; 0                 ; 6       ;
;      - fase:U24|fase8e~23                     ; 0                 ; 6       ;
;      - fase:U24|fase8e~27                     ; 0                 ; 6       ;
;      - fase:U24|fase8e~35                     ; 0                 ; 6       ;
;      - fase:U24|fase12e~12                    ; 0                 ; 6       ;
;      - fase:U24|fase12e~17                    ; 0                 ; 6       ;
;      - fase:U24|fase12e~20                    ; 0                 ; 6       ;
;      - fase:U24|fase12e~21                    ; 0                 ; 6       ;
;      - fase:U24|fase12e~22                    ; 0                 ; 6       ;
;      - fase:U24|fase12e~27                    ; 0                 ; 6       ;
;      - fase:U24|fase7e~19                     ; 0                 ; 6       ;
;      - fase:U24|fase7e~20                     ; 0                 ; 6       ;
;      - fase:U24|fase7e~26                     ; 0                 ; 6       ;
;      - fase:U24|fase7e~27                     ; 0                 ; 6       ;
;      - fase:U24|fase7e~30                     ; 0                 ; 6       ;
;      - fase:U24|fase11e~16                    ; 0                 ; 6       ;
;      - fase:U24|fase11e~17                    ; 0                 ; 6       ;
;      - fase:U24|fase3e~15                     ; 0                 ; 6       ;
;      - fase:U24|fase3e~31                     ; 0                 ; 6       ;
;      - fase:U24|fase3e~34                     ; 0                 ; 6       ;
;      - fase:U24|fase15e~10                    ; 0                 ; 6       ;
;      - fase:U24|fase15e~17                    ; 0                 ; 6       ;
;      - fase:U24|fase15e~18                    ; 0                 ; 6       ;
;      - fase:U24|fase15e~21                    ; 0                 ; 6       ;
;      - fase:U24|fase15e~24                    ; 0                 ; 6       ;
;      - fase:U24|fase17e~18                    ; 0                 ; 6       ;
;      - fase:U24|fase19e~19                    ; 0                 ; 6       ;
;      - fase:U24|fase2e~32                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~36                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~31                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~32                     ; 0                 ; 6       ;
;      - fase:U24|fase14e~26                    ; 0                 ; 6       ;
;      - fase:U24|fase6e~28                     ; 0                 ; 6       ;
;      - fase:U24|fase6e~29                     ; 0                 ; 6       ;
;      - fase:U24|fase15e~27                    ; 0                 ; 6       ;
;      - fase:U24|fase15e~28                    ; 0                 ; 6       ;
;      - fase:U6|fase17e~11                     ; 0                 ; 6       ;
;      - fase:U6|fase17e~12                     ; 0                 ; 6       ;
;      - fase:U6|fase16e~10                     ; 0                 ; 6       ;
;      - fase:U6|fase16e~18                     ; 0                 ; 6       ;
;      - fase:U6|fase6e~24                      ; 0                 ; 6       ;
;      - fase:U6|fase12e~11                     ; 0                 ; 6       ;
;      - fase:U6|fase12e~16                     ; 0                 ; 6       ;
;      - fase:U6|fase12e~19                     ; 0                 ; 6       ;
;      - fase:U6|fase12e~20                     ; 0                 ; 6       ;
;      - fase:U6|fase12e~21                     ; 0                 ; 6       ;
;      - fase:U6|fase12e~26                     ; 0                 ; 6       ;
;      - fase:U6|fase4e~18                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~19                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~20                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~21                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~23                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~25                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~26                      ; 0                 ; 6       ;
;      - fase:U6|fase14e~10                     ; 0                 ; 6       ;
;      - fase:U6|fase14e~11                     ; 0                 ; 6       ;
;      - fase:U6|fase3e~14                      ; 0                 ; 6       ;
;      - fase:U6|fase3e~30                      ; 0                 ; 6       ;
;      - fase:U6|fase3e~34                      ; 0                 ; 6       ;
;      - fase:U6|fase9e~15                      ; 0                 ; 6       ;
;      - fase:U6|fase9e~18                      ; 0                 ; 6       ;
;      - fase:U6|fase9e~19                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~15                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~18                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~22                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~23                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~28                      ; 0                 ; 6       ;
;      - fase:U6|fase11e~16                     ; 0                 ; 6       ;
;      - fase:U6|fase11e~17                     ; 0                 ; 6       ;
;      - fase:U6|fase2e~18                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~25                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~28                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~29                      ; 0                 ; 6       ;
;      - fase:U6|fase8e~21                      ; 0                 ; 6       ;
;      - fase:U6|fase8e~22                      ; 0                 ; 6       ;
;      - fase:U6|fase8e~26                      ; 0                 ; 6       ;
;      - fase:U6|fase8e~34                      ; 0                 ; 6       ;
;      - fase:U6|fase10e~19                     ; 0                 ; 6       ;
;      - fase:U6|fase10e~33                     ; 0                 ; 6       ;
;      - fase:U6|fase7e~25                      ; 0                 ; 6       ;
;      - fase:U6|fase7e~33                      ; 0                 ; 6       ;
;      - fase:U6|fase13e~11                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~9                      ; 0                 ; 6       ;
;      - fase:U6|fase15e~16                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~17                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~20                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~23                     ; 0                 ; 6       ;
;      - fase:U6|fase17e~18                     ; 0                 ; 6       ;
;      - fase:U6|fase19e~21                     ; 0                 ; 6       ;
;      - fase:U6|fase6e~28                      ; 0                 ; 6       ;
;      - fase:U6|fase6e~29                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~31                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~32                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~33                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~36                      ; 0                 ; 6       ;
;      - fase:U6|fase14e~26                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~26                     ; 0                 ; 6       ;
;      - fase:U6|fase15e~27                     ; 0                 ; 6       ;
;      - incrementos:U26|INCe~21                ; 0                 ; 6       ;
;      - incrementos:U26|INCe~22                ; 0                 ; 6       ;
;      - incrementos:U26|INCe~23                ; 0                 ; 6       ;
;      - incrementos:U26|INCe~24                ; 0                 ; 6       ;
;      - incrementos:U26|INCe~27                ; 0                 ; 6       ;
;      - incrementos:U26|INCe~28                ; 0                 ; 6       ;
;      - incrementos:U9|INCe~16                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe~17                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe~18                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe~19                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe~22                 ; 0                 ; 6       ;
;      - incrementos:U9|INCe~23                 ; 0                 ; 6       ;
;      - amplitud:U25|amp11e~5                  ; 0                 ; 6       ;
;      - amplitud:U25|amp10e~10                 ; 0                 ; 6       ;
;      - amplitud:U7|amp11e~5                   ; 0                 ; 6       ;
;      - amplitud:U7|amp10e~10                  ; 0                 ; 6       ;
;      - amplitud:U25|amp13e~3                  ; 0                 ; 6       ;
;      - amplitud:U25|amp12e~10                 ; 0                 ; 6       ;
;      - amplitud:U25|amp10e~11                 ; 0                 ; 6       ;
;      - amplitud:U25|amp11e~6                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e~35                  ; 0                 ; 6       ;
;      - amplitud:U25|amp1e~36                  ; 0                 ; 6       ;
;      - amplitud:U7|amp13e~3                   ; 0                 ; 6       ;
;      - amplitud:U7|amp12e~9                   ; 0                 ; 6       ;
;      - amplitud:U7|amp10e~11                  ; 0                 ; 6       ;
;      - amplitud:U7|amp11e~6                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e~34                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e~35                   ; 0                 ; 6       ;
;      - amplitud:U25|amp1e~37                  ; 0                 ; 6       ;
;      - amplitud:U25|amp7e~8                   ; 0                 ; 6       ;
;      - amplitud:U7|amp1e~36                   ; 0                 ; 6       ;
;      - amplitud:U7|amp7e~8                    ; 0                 ; 6       ;
;      - fase:U24|fase2e~33                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~38                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~39                     ; 0                 ; 6       ;
;      - fase:U24|fase1e~37                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~33                     ; 0                 ; 6       ;
;      - fase:U24|fase8e~38                     ; 0                 ; 6       ;
;      - fase:U24|fase7e~33                     ; 0                 ; 6       ;
;      - fase:U24|fase4e~34                     ; 0                 ; 6       ;
;      - fase:U24|fase14e~27                    ; 0                 ; 6       ;
;      - fase:U6|fase4e~34                      ; 0                 ; 6       ;
;      - fase:U6|fase1e~36                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~32                      ; 0                 ; 6       ;
;      - fase:U6|fase8e~37                      ; 0                 ; 6       ;
;      - fase:U6|fase7e~37                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~37                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~38                      ; 0                 ; 6       ;
;      - fase:U6|fase4e~35                      ; 0                 ; 6       ;
;      - fase:U6|fase14e~27                     ; 0                 ; 6       ;
;      - incrementos:U26|INCe~29                ; 0                 ; 6       ;
;      - incrementos:U9|INCe~29                 ; 0                 ; 6       ;
;      - amplitud:U7|amp6e~19                   ; 0                 ; 6       ;
;      - fase:U24|fase1e~9                      ; 0                 ; 6       ;
;      - fase:U24|fase1e~10                     ; 0                 ; 6       ;
;      - fase:U6|fase1e~9                       ; 0                 ; 6       ;
;      - fase:U6|fase1e~10                      ; 0                 ; 6       ;
;      - fase:U24|fase2e~10                     ; 0                 ; 6       ;
;      - fase:U24|fase2e~11                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~12                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~13                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~16                     ; 0                 ; 6       ;
;      - fase:U24|fase5e~17                     ; 0                 ; 6       ;
;      - fase:U6|fase2e~10                      ; 0                 ; 6       ;
;      - fase:U6|fase2e~11                      ; 0                 ; 6       ;
;      - fase:U6|fase7e~16                      ; 0                 ; 6       ;
;      - fase:U6|fase7e~17                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~12                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~13                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~16                      ; 0                 ; 6       ;
;      - fase:U6|fase5e~17                      ; 0                 ; 6       ;
;      - fase:U6|fase7e~42                      ; 0                 ; 6       ;
;      - fase:U24|fase7e~37                     ; 0                 ; 6       ;
;      - LED_inst[0]~output                     ; 0                 ; 6       ;
; num_inst[1]                                   ;                   ;         ;
;      - amplitud:U25|amp9e[1]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp9e[2]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp12e[1]                 ; 1                 ; 6       ;
;      - amplitud:U25|amp8e[2]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp8e[3]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp3e[6]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp2e[6]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp7e[4]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp6e[3]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp5e[4]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[4]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[5]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[6]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp11e[2]                 ; 1                 ; 6       ;
;      - amplitud:U25|amp11e[3]                 ; 1                 ; 6       ;
;      - amplitud:U7|amp9e[1]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp9e[2]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp12e[1]                  ; 1                 ; 6       ;
;      - amplitud:U7|amp8e[2]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp8e[3]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp3e[6]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp2e[6]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp7e[4]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp6e[3]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp5e[4]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[4]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[5]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[6]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp11e[2]                  ; 1                 ; 6       ;
;      - amplitud:U7|amp11e[3]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp9e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp8e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U7|amp9e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp8e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U25|amp10e[0]                 ; 1                 ; 6       ;
;      - amplitud:U25|amp1e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp1e[2]~1                ; 1                 ; 6       ;
;      - amplitud:U25|amp1e[3]~2                ; 1                 ; 6       ;
;      - amplitud:U25|amp1e[5]~4                ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde[7]~0             ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde[5]~2             ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde[3]~4             ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde[2]~5             ; 1                 ; 6       ;
;      - amplitud:U25|amp3e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp3e[5]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp2e[5]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp2e[4]~1                ; 1                 ; 6       ;
;      - amplitud:U25|amp2e[0]~3                ; 1                 ; 6       ;
;      - amplitud:U25|amp6e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp6e[1]~1                ; 1                 ; 6       ;
;      - amplitud:U25|amp5e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp5e[1]~1                ; 1                 ; 6       ;
;      - amplitud:U25|amp5e[2]~2                ; 1                 ; 6       ;
;      - amplitud:U25|amp5e[3]                  ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[0]~0                ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[1]~1                ; 1                 ; 6       ;
;      - amplitud:U25|amp4e[3]~3                ; 1                 ; 6       ;
;      - amplitud:U7|amp10e[0]                  ; 1                 ; 6       ;
;      - amplitud:U7|amp1e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp1e[2]~1                 ; 1                 ; 6       ;
;      - amplitud:U7|amp1e[3]~2                 ; 1                 ; 6       ;
;      - amplitud:U7|amp1e[5]~4                 ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde[7]~0              ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde[5]~2              ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde[3]~4              ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde[2]~5              ; 1                 ; 6       ;
;      - amplitud:U7|amp3e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp3e[5]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp2e[5]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp2e[4]~1                 ; 1                 ; 6       ;
;      - amplitud:U7|amp2e[0]~3                 ; 1                 ; 6       ;
;      - amplitud:U7|amp6e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp6e[1]~1                 ; 1                 ; 6       ;
;      - amplitud:U7|amp5e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp5e[1]~1                 ; 1                 ; 6       ;
;      - amplitud:U7|amp5e[2]~2                 ; 1                 ; 6       ;
;      - amplitud:U7|amp5e[3]                   ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[0]~0                 ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[1]~1                 ; 1                 ; 6       ;
;      - amplitud:U7|amp4e[3]~3                 ; 1                 ; 6       ;
;      - fase:U24|fase11e[0]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase4e[0]~0                   ; 1                 ; 6       ;
;      - fase:U24|fase13e[0]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase17e[0]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[8]~0                   ; 1                 ; 6       ;
;      - fase:U24|fase12e[8]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase1e[8]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase16e[8]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase6e[7]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase14e[7]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase1e[7]~2                   ; 1                 ; 6       ;
;      - fase:U24|fase13e[7]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase4e[7]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase8e[7]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase11e[7]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase15e[7]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase17e[7]~1                  ; 1                 ; 6       ;
;      - fase:U24|fase18e[7]~0                  ; 1                 ; 6       ;
;      - fase:U24|fase10e[4]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase2e[4]~2                   ; 1                 ; 6       ;
;      - fase:U24|fase14e[4]~1                  ; 1                 ; 6       ;
;      - fase:U24|fase5e[4]~0                   ; 1                 ; 6       ;
;      - fase:U24|fase11e[4]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[4]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase17e[4]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase16e[4]~1                  ; 1                 ; 6       ;
;      - fase:U24|fase10e[5]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[5]~2                   ; 1                 ; 6       ;
;      - fase:U24|fase11e[5]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase5e[5]~1                   ; 1                 ; 6       ;
;      - fase:U24|fase13e[5]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase1e[5]~3                   ; 1                 ; 6       ;
;      - fase:U24|fase9e[5]~2                   ; 1                 ; 6       ;
;      - fase:U24|fase7e[5]~3                   ; 1                 ; 6       ;
;      - fase:U24|fase18e[5]~1                  ; 1                 ; 6       ;
;      - fase:U24|fase16e[5]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[3]~3                   ; 1                 ; 6       ;
;      - fase:U24|fase7e[3]~4                   ; 1                 ; 6       ;
;      - fase:U24|fase9e[3]~3                   ; 1                 ; 6       ;
;      - fase:U24|fase13e[3]~5                  ; 1                 ; 6       ;
;      - fase:U24|fase5e[3]~2                   ; 1                 ; 6       ;
;      - fase:U24|fase11e[3]~5                  ; 1                 ; 6       ;
;      - fase:U24|fase14e[3]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase17e[3]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase18e[3]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase12e[2]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase14e[2]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[2]~4                   ; 1                 ; 6       ;
;      - fase:U24|fase9e[2]~4                   ; 1                 ; 6       ;
;      - fase:U24|fase1e[2]~4                   ; 1                 ; 6       ;
;      - fase:U24|fase10e[2]~5                  ; 1                 ; 6       ;
;      - fase:U24|fase13e[2]~6                  ; 1                 ; 6       ;
;      - fase:U24|fase15e[2]~2                  ; 1                 ; 6       ;
;      - fase:U24|fase18e[2]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase16e[2]~3                  ; 1                 ; 6       ;
;      - fase:U24|fase19e[2]~1                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[6]~5                   ; 1                 ; 6       ;
;      - fase:U24|fase6e[6]~5                   ; 1                 ; 6       ;
;      - fase:U24|fase9e[6]~5                   ; 1                 ; 6       ;
;      - fase:U24|fase4e[6]~4                   ; 1                 ; 6       ;
;      - fase:U24|fase18e[6]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase17e[6]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase16e[6]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase3e[1]~6                   ; 1                 ; 6       ;
;      - fase:U24|fase9e[1]~6                   ; 1                 ; 6       ;
;      - fase:U24|fase12e[1]~4                  ; 1                 ; 6       ;
;      - fase:U24|fase8e[1]~5                   ; 1                 ; 6       ;
;      - fase:U24|fase13e[1]~7                  ; 1                 ; 6       ;
;      - fase:U24|fase4e[1]~5                   ; 1                 ; 6       ;
;      - fase:U24|fase14e[1]~5                  ; 1                 ; 6       ;
;      - fase:U24|fase11e[1]~7                  ; 1                 ; 6       ;
;      - fase:U24|fase10e[1]~7                  ; 1                 ; 6       ;
;      - fase:U24|fase17e[1]~5                  ; 1                 ; 6       ;
;      - fase:U24|fase16e[1]~5                  ; 1                 ; 6       ;
;      - fase:U6|fase13e[0]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase4e[0]~0                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[0]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase17e[0]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase3e[8]~0                    ; 1                 ; 6       ;
;      - fase:U6|fase12e[8]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase1e[8]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase16e[8]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase6e[7]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase4e[7]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase14e[7]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase1e[7]~2                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[7]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase8e[7]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase13e[7]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase15e[7]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase18e[7]~0                   ; 1                 ; 6       ;
;      - fase:U6|fase17e[7]~1                   ; 1                 ; 6       ;
;      - fase:U6|fase3e[4]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase2e[4]~2                    ; 1                 ; 6       ;
;      - fase:U6|fase5e[4]~0                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[4]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase14e[4]~1                   ; 1                 ; 6       ;
;      - fase:U6|fase10e[4]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase17e[4]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase16e[4]~1                   ; 1                 ; 6       ;
;      - fase:U6|fase9e[5]~2                    ; 1                 ; 6       ;
;      - fase:U6|fase3e[5]~2                    ; 1                 ; 6       ;
;      - fase:U6|fase1e[5]~3                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[5]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase10e[5]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase13e[5]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase7e[5]~3                    ; 1                 ; 6       ;
;      - fase:U6|fase5e[5]~1                    ; 1                 ; 6       ;
;      - fase:U6|fase18e[5]~1                   ; 1                 ; 6       ;
;      - fase:U6|fase16e[5]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase14e[3]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase3e[3]~3                    ; 1                 ; 6       ;
;      - fase:U6|fase9e[3]~3                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[3]~5                   ; 1                 ; 6       ;
;      - fase:U6|fase7e[3]~4                    ; 1                 ; 6       ;
;      - fase:U6|fase13e[3]~5                   ; 1                 ; 6       ;
;      - fase:U6|fase5e[3]~2                    ; 1                 ; 6       ;
;      - fase:U6|fase18e[3]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase17e[3]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase9e[2]~4                    ; 1                 ; 6       ;
;      - fase:U6|fase12e[2]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase13e[2]~6                   ; 1                 ; 6       ;
;      - fase:U6|fase3e[2]~4                    ; 1                 ; 6       ;
;      - fase:U6|fase1e[2]~4                    ; 1                 ; 6       ;
;      - fase:U6|fase14e[2]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase10e[2]~5                   ; 1                 ; 6       ;
;      - fase:U6|fase15e[2]~2                   ; 1                 ; 6       ;
;      - fase:U6|fase18e[2]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase16e[2]~3                   ; 1                 ; 6       ;
;      - fase:U6|fase19e[2]~1                   ; 1                 ; 6       ;
;      - fase:U6|fase9e[6]~5                    ; 1                 ; 6       ;
;      - fase:U6|fase6e[6]~5                    ; 1                 ; 6       ;
;      - fase:U6|fase3e[6]~5                    ; 1                 ; 6       ;
;      - fase:U6|fase4e[6]~4                    ; 1                 ; 6       ;
;      - fase:U6|fase17e[6]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase18e[6]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase16e[6]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase9e[1]~6                    ; 1                 ; 6       ;
;      - fase:U6|fase3e[1]~6                    ; 1                 ; 6       ;
;      - fase:U6|fase11e[1]~7                   ; 1                 ; 6       ;
;      - fase:U6|fase12e[1]~4                   ; 1                 ; 6       ;
;      - fase:U6|fase4e[1]~5                    ; 1                 ; 6       ;
;      - fase:U6|fase14e[1]~5                   ; 1                 ; 6       ;
;      - fase:U6|fase8e[1]~5                    ; 1                 ; 6       ;
;      - fase:U6|fase10e[1]~7                   ; 1                 ; 6       ;
;      - fase:U6|fase13e[1]~7                   ; 1                 ; 6       ;
;      - fase:U6|fase17e[1]~5                   ; 1                 ; 6       ;
;      - fase:U6|fase16e[1]~5                   ; 1                 ; 6       ;
;      - incrementos:U26|INCe[9]~0              ; 1                 ; 6       ;
;      - incrementos:U26|INCe[10]~1             ; 1                 ; 6       ;
;      - incrementos:U26|INCe[8]~2              ; 1                 ; 6       ;
;      - incrementos:U26|INCe[3]~3              ; 1                 ; 6       ;
;      - incrementos:U26|INCe[6]~4              ; 1                 ; 6       ;
;      - incrementos:U26|INCe[7]~5              ; 1                 ; 6       ;
;      - incrementos:U26|INCe[11]~6             ; 1                 ; 6       ;
;      - incrementos:U26|INCe[12]~7             ; 1                 ; 6       ;
;      - incrementos:U9|INCe[9]~0               ; 1                 ; 6       ;
;      - incrementos:U9|INCe[8]~1               ; 1                 ; 6       ;
;      - incrementos:U9|INCe[10]~2              ; 1                 ; 6       ;
;      - incrementos:U9|INCe[11]~3              ; 1                 ; 6       ;
;      - incrementos:U9|INCe[3]~4               ; 1                 ; 6       ;
;      - incrementos:U9|INCe[6]~5               ; 1                 ; 6       ;
;      - incrementos:U9|INCe[7]~6               ; 1                 ; 6       ;
;      - incrementos:U9|INCe[12]~7              ; 1                 ; 6       ;
;      - amplitud:U7|Equal1~0                   ; 1                 ; 6       ;
;      - amplitud:U25|amp10e~7                  ; 1                 ; 6       ;
;      - amplitud:U25|amp12e~5                  ; 1                 ; 6       ;
;      - amplitud:U25|amp10e~9                  ; 1                 ; 6       ;
;      - amplitud:U25|amp12e~6                  ; 1                 ; 6       ;
;      - amplitud:U7|amp10e~7                   ; 1                 ; 6       ;
;      - amplitud:U7|amp10e~9                   ; 1                 ; 6       ;
;      - amplitud:U7|amp12e~5                   ; 1                 ; 6       ;
;      - amplitud:U25|amp13e~2                  ; 1                 ; 6       ;
;      - amplitud:U25|amp15e~0                  ; 1                 ; 6       ;
;      - amplitud:U25|amp15e~1                  ; 1                 ; 6       ;
;      - fase:U24|fase15e[6]~7                  ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~12               ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~13               ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~15               ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~17               ; 1                 ; 6       ;
;      - amplitud:U25|amp2e~4                   ; 1                 ; 6       ;
;      - amplitud:U25|amp2e~5                   ; 1                 ; 6       ;
;      - amplitud:U25|amp7e~5                   ; 1                 ; 6       ;
;      - amplitud:U25|amp8e~1                   ; 1                 ; 6       ;
;      - amplitud:U25|amp8e~2                   ; 1                 ; 6       ;
;      - amplitud:U7|amp13e~2                   ; 1                 ; 6       ;
;      - amplitud:U7|amp15e~0                   ; 1                 ; 6       ;
;      - amplitud:U7|amp15e~1                   ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde~12                ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde~13                ; 1                 ; 6       ;
;      - amplitud:U7|amp2e~4                    ; 1                 ; 6       ;
;      - amplitud:U7|amp7e~5                    ; 1                 ; 6       ;
;      - amplitud:U7|amp8e~1                    ; 1                 ; 6       ;
;      - amplitud:U7|amp8e~2                    ; 1                 ; 6       ;
;      - amplitud:U25|amp1e~18                  ; 1                 ; 6       ;
;      - amplitud:U25|Mux9~0                    ; 1                 ; 6       ;
;      - amplitud:U25|Mux9~1                    ; 1                 ; 6       ;
;      - amplitud:U25|amp3e~14                  ; 1                 ; 6       ;
;      - amplitud:U25|amp3e~15                  ; 1                 ; 6       ;
;      - amplitud:U25|amp2e~7                   ; 1                 ; 6       ;
;      - amplitud:U25|amp2e~16                  ; 1                 ; 6       ;
;      - amplitud:U25|amp2e~18                  ; 1                 ; 6       ;
;      - amplitud:U25|amp6e~9                   ; 1                 ; 6       ;
;      - amplitud:U25|amp6e~11                  ; 1                 ; 6       ;
;      - amplitud:U25|amp6e~12                  ; 1                 ; 6       ;
;      - amplitud:U25|amp7e~7                   ; 1                 ; 6       ;
;      - amplitud:U25|amp4e~12                  ; 1                 ; 6       ;
;      - amplitud:U7|amp1e~18                   ; 1                 ; 6       ;
;      - amplitud:U7|Mux9~0                     ; 1                 ; 6       ;
;      - amplitud:U7|Mux9~1                     ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde~26                ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde~28                ; 1                 ; 6       ;
;      - amplitud:U7|amp3e~14                   ; 1                 ; 6       ;
;      - amplitud:U7|amp3e~15                   ; 1                 ; 6       ;
;      - amplitud:U7|amp2e~7                    ; 1                 ; 6       ;
;      - amplitud:U7|amp2e~16                   ; 1                 ; 6       ;
;      - amplitud:U7|amp2e~17                   ; 1                 ; 6       ;
;      - amplitud:U7|amp6e~12                   ; 1                 ; 6       ;
;      - amplitud:U7|amp6e~14                   ; 1                 ; 6       ;
;      - amplitud:U7|amp7e~7                    ; 1                 ; 6       ;
;      - amplitud:U7|amp4e~12                   ; 1                 ; 6       ;
;      - fase:U24|fase18e~18                    ; 1                 ; 6       ;
;      - fase:U24|fase16e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase16e~17                    ; 1                 ; 6       ;
;      - fase:U24|fase19e~2                     ; 1                 ; 6       ;
;      - fase:U24|fase19e~3                     ; 1                 ; 6       ;
;      - fase:U24|Mux164~0                      ; 1                 ; 6       ;
;      - fase:U24|Mux164~1                      ; 1                 ; 6       ;
;      - fase:U24|fase19e~10                    ; 1                 ; 6       ;
;      - fase:U24|fase19e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase6e~22                     ; 1                 ; 6       ;
;      - fase:U24|fase6e~23                     ; 1                 ; 6       ;
;      - fase:U24|Mux53~0                       ; 1                 ; 6       ;
;      - fase:U24|Mux53~1                       ; 1                 ; 6       ;
;      - fase:U24|fase10e~13                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~14                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~17                    ; 1                 ; 6       ;
;      - fase:U24|Mux11~0                       ; 1                 ; 6       ;
;      - fase:U24|Mux11~1                       ; 1                 ; 6       ;
;      - fase:U24|fase2e~21                     ; 1                 ; 6       ;
;      - fase:U24|fase2e~22                     ; 1                 ; 6       ;
;      - fase:U24|fase2e~27                     ; 1                 ; 6       ;
;      - fase:U24|fase14e~10                    ; 1                 ; 6       ;
;      - fase:U24|fase14e~11                    ; 1                 ; 6       ;
;      - fase:U24|fase5e~22                     ; 1                 ; 6       ;
;      - fase:U24|fase5e~23                     ; 1                 ; 6       ;
;      - fase:U24|Mux42~0                       ; 1                 ; 6       ;
;      - fase:U24|Mux42~1                       ; 1                 ; 6       ;
;      - fase:U24|fase9e~14                     ; 1                 ; 6       ;
;      - fase:U24|fase9e~26                     ; 1                 ; 6       ;
;      - fase:U24|fase9e~27                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~13                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~17                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~25                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~26                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~31                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~32                     ; 1                 ; 6       ;
;      - fase:U24|fase13e~8                     ; 1                 ; 6       ;
;      - fase:U24|fase13e~9                     ; 1                 ; 6       ;
;      - fase:U24|Mux112~0                      ; 1                 ; 6       ;
;      - fase:U24|Mux112~1                      ; 1                 ; 6       ;
;      - fase:U24|fase4e~19                     ; 1                 ; 6       ;
;      - fase:U24|fase4e~20                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~18                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~20                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~25                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~26                     ; 1                 ; 6       ;
;      - fase:U24|Mux68~1                       ; 1                 ; 6       ;
;      - fase:U24|Mux68~2                       ; 1                 ; 6       ;
;      - fase:U24|fase8e~28                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~33                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~34                     ; 1                 ; 6       ;
;      - fase:U24|fase12e~10                    ; 1                 ; 6       ;
;      - fase:U24|fase12e~11                    ; 1                 ; 6       ;
;      - fase:U24|fase12e~14                    ; 1                 ; 6       ;
;      - fase:U24|fase12e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase12e~25                    ; 1                 ; 6       ;
;      - fase:U24|fase12e~26                    ; 1                 ; 6       ;
;      - fase:U24|fase7e~28                     ; 1                 ; 6       ;
;      - fase:U24|fase7e~29                     ; 1                 ; 6       ;
;      - fase:U24|fase11e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase3e~32                     ; 1                 ; 6       ;
;      - fase:U24|fase3e~33                     ; 1                 ; 6       ;
;      - fase:U24|fase15e~14                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~15                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~16                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~17                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~22                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~23                    ; 1                 ; 6       ;
;      - fase:U24|fase18e~19                    ; 1                 ; 6       ;
;      - fase:U24|fase18e~20                    ; 1                 ; 6       ;
;      - fase:U24|fase17e~15                    ; 1                 ; 6       ;
;      - fase:U24|fase17e~17                    ; 1                 ; 6       ;
;      - fase:U24|fase19e~17                    ; 1                 ; 6       ;
;      - fase:U24|fase19e~18                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~33                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~35                    ; 1                 ; 6       ;
;      - fase:U24|Mux108~0                      ; 1                 ; 6       ;
;      - fase:U24|Mux108~1                      ; 1                 ; 6       ;
;      - fase:U24|fase8e~37                     ; 1                 ; 6       ;
;      - fase:U24|fase9e~29                     ; 1                 ; 6       ;
;      - fase:U24|fase9e~30                     ; 1                 ; 6       ;
;      - fase:U24|Mux54~0                       ; 1                 ; 6       ;
;      - fase:U24|Mux54~1                       ; 1                 ; 6       ;
;      - fase:U24|fase6e~28                     ; 1                 ; 6       ;
;      - fase:U24|fase15e~25                    ; 1                 ; 6       ;
;      - fase:U24|fase15e~26                    ; 1                 ; 6       ;
;      - fase:U6|fase18e~18                     ; 1                 ; 6       ;
;      - fase:U6|Mux147~0                       ; 1                 ; 6       ;
;      - fase:U6|fase16e~16                     ; 1                 ; 6       ;
;      - fase:U6|fase16e~17                     ; 1                 ; 6       ;
;      - fase:U6|Mux164~0                       ; 1                 ; 6       ;
;      - fase:U6|Mux164~1                       ; 1                 ; 6       ;
;      - fase:U6|fase19e~12                     ; 1                 ; 6       ;
;      - fase:U6|fase19e~18                     ; 1                 ; 6       ;
;      - fase:U6|fase6e~22                      ; 1                 ; 6       ;
;      - fase:U6|fase6e~23                      ; 1                 ; 6       ;
;      - fase:U6|Mux53~0                        ; 1                 ; 6       ;
;      - fase:U6|Mux53~1                        ; 1                 ; 6       ;
;      - fase:U6|fase12e~9                      ; 1                 ; 6       ;
;      - fase:U6|fase12e~10                     ; 1                 ; 6       ;
;      - fase:U6|fase12e~13                     ; 1                 ; 6       ;
;      - fase:U6|fase12e~15                     ; 1                 ; 6       ;
;      - fase:U6|fase12e~24                     ; 1                 ; 6       ;
;      - fase:U6|fase12e~25                     ; 1                 ; 6       ;
;      - fase:U6|fase14e~10                     ; 1                 ; 6       ;
;      - fase:U6|fase14e~11                     ; 1                 ; 6       ;
;      - fase:U6|fase3e~31                      ; 1                 ; 6       ;
;      - fase:U6|fase3e~33                      ; 1                 ; 6       ;
;      - fase:U6|fase9e~18                      ; 1                 ; 6       ;
;      - fase:U6|fase9e~30                      ; 1                 ; 6       ;
;      - fase:U6|fase9e~31                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~13                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~17                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~25                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~26                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~31                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~32                      ; 1                 ; 6       ;
;      - fase:U6|fase11e~16                     ; 1                 ; 6       ;
;      - fase:U6|Mux11~0                        ; 1                 ; 6       ;
;      - fase:U6|Mux11~1                        ; 1                 ; 6       ;
;      - fase:U6|fase2e~22                      ; 1                 ; 6       ;
;      - fase:U6|fase2e~23                      ; 1                 ; 6       ;
;      - fase:U6|fase2e~28                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~18                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~19                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~24                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~25                      ; 1                 ; 6       ;
;      - fase:U6|Mux68~1                        ; 1                 ; 6       ;
;      - fase:U6|Mux68~2                        ; 1                 ; 6       ;
;      - fase:U6|fase8e~27                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~32                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~33                      ; 1                 ; 6       ;
;      - fase:U6|fase10e~17                     ; 1                 ; 6       ;
;      - fase:U6|fase10e~18                     ; 1                 ; 6       ;
;      - fase:U6|fase10e~20                     ; 1                 ; 6       ;
;      - fase:U6|fase10e~21                     ; 1                 ; 6       ;
;      - fase:U6|fase7e~31                      ; 1                 ; 6       ;
;      - fase:U6|fase7e~32                      ; 1                 ; 6       ;
;      - fase:U6|fase13e~8                      ; 1                 ; 6       ;
;      - fase:U6|fase13e~9                      ; 1                 ; 6       ;
;      - fase:U6|Mux112~0                       ; 1                 ; 6       ;
;      - fase:U6|Mux112~1                       ; 1                 ; 6       ;
;      - fase:U6|fase5e~22                      ; 1                 ; 6       ;
;      - fase:U6|fase5e~23                      ; 1                 ; 6       ;
;      - fase:U6|Mux42~0                        ; 1                 ; 6       ;
;      - fase:U6|Mux42~1                        ; 1                 ; 6       ;
;      - fase:U6|fase15e~13                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~14                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~15                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~16                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~21                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~22                     ; 1                 ; 6       ;
;      - fase:U6|fase17e~15                     ; 1                 ; 6       ;
;      - fase:U6|fase17e~17                     ; 1                 ; 6       ;
;      - fase:U6|fase18e~19                     ; 1                 ; 6       ;
;      - fase:U6|fase18e~20                     ; 1                 ; 6       ;
;      - fase:U6|fase19e~19                     ; 1                 ; 6       ;
;      - fase:U6|fase19e~20                     ; 1                 ; 6       ;
;      - fase:U6|fase6e~28                      ; 1                 ; 6       ;
;      - fase:U6|Mux54~0                        ; 1                 ; 6       ;
;      - fase:U6|Mux54~1                        ; 1                 ; 6       ;
;      - fase:U6|fase8e~36                      ; 1                 ; 6       ;
;      - fase:U6|Mux108~0                       ; 1                 ; 6       ;
;      - fase:U6|Mux108~1                       ; 1                 ; 6       ;
;      - fase:U6|fase15e~24                     ; 1                 ; 6       ;
;      - fase:U6|fase15e~25                     ; 1                 ; 6       ;
;      - incrementos:U26|INCe~21                ; 1                 ; 6       ;
;      - incrementos:U26|INCe~23                ; 1                 ; 6       ;
;      - incrementos:U26|INCe~27                ; 1                 ; 6       ;
;      - incrementos:U9|INCe~16                 ; 1                 ; 6       ;
;      - incrementos:U9|INCe~18                 ; 1                 ; 6       ;
;      - incrementos:U9|INCe~22                 ; 1                 ; 6       ;
;      - amplitud:U25|amp11e~5                  ; 1                 ; 6       ;
;      - amplitud:U25|amp10e~10                 ; 1                 ; 6       ;
;      - amplitud:U7|amp11e~5                   ; 1                 ; 6       ;
;      - amplitud:U7|amp10e~10                  ; 1                 ; 6       ;
;      - amplitud:U25|amp13e~3                  ; 1                 ; 6       ;
;      - amplitud:U25|amp12e~10                 ; 1                 ; 6       ;
;      - amplitud:U25|amp10e~11                 ; 1                 ; 6       ;
;      - amplitud:U25|amp11e~6                  ; 1                 ; 6       ;
;      - amplitud:U25|amp1e~35                  ; 1                 ; 6       ;
;      - amplitud:U25|amp1e~36                  ; 1                 ; 6       ;
;      - amplitud:U7|amp13e~3                   ; 1                 ; 6       ;
;      - amplitud:U7|amp12e~9                   ; 1                 ; 6       ;
;      - amplitud:U7|amp10e~11                  ; 1                 ; 6       ;
;      - amplitud:U7|amp11e~6                   ; 1                 ; 6       ;
;      - amplitud:U7|amp1e~34                   ; 1                 ; 6       ;
;      - amplitud:U7|amp1e~35                   ; 1                 ; 6       ;
;      - amplitud:U25|amp1e~37                  ; 1                 ; 6       ;
;      - amplitud:U25|amp7e~8                   ; 1                 ; 6       ;
;      - amplitud:U7|amp1e~36                   ; 1                 ; 6       ;
;      - amplitud:U7|amp7e~8                    ; 1                 ; 6       ;
;      - fase:U24|fase2e~33                     ; 1                 ; 6       ;
;      - fase:U24|fase5e~38                     ; 1                 ; 6       ;
;      - fase:U24|fase5e~39                     ; 1                 ; 6       ;
;      - fase:U24|fase1e~37                     ; 1                 ; 6       ;
;      - fase:U24|fase4e~33                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~38                     ; 1                 ; 6       ;
;      - fase:U24|fase7e~32                     ; 1                 ; 6       ;
;      - fase:U24|fase7e~33                     ; 1                 ; 6       ;
;      - fase:U24|fase4e~34                     ; 1                 ; 6       ;
;      - fase:U24|fase8e~39                     ; 1                 ; 6       ;
;      - fase:U24|fase14e~27                    ; 1                 ; 6       ;
;      - fase:U6|fase4e~34                      ; 1                 ; 6       ;
;      - fase:U6|fase1e~36                      ; 1                 ; 6       ;
;      - fase:U6|fase2e~32                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~37                      ; 1                 ; 6       ;
;      - fase:U6|fase7e~36                      ; 1                 ; 6       ;
;      - fase:U6|fase7e~37                      ; 1                 ; 6       ;
;      - fase:U6|fase5e~37                      ; 1                 ; 6       ;
;      - fase:U6|fase5e~38                      ; 1                 ; 6       ;
;      - fase:U6|fase8e~38                      ; 1                 ; 6       ;
;      - fase:U6|fase4e~35                      ; 1                 ; 6       ;
;      - fase:U6|fase14e~27                     ; 1                 ; 6       ;
;      - incrementos:U26|INCe~29                ; 1                 ; 6       ;
;      - incrementos:U9|INCe~29                 ; 1                 ; 6       ;
;      - fase:U24|fase9e~9                      ; 1                 ; 6       ;
;      - fase:U24|fase9e~10                     ; 1                 ; 6       ;
;      - fase:U6|fase9e~9                       ; 1                 ; 6       ;
;      - fase:U6|fase9e~10                      ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~8                ; 1                 ; 6       ;
;      - amplitud:U25|ampfunde~9                ; 1                 ; 6       ;
;      - fase:U24|fase16e~8                     ; 1                 ; 6       ;
;      - fase:U24|fase16e~9                     ; 1                 ; 6       ;
;      - fase:U24|fase10e~10                    ; 1                 ; 6       ;
;      - fase:U24|fase10e~11                    ; 1                 ; 6       ;
;      - fase:U24|fase7e~12                     ; 1                 ; 6       ;
;      - fase:U24|fase7e~13                     ; 1                 ; 6       ;
;      - fase:U24|fase3e~9                      ; 1                 ; 6       ;
;      - fase:U24|fase3e~10                     ; 1                 ; 6       ;
;      - fase:U24|fase15e~5                     ; 1                 ; 6       ;
;      - fase:U24|fase15e~6                     ; 1                 ; 6       ;
;      - fase:U24|fase5e~20                     ; 1                 ; 6       ;
;      - fase:U24|fase5e~21                     ; 1                 ; 6       ;
;      - fase:U6|fase16e~8                      ; 1                 ; 6       ;
;      - fase:U6|fase16e~9                      ; 1                 ; 6       ;
;      - fase:U6|fase19e~4                      ; 1                 ; 6       ;
;      - fase:U6|fase19e~5                      ; 1                 ; 6       ;
;      - fase:U6|fase4e~12                      ; 1                 ; 6       ;
;      - fase:U6|fase4e~13                      ; 1                 ; 6       ;
;      - fase:U6|fase3e~9                       ; 1                 ; 6       ;
;      - fase:U6|fase3e~10                      ; 1                 ; 6       ;
;      - fase:U6|fase10e~10                     ; 1                 ; 6       ;
;      - fase:U6|fase10e~11                     ; 1                 ; 6       ;
;      - fase:U6|fase7e~12                      ; 1                 ; 6       ;
;      - fase:U6|fase7e~13                      ; 1                 ; 6       ;
;      - fase:U6|fase15e~5                      ; 1                 ; 6       ;
;      - fase:U6|fase15e~6                      ; 1                 ; 6       ;
;      - fase:U6|fase9e~13                      ; 1                 ; 6       ;
;      - fase:U6|fase9e~14                      ; 1                 ; 6       ;
;      - fase:U6|fase5e~20                      ; 1                 ; 6       ;
;      - fase:U6|fase5e~21                      ; 1                 ; 6       ;
;      - fase:U24|fase6e~13                     ; 1                 ; 6       ;
;      - fase:U24|fase6e~14                     ; 1                 ; 6       ;
;      - fase:U24|fase12e~29                    ; 1                 ; 6       ;
;      - fase:U24|fase7e~16                     ; 1                 ; 6       ;
;      - fase:U24|fase7e~17                     ; 1                 ; 6       ;
;      - fase:U6|fase6e~13                      ; 1                 ; 6       ;
;      - fase:U6|fase6e~14                      ; 1                 ; 6       ;
;      - fase:U6|fase12e~28                     ; 1                 ; 6       ;
;      - fase:U6|fase7e~20                      ; 1                 ; 6       ;
;      - fase:U6|fase7e~21                      ; 1                 ; 6       ;
;      - fase:U6|fase10e~14                     ; 1                 ; 6       ;
;      - fase:U6|fase10e~15                     ; 1                 ; 6       ;
;      - fase:U6|fase6e~31                      ; 1                 ; 6       ;
;      - fase:U24|fase6e~31                     ; 1                 ; 6       ;
;      - fase:U24|Mux147~1                      ; 1                 ; 6       ;
;      - amplitud:U7|ampfunde~34                ; 1                 ; 6       ;
;      - LED_inst[1]~output                     ; 1                 ; 6       ;
; RST                                           ;                   ;         ;
;      - g00_audio_interface:U4|AUD_DACDAT      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|AUD_DACLRCK     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|AUD_BCLK        ; 0                 ; 6       ;
;      - g00_audio_interface:U4|AUD_MCLK        ; 0                 ; 6       ;
;      - g00_audio_interface:U4|pulse_48KHz     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|I2C_SCLK        ; 0                 ; 6       ;
;      - arm:U27|B12_1[4]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[5]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[6]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[7]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[8]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[9]                       ; 0                 ; 6       ;
;      - arm:U27|B12_1[10]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[11]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[12]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B12_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[3]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[4]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[5]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[6]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[7]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[8]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[9]                       ; 0                 ; 6       ;
;      - arm:U27|B10_1[10]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[11]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[12]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B10_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[3]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[4]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[5]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[6]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[7]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[8]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[9]                       ; 0                 ; 6       ;
;      - arm:U27|B18_1[10]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[11]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[12]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B18_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[4]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[5]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[6]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[7]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[8]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[9]                       ; 0                 ; 6       ;
;      - arm:U10|B12_1[10]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[11]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[12]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B12_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[3]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[4]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[5]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[6]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[7]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[8]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[9]                       ; 0                 ; 6       ;
;      - arm:U10|B10_1[10]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[11]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[12]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B10_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[3]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[4]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[5]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[6]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[7]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[8]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[9]                       ; 0                 ; 6       ;
;      - arm:U10|B18_1[10]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[11]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[12]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B18_1[19]                      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[13]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[29]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[21]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[20]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[12]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[19]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[11]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[18]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[10]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[17]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[33]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[16]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[24]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[32]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[25]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[14]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[22]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[31]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[15]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[23]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[30]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[0]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[1]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[2]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[3]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[4]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|clk_count[5]    ; 0                 ; 6       ;
;      - acum:U28|B3_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B4_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B2_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B8_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B10_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[11]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[11]                     ; 0                 ; 6       ;
;      - acum:U28|B10_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B4_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B8_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[19]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[19]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B10_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B2_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B4_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B8_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[18]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[18]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B10_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B2_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B4_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B8_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B11_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[15]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[15]                     ; 0                 ; 6       ;
;      - acum:U28|B10_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B12_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B8_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[16]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[16]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B8_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B1_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[14]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B14_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B10_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B15_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[14]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B4_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B2_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B8_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B10_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B5_2[13]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[13]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B8_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B1_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[17]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B11_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B10_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B15_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[17]                     ; 0                 ; 6       ;
;      - acum:U28|B6_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B8_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B1_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[12]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B11_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B10_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B15_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B17_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B16_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B19_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B3_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[11]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B14_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[11]                     ; 0                 ; 6       ;
;      - acum:U11|B3_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[19]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B14_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[19]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B3_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B2_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B7_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B5_2[18]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[18]                     ; 0                 ; 6       ;
;      - acum:U11|B3_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[15]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B14_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[15]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B2_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B13_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B7_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[16]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[16]                     ; 0                 ; 6       ;
;      - acum:U11|B12_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B3_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B8_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B7_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B5_2[14]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[14]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B8_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[13]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B11_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[13]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B8_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[17]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B11_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[17]                     ; 0                 ; 6       ;
;      - acum:U11|B9_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B6_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B4_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B2_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B13_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B7_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[12]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B17_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B16_2[12]                     ; 0                 ; 6       ;
;      - acum:U11|B19_2[12]                     ; 0                 ; 6       ;
;      - acum:U28|B3_2[10]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[12]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[10]                      ; 0                 ; 6       ;
;      - acum:U28|B1_2[10]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B13_1[12]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[10]                      ; 0                 ; 6       ;
;      - acum:U28|B12_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B19_1[13]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[10]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B11_1[13]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[10]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[12]                      ; 0                 ; 6       ;
;      - acum:U28|B8_2[10]                      ; 0                 ; 6       ;
;      - acum:U28|Bf_2[10]                      ; 0                 ; 6       ;
;      - acum:U28|B10_2[10]                     ; 0                 ; 6       ;
;      - acum:U28|B7_2[10]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B11_1[12]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[10]                      ; 0                 ; 6       ;
;      - acum:U28|B15_2[10]                     ; 0                 ; 6       ;
;      - acum:U28|B18_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B17_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B17_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B16_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B16_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B19_1[11]                      ; 0                 ; 6       ;
;      - acum:U28|B19_2[10]                     ; 0                 ; 6       ;
;      - arm:U27|B13_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B6_1[19]                       ; 0                 ; 6       ;
;      - arm:U27|B17_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[19]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[18]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[15]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[16]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B11_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[14]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B13_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[13]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[17]                      ; 0                 ; 6       ;
;      - arm:U27|B14_1[12]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[12]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[12]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[13]                      ; 0                 ; 6       ;
;      - acum:U11|B2_2[10]                      ; 0                 ; 6       ;
;      - acum:U11|B7_2[10]                      ; 0                 ; 6       ;
;      - acum:U11|B12_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B19_1[12]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[12]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B19_1[13]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[10]                      ; 0                 ; 6       ;
;      - acum:U11|B1_2[10]                      ; 0                 ; 6       ;
;      - acum:U11|Bf_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[12]                      ; 0                 ; 6       ;
;      - acum:U11|B5_2[10]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B14_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[10]                     ; 0                 ; 6       ;
;      - acum:U11|B10_2[10]                     ; 0                 ; 6       ;
;      - acum:U11|B15_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B17_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B17_2[10]                     ; 0                 ; 6       ;
;      - acum:U11|B18_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B16_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B16_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B19_1[11]                      ; 0                 ; 6       ;
;      - acum:U11|B19_2[10]                     ; 0                 ; 6       ;
;      - arm:U10|B6_1[19]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[19]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[18]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[15]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[16]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B11_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[14]                      ; 0                 ; 6       ;
;      - arm:U10|B13_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[13]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[17]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[12]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[12]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[9]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B11_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[9]                       ; 0                 ; 6       ;
;      - arm:U27|B14_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B14_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[9]                       ; 0                 ; 6       ;
;      - arm:U27|B13_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[9]                       ; 0                 ; 6       ;
;      - acum:U28|B15_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B18_2[9]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B17_2[9]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B16_2[9]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[10]                      ; 0                 ; 6       ;
;      - acum:U28|B19_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B7_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[9]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B13_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[9]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[9]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B11_2[9]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[9]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B17_2[9]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[9]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B16_2[9]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[10]                      ; 0                 ; 6       ;
;      - acum:U11|B19_2[9]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[8]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B11_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[8]                       ; 0                 ; 6       ;
;      - arm:U27|B14_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[8]                       ; 0                 ; 6       ;
;      - arm:U27|B13_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B13_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[8]                       ; 0                 ; 6       ;
;      - acum:U28|B15_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B18_2[8]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B17_2[8]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B16_2[8]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[9]                       ; 0                 ; 6       ;
;      - acum:U28|B19_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B7_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[8]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[8]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[8]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B11_2[8]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[8]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B17_2[8]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[8]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B16_2[8]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[9]                       ; 0                 ; 6       ;
;      - acum:U11|B19_2[8]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[7]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B11_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[7]                       ; 0                 ; 6       ;
;      - arm:U27|B14_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[7]                       ; 0                 ; 6       ;
;      - arm:U27|B13_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B13_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[7]                       ; 0                 ; 6       ;
;      - acum:U28|B15_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B18_2[7]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B17_2[7]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B16_2[7]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[8]                       ; 0                 ; 6       ;
;      - acum:U28|B19_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B7_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[7]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[7]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[7]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B11_2[7]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[7]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B17_2[7]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[7]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B16_2[7]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[8]                       ; 0                 ; 6       ;
;      - acum:U11|B19_2[7]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[6]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B11_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[6]                       ; 0                 ; 6       ;
;      - arm:U27|B14_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[6]                       ; 0                 ; 6       ;
;      - arm:U27|B13_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B13_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[6]                       ; 0                 ; 6       ;
;      - acum:U28|B15_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B18_2[6]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B17_2[6]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B16_2[6]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[7]                       ; 0                 ; 6       ;
;      - acum:U28|B19_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B7_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[6]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[6]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[6]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B11_2[6]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B15_2[6]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B17_2[6]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[6]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B16_2[6]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[7]                       ; 0                 ; 6       ;
;      - acum:U11|B19_2[6]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[5]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B11_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[5]                       ; 0                 ; 6       ;
;      - arm:U27|B14_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B7_2[5]                       ; 0                 ; 6       ;
;      - arm:U27|B13_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B13_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[5]                       ; 0                 ; 6       ;
;      - acum:U28|B18_2[5]                      ; 0                 ; 6       ;
;      - arm:U27|B17_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B17_2[5]                      ; 0                 ; 6       ;
;      - arm:U27|B16_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B16_2[5]                      ; 0                 ; 6       ;
;      - arm:U27|B19_1[6]                       ; 0                 ; 6       ;
;      - acum:U28|B19_2[5]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B7_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[5]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[5]                       ; 0                 ; 6       ;
;      - arm:U10|B13_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[5]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[5]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[5]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B11_2[5]                      ; 0                 ; 6       ;
;      - arm:U10|B14_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[5]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[5]                      ; 0                 ; 6       ;
;      - arm:U10|B17_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B17_2[5]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[5]                      ; 0                 ; 6       ;
;      - arm:U10|B16_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B16_2[5]                      ; 0                 ; 6       ;
;      - arm:U10|B19_1[6]                       ; 0                 ; 6       ;
;      - acum:U11|B19_2[5]                      ; 0                 ; 6       ;
;      - acum:U28|B3_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B9_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[4]                       ; 0                 ; 6       ;
;      - arm:U27|B11_1[5]                       ; 0                 ; 6       ;
;      - acum:U28|B11_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[4]                       ; 0                 ; 6       ;
;      - acum:U28|B18_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B17_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B16_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B19_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B3_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B6_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[4]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[4]                       ; 0                 ; 6       ;
;      - arm:U10|B11_1[5]                       ; 0                 ; 6       ;
;      - acum:U11|B11_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B14_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B17_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B16_2[4]                      ; 0                 ; 6       ;
;      - acum:U11|B19_2[4]                      ; 0                 ; 6       ;
;      - acum:U28|B9_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B1_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B6_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B13_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B5_2[3]                       ; 0                 ; 6       ;
;      - acum:U28|B18_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B17_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B16_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B9_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B8_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B13_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B4_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B1_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B5_2[3]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B17_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[3]                      ; 0                 ; 6       ;
;      - acum:U11|B16_2[3]                      ; 0                 ; 6       ;
;      - acum:U28|B6_2[2]                       ; 0                 ; 6       ;
;      - acum:U28|B12_2[2]                      ; 0                 ; 6       ;
;      - acum:U28|B4_2[2]                       ; 0                 ; 6       ;
;      - acum:U28|B14_2[2]                      ; 0                 ; 6       ;
;      - acum:U28|B2_2[2]                       ; 0                 ; 6       ;
;      - acum:U28|B8_2[2]                       ; 0                 ; 6       ;
;      - acum:U28|Bf_2[2]                       ; 0                 ; 6       ;
;      - acum:U28|B10_2[2]                      ; 0                 ; 6       ;
;      - acum:U28|B18_2[2]                      ; 0                 ; 6       ;
;      - acum:U28|B16_2[2]                      ; 0                 ; 6       ;
;      - acum:U11|B6_2[2]                       ; 0                 ; 6       ;
;      - acum:U11|B2_2[2]                       ; 0                 ; 6       ;
;      - acum:U11|B12_2[2]                      ; 0                 ; 6       ;
;      - acum:U11|B8_2[2]                       ; 0                 ; 6       ;
;      - acum:U11|B4_2[2]                       ; 0                 ; 6       ;
;      - acum:U11|Bf_2[2]                       ; 0                 ; 6       ;
;      - acum:U11|B14_2[2]                      ; 0                 ; 6       ;
;      - acum:U11|B10_2[2]                      ; 0                 ; 6       ;
;      - acum:U11|B18_2[2]                      ; 0                 ; 6       ;
;      - acum:U11|B16_2[2]                      ; 0                 ; 6       ;
;      - LED3:U43|inter2~0                      ; 0                 ; 6       ;
;      - LED3:U43|inter2~1                      ; 0                 ; 6       ;
;      - divisor1:U1|sint                       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[0]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[5]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[3]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[2]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[1]      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|BBcount[4]      ; 0                 ; 6       ;
;      - divisor2:U2|sint                       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Mcount          ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Bcount[2]       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Bcount[1]       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Bcount[0]       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|I2C_SDAT~reg0   ; 0                 ; 6       ;
;      - g00_audio_interface:U4|I2C_SDAT~en     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.s1        ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.s0        ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw_init1  ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw_init0  ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.send      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack12    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack22    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack32    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sab2      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw1b2     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw2b2     ; 0                 ; 6       ;
;      - divisor1:U1|Qint[10]                   ; 0                 ; 6       ;
;      - divisor1:U1|Qint[9]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[8]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[7]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[4]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[6]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[5]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[3]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[0]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[2]                    ; 0                 ; 6       ;
;      - divisor1:U1|Qint[1]                    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw2b1     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw2b3     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|bit_count[0]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|bit_count[1]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|bit_count[2]    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sab1      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sab3      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw1b1     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sw1b3     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack21    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack31    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack11    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack13    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack23    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.sack33    ; 0                 ; 6       ;
;      - g00_audio_interface:U4|SCI_WRITE       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state.s2        ; 0                 ; 6       ;
;      - divisor3:U3|sint                       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|word_count[0]   ; 0                 ; 6       ;
;      - g00_audio_interface:U4|word_count[2]   ; 0                 ; 6       ;
;      - g00_audio_interface:U4|word_count[1]   ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state2.sw_write ; 0                 ; 6       ;
;      - g00_audio_interface:U4|word_count[3]   ; 0                 ; 6       ;
;      - g00_audio_interface:U4|SCI_WORD1[4]~0  ; 0                 ; 6       ;
;      - divisor3:U3|Qint[10]                   ; 0                 ; 6       ;
;      - divisor3:U3|Qint[9]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[8]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[5]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[4]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[7]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[6]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[3]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[2]                    ; 0                 ; 6       ;
;      - divisor3:U3|Qint[1]                    ; 0                 ; 6       ;
;      - control:U8|Qint[4]~15                  ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state2.sw_init1 ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state2.sw_ready ; 0                 ; 6       ;
;      - g00_audio_interface:U4|SCI_READY       ; 0                 ; 6       ;
;      - g00_audio_interface:U4|state2.sw_init0 ; 0                 ; 6       ;
;      - arm:U27|B16_1~14                       ; 0                 ; 6       ;
;      - arm:U27|B1_1~0                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~1                         ; 0                 ; 6       ;
;      - arm:U27|B16_1~41                       ; 0                 ; 6       ;
;      - arm:U27|B6_1~1                         ; 0                 ; 6       ;
;      - arm:U27|B6_1~2                         ; 0                 ; 6       ;
;      - arm:U27|B14_1~40                       ; 0                 ; 6       ;
;      - arm:U27|B1_1~2                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~3                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~4                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~5                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~6                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~7                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~8                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~9                         ; 0                 ; 6       ;
;      - arm:U27|B1_1~10                        ; 0                 ; 6       ;
;      - arm:U27|Bf_1~0                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~1                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~2                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~3                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~4                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~5                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~6                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~7                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~8                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~9                         ; 0                 ; 6       ;
;      - arm:U27|Bf_1~10                        ; 0                 ; 6       ;
;      - arm:U27|Bf_1~11                        ; 0                 ; 6       ;
;      - arm:U27|Bf_1~12                        ; 0                 ; 6       ;
;      - arm:U10|B1_1~0                         ; 0                 ; 6       ;
;      - arm:U10|B16_1~14                       ; 0                 ; 6       ;
;      - arm:U10|B1_1~1                         ; 0                 ; 6       ;
;      - arm:U10|B16_1~41                       ; 0                 ; 6       ;
;      - arm:U10|B6_1~1                         ; 0                 ; 6       ;
;      - arm:U10|B6_1~2                         ; 0                 ; 6       ;
;      - arm:U10|B14_1~40                       ; 0                 ; 6       ;
;      - arm:U10|B1_1~2                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~3                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~4                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~5                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~6                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~7                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~8                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~9                         ; 0                 ; 6       ;
;      - arm:U10|B1_1~10                        ; 0                 ; 6       ;
;      - arm:U10|Bf_1~0                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~1                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~2                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~3                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~4                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~5                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~6                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~7                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~8                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~9                         ; 0                 ; 6       ;
;      - arm:U10|Bf_1~10                        ; 0                 ; 6       ;
;      - arm:U10|Bf_1~11                        ; 0                 ; 6       ;
;      - arm:U10|Bf_1~12                        ; 0                 ; 6       ;
;      - LED3:U43|inter2[0]~2                   ; 0                 ; 6       ;
; CLK                                           ;                   ;         ;
; W_EN                                          ;                   ;         ;
;      - LED3:U43|inter2~0                      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|LRDATA[25]~24   ; 0                 ; 6       ;
; INIT                                          ;                   ;         ;
;      - LED3:U43|inter2~1                      ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Selector5~1     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Selector6~2     ; 0                 ; 6       ;
;      - g00_audio_interface:U4|Selector4~3     ; 0                 ; 6       ;
; notas_int[0]                                  ;                   ;         ;
;      - seleccion:U41|inter~0                  ; 0                 ; 6       ;
; notas_int[1]                                  ;                   ;         ;
;      - seleccion:U41|inter~1                  ; 1                 ; 6       ;
; notas_int[2]                                  ;                   ;         ;
;      - seleccion:U41|inter~2                  ; 1                 ; 6       ;
; notas_int[3]                                  ;                   ;         ;
;      - seleccion:U41|inter~3                  ; 1                 ; 6       ;
; notas_int[4]                                  ;                   ;         ;
;      - seleccion:U41|inter~4                  ; 0                 ; 6       ;
; notas_int[5]                                  ;                   ;         ;
;      - seleccion:U41|inter~5                  ; 0                 ; 6       ;
; notas_int[6]                                  ;                   ;         ;
;      - seleccion:U41|inter~6                  ; 0                 ; 6       ;
; notas_int[7]                                  ;                   ;         ;
;      - seleccion:U41|inter~7                  ; 0                 ; 6       ;
; notas_int[8]                                  ;                   ;         ;
;      - seleccion:U41|inter~8                  ; 1                 ; 6       ;
; notas_int[9]                                  ;                   ;         ;
;      - seleccion:U41|inter~9                  ; 1                 ; 6       ;
; notas_int[10]                                 ;                   ;         ;
;      - seleccion:U41|inter~10                 ; 0                 ; 6       ;
; notas_int[11]                                 ;                   ;         ;
;      - seleccion:U41|inter~11                 ; 0                 ; 6       ;
; notas[0]                                      ;                   ;         ;
;      - invertir:U42|Salint[0]~0               ; 1                 ; 6       ;
; en                                            ;                   ;         ;
;      - deteccion:U40|Salint[0]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[1]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[2]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[3]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[5]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[6]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[7]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[8]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[9]                ; 1                 ; 6       ;
;      - deteccion:U40|Salint[10]               ; 1                 ; 6       ;
;      - deteccion:U40|Salint[11]               ; 1                 ; 6       ;
; notas[1]                                      ;                   ;         ;
;      - invertir:U42|Salint[1]~1               ; 1                 ; 6       ;
; notas[2]                                      ;                   ;         ;
;      - invertir:U42|Salint[2]~2               ; 0                 ; 6       ;
; notas[3]                                      ;                   ;         ;
;      - invertir:U42|Salint[3]~3               ; 1                 ; 6       ;
; notas[5]                                      ;                   ;         ;
;      - invertir:U42|Salint[5]~4               ; 0                 ; 6       ;
; notas[6]                                      ;                   ;         ;
;      - invertir:U42|Salint[6]~5               ; 0                 ; 6       ;
; notas[7]                                      ;                   ;         ;
;      - invertir:U42|Salint[7]~6               ; 1                 ; 6       ;
; notas[8]                                      ;                   ;         ;
;      - invertir:U42|Salint[8]~7               ; 0                 ; 6       ;
; notas[9]                                      ;                   ;         ;
;      - invertir:U42|Salint[9]~8               ; 0                 ; 6       ;
; notas[10]                                     ;                   ;         ;
;      - invertir:U42|Salint[10]~9              ; 0                 ; 6       ;
; notas[11]                                     ;                   ;         ;
;      - invertir:U42|Salint[11]~10             ; 1                 ; 6       ;
; notas[4]                                      ;                   ;         ;
;      - invertir:U42|Salint[4]~11              ; 1                 ; 6       ;
+-----------------------------------------------+-------------------+---------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; Control Signals                                                                                                                                                                                ;
+----------------------------------------+--------------------+---------+-----------------------------------------+--------+----------------------+------------------+---------------------------+
; Name                                   ; Location           ; Fan-Out ; Usage                                   ; Global ; Global Resource Used ; Global Line Name ; Enable Signal Source Name ;
+----------------------------------------+--------------------+---------+-----------------------------------------+--------+----------------------+------------------+---------------------------+
; CLK                                    ; PIN_Y2             ; 27      ; Clock                                   ; yes    ; Global Clock         ; GCLK4            ; --                        ;
; FF2:U34|Equal0~1                       ; LCCOMB_X79_Y38_N24 ; 180     ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~10                      ; LCCOMB_X73_Y38_N2  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~12                      ; LCCOMB_X74_Y38_N18 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~13                      ; LCCOMB_X73_Y38_N8  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~14                      ; LCCOMB_X74_Y38_N16 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~16                      ; LCCOMB_X75_Y36_N24 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~17                      ; LCCOMB_X79_Y38_N28 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~18                      ; LCCOMB_X79_Y40_N10 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~20                      ; LCCOMB_X72_Y39_N2  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~22                      ; LCCOMB_X73_Y38_N4  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~23                      ; LCCOMB_X72_Y39_N20 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~25                      ; LCCOMB_X79_Y38_N20 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~27                      ; LCCOMB_X74_Y41_N4  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~28                      ; LCCOMB_X73_Y38_N6  ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~29                      ; LCCOMB_X74_Y41_N10 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~3                       ; LCCOMB_X73_Y43_N20 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~30                      ; LCCOMB_X79_Y38_N30 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~31                      ; LCCOMB_X75_Y36_N22 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~6                       ; LCCOMB_X79_Y38_N16 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~7                       ; LCCOMB_X73_Y43_N22 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; FF2:U34|Equal0~8                       ; LCCOMB_X79_Y38_N14 ; 16      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; RST                                    ; PIN_AA22           ; 1123    ; Async. clear, Clock enable, Sync. clear ; no     ; --                   ; --               ; --                        ;
; amplitud:U25|amp12e~5                  ; LCCOMB_X83_Y44_N0  ; 44      ; Sync. load                              ; no     ; --                   ; --               ; --                        ;
; amplitud:U7|Equal1~0                   ; LCCOMB_X77_Y52_N8  ; 1012    ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; calc_notas:U23|nota1int[0]~12          ; LCCOMB_X83_Y61_N10 ; 7       ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; calc_notas:U23|nota1int[3]             ; FF_X83_Y61_N27     ; 583     ; Sync. load                              ; no     ; --                   ; --               ; --                        ;
; calc_notas:U23|nota2int[3]             ; FF_X83_Y61_N1      ; 583     ; Sync. load                              ; no     ; --                   ; --               ; --                        ;
; control:U8|Qint[4]~15                  ; LCCOMB_X79_Y38_N12 ; 5       ; Sync. clear                             ; no     ; --                   ; --               ; --                        ;
; divisor1:U1|sint                       ; FF_X67_Y36_N25     ; 2464    ; Clock                                   ; yes    ; Global Clock         ; GCLK7            ; --                        ;
; divisor2:U2|sint                       ; FF_X67_Y36_N17     ; 93      ; Clock                                   ; yes    ; Global Clock         ; GCLK5            ; --                        ;
; divisor3:U3|sint                       ; FF_X66_Y32_N9      ; 523     ; Clock                                   ; yes    ; Global Clock         ; GCLK15           ; --                        ;
; en                                     ; PIN_R24            ; 11      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; fase:U24|fase15e[6]~7                  ; LCCOMB_X89_Y52_N10 ; 36      ; Sync. load                              ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|Equal7~0        ; LCCOMB_X60_Y55_N28 ; 19      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|I2C_SDAT~en     ; FF_X59_Y55_N25     ; 1       ; Output enable                           ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|LRDATA[19]~21   ; LCCOMB_X58_Y45_N16 ; 9       ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|LRDATA[25]~26   ; LCCOMB_X59_Y45_N22 ; 21      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|Mcount          ; FF_X58_Y45_N25     ; 8       ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|SCI_WORD1[4]~0  ; LCCOMB_X65_Y54_N16 ; 11      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|Selector12~10   ; LCCOMB_X60_Y55_N2  ; 6       ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|bit_count[2]~0  ; LCCOMB_X61_Y54_N4  ; 3       ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|clk_count[4]~20 ; LCCOMB_X60_Y55_N16 ; 6       ; Sync. clear                             ; no     ; --                   ; --               ; --                        ;
; g00_audio_interface:U4|word_count[1]   ; FF_X63_Y54_N23     ; 13      ; Sync. clear                             ; no     ; --                   ; --               ; --                        ;
; mux1:U31|dir_mem[0]~16                 ; LCCOMB_X81_Y35_N14 ; 18      ; Clock enable                            ; no     ; --                   ; --               ; --                        ;
; num_inst[0]                            ; PIN_AB23           ; 544     ; Sync. clear, Sync. load                 ; no     ; --                   ; --               ; --                        ;
; num_inst[1]                            ; PIN_AA24           ; 571     ; Sync. clear, Sync. load                 ; no     ; --                   ; --               ; --                        ;
+----------------------------------------+--------------------+---------+-----------------------------------------+--------+----------------------+------------------+---------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------------------+
; Global & Other Fast Signals                                                                                                                              ;
+------------------+----------------+---------+--------------------------------------+----------------------+------------------+---------------------------+
; Name             ; Location       ; Fan-Out ; Fan-Out Using Intentional Clock Skew ; Global Resource Used ; Global Line Name ; Enable Signal Source Name ;
+------------------+----------------+---------+--------------------------------------+----------------------+------------------+---------------------------+
; CLK              ; PIN_Y2         ; 27      ; 8                                    ; Global Clock         ; GCLK4            ; --                        ;
; divisor1:U1|sint ; FF_X67_Y36_N25 ; 2464    ; 184                                  ; Global Clock         ; GCLK7            ; --                        ;
; divisor2:U2|sint ; FF_X67_Y36_N17 ; 93      ; 16                                   ; Global Clock         ; GCLK5            ; --                        ;
; divisor3:U3|sint ; FF_X66_Y32_N9  ; 523     ; 278                                  ; Global Clock         ; GCLK15           ; --                        ;
+------------------+----------------+---------+--------------------------------------+----------------------+------------------+---------------------------+


+----------------------------------------------------------------------------------------------------------------------------------------------+
; Non-Global High Fan-Out Signals                                                                                                              ;
+------------------------------------------------------------------------------------------------------------------------------------+---------+
; Name                                                                                                                               ; Fan-Out ;
+------------------------------------------------------------------------------------------------------------------------------------+---------+
; RST~input                                                                                                                          ; 1123    ;
; amplitud:U7|Equal1~0                                                                                                               ; 1012    ;
; calc_notas:U23|nota1int[1]                                                                                                         ; 603     ;
; calc_notas:U23|nota2int[1]                                                                                                         ; 601     ;
; calc_notas:U23|nota1int[0]                                                                                                         ; 597     ;
; calc_notas:U23|nota2int[0]                                                                                                         ; 595     ;
; calc_notas:U23|nota1int[2]                                                                                                         ; 591     ;
; calc_notas:U23|nota2int[2]                                                                                                         ; 586     ;
; calc_notas:U23|nota1int[3]                                                                                                         ; 583     ;
; calc_notas:U23|nota2int[3]                                                                                                         ; 583     ;
; num_inst[1]~input                                                                                                                  ; 571     ;
; num_inst[0]~input                                                                                                                  ; 544     ;
; FF2:U34|Equal0~1                                                                                                                   ; 180     ;
; mux1:U14|dir_mem[3]                                                                                                                ; 107     ;
; mux1:U31|dir_mem[3]                                                                                                                ; 106     ;
; amplitud:U7|amp12[3]                                                                                                               ; 102     ;
; amplitud:U25|amp12[3]                                                                                                              ; 102     ;
; mux1:U31|dir_mem[7]                                                                                                                ; 99      ;
; mux1:U14|dir_mem[7]                                                                                                                ; 97      ;
; mux1:U14|dir_mem[5]                                                                                                                ; 95      ;
; mux1:U31|dir_mem[5]                                                                                                                ; 95      ;
; control:U8|Qint[1]                                                                                                                 ; 89      ;
; mux1:U14|dir_mem[4]                                                                                                                ; 88      ;
; mux1:U31|dir_mem[4]                                                                                                                ; 88      ;
; mux1:U14|dir_mem[6]                                                                                                                ; 86      ;
; control:U8|Qint[0]                                                                                                                 ; 86      ;
; control:U8|Qint[2]                                                                                                                 ; 86      ;
; mux1:U31|dir_mem[0]                                                                                                                ; 84      ;
; mux1:U31|dir_mem[6]                                                                                                                ; 84      ;
; mux1:U14|dir_mem[0]                                                                                                                ; 83      ;
; mux1:U31|dir_mem[1]                                                                                                                ; 82      ;
; mux1:U31|dir_mem[2]                                                                                                                ; 81      ;
; mux1:U14|dir_mem[1]                                                                                                                ; 80      ;
; mux1:U14|dir_mem[2]                                                                                                                ; 80      ;
; control:U8|Qint[3]                                                                                                                 ; 76      ;
; amplitud:U25|amp12e~5                                                                                                              ; 44      ;
; amplitud:U7|amp10[2]                                                                                                               ; 39      ;
; amplitud:U25|amp10[2]                                                                                                              ; 39      ;
; fase:U24|fase15e[6]~7                                                                                                              ; 36      ;
; mux1:U14|dir_mem[8]                                                                                                                ; 35      ;
; mux1:U31|dir_mem[8]                                                                                                                ; 35      ;
; incrementos:U9|INCe[12]                                                                                                            ; 33      ;
; incrementos:U26|INCe[12]                                                                                                           ; 33      ;
; incrementos:U9|INCe[4]                                                                                                             ; 32      ;
; incrementos:U9|INCe[5]                                                                                                             ; 32      ;
; incrementos:U26|INCe[4]                                                                                                            ; 32      ;
; incrementos:U26|INCe[5]                                                                                                            ; 32      ;
; incrementos:U9|INCe[6]                                                                                                             ; 32      ;
; incrementos:U26|INCe[6]                                                                                                            ; 32      ;
; incrementos:U9|INCe[8]                                                                                                             ; 31      ;
; incrementos:U9|INCe[9]                                                                                                             ; 31      ;
; incrementos:U9|INCe[10]                                                                                                            ; 31      ;
; incrementos:U26|INCe[8]                                                                                                            ; 31      ;
; incrementos:U26|INCe[9]                                                                                                            ; 31      ;
; incrementos:U26|INCe[10]                                                                                                           ; 31      ;
; control:U8|Qint[4]                                                                                                                 ; 31      ;
; mult:U18|lpm_mult:Mult19|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_nbh:auto_generated|~QUARTUS_CREATED_GND~I ; 30      ;
; incrementos:U9|INCe[13]                                                                                                            ; 30      ;
; incrementos:U26|INCe[13]                                                                                                           ; 30      ;
; incrementos:U9|INCe[7]                                                                                                             ; 30      ;
; incrementos:U26|INCe[7]                                                                                                            ; 30      ;
; incrementos:U9|INCe[11]                                                                                                            ; 29      ;
; incrementos:U9|INCe[14]                                                                                                            ; 29      ;
; incrementos:U26|INCe[11]                                                                                                           ; 29      ;
; incrementos:U26|INCe[14]                                                                                                           ; 29      ;
; amplitud:U7|amp12[1]                                                                                                               ; 28      ;
; amplitud:U25|amp12[1]                                                                                                              ; 28      ;
; mux1:U31|dir_mem[0]~1                                                                                                              ; 27      ;
; mux1:U31|dir_mem[0]~0                                                                                                              ; 27      ;
; amplitud:U7|amp10[1]                                                                                                               ; 26      ;
; amplitud:U7|amp11[1]                                                                                                               ; 26      ;
; amplitud:U25|amp10[1]                                                                                                              ; 26      ;
; amplitud:U25|amp11[1]                                                                                                              ; 26      ;
; amplitud:U7|amp13[2]                                                                                                               ; 24      ;
; amplitud:U25|amp13[2]                                                                                                              ; 24      ;
; g00_audio_interface:U4|LRDATA[25]~26                                                                                               ; 21      ;
; sen:U15|Mux6~49                                                                                                                    ; 20      ;
; sen:U15|Mux5~49                                                                                                                    ; 20      ;
; sen:U15|Mux4~39                                                                                                                    ; 20      ;
; sen:U15|Mux3~29                                                                                                                    ; 20      ;
; sen:U15|Mux2~19                                                                                                                    ; 20      ;
; sen:U15|Mux1~10                                                                                                                    ; 20      ;
; sen:U15|Mux0~2                                                                                                                     ; 20      ;
; sen:U32|Mux6~49                                                                                                                    ; 20      ;
; sen:U32|Mux5~49                                                                                                                    ; 20      ;
; sen:U32|Mux4~39                                                                                                                    ; 20      ;
; sen:U32|Mux3~29                                                                                                                    ; 20      ;
; sen:U32|Mux2~19                                                                                                                    ; 20      ;
; sen:U32|Mux1~10                                                                                                                    ; 20      ;
; sen:U32|Mux0~2                                                                                                                     ; 20      ;
; sen:U15|Mux7~52                                                                                                                    ; 20      ;
; sen:U32|Mux7~52                                                                                                                    ; 20      ;
; g00_audio_interface:U4|Equal7~0                                                                                                    ; 19      ;
; g00_audio_interface:U4|BBcount[0]                                                                                                  ; 19      ;
; mux1:U31|dir_mem[0]~16                                                                                                             ; 18      ;
; seleccion:U41|inter[4]                                                                                                             ; 18      ;
; seleccion:U41|inter[7]                                                                                                             ; 17      ;
; incrementos:U9|INCe[2]                                                                                                             ; 16      ;
; incrementos:U26|INCe[2]                                                                                                            ; 16      ;
; arm:U10|B10_1[2]                                                                                                                   ; 16      ;
; arm:U27|B10_1[2]                                                                                                                   ; 16      ;
; FF2:U34|Equal0~31                                                                                                                  ; 16      ;
; FF2:U34|Equal0~30                                                                                                                  ; 16      ;
; FF2:U34|Equal0~29                                                                                                                  ; 16      ;
; FF2:U34|Equal0~28                                                                                                                  ; 16      ;
; FF2:U34|Equal0~27                                                                                                                  ; 16      ;
; FF2:U34|Equal0~25                                                                                                                  ; 16      ;
; FF2:U34|Equal0~23                                                                                                                  ; 16      ;
; FF2:U34|Equal0~22                                                                                                                  ; 16      ;
; FF2:U34|Equal0~20                                                                                                                  ; 16      ;
; FF2:U34|Equal0~18                                                                                                                  ; 16      ;
; FF2:U34|Equal0~17                                                                                                                  ; 16      ;
; FF2:U34|Equal0~16                                                                                                                  ; 16      ;
; FF2:U34|Equal0~14                                                                                                                  ; 16      ;
; FF2:U34|Equal0~13                                                                                                                  ; 16      ;
; FF2:U34|Equal0~12                                                                                                                  ; 16      ;
; FF2:U34|Equal0~10                                                                                                                  ; 16      ;
; FF2:U34|Equal0~8                                                                                                                   ; 16      ;
; FF2:U34|Equal0~7                                                                                                                   ; 16      ;
; FF2:U34|Equal0~6                                                                                                                   ; 16      ;
; FF2:U34|Equal0~3                                                                                                                   ; 16      ;
; seleccion:U41|inter[6]                                                                                                             ; 16      ;
; amplitud:U7|amp12[2]                                                                                                               ; 15      ;
; amplitud:U25|amp12[2]                                                                                                              ; 15      ;
; seleccion:U41|inter[5]                                                                                                             ; 15      ;
; seleccion:U41|inter[2]                                                                                                             ; 15      ;
; incrementos:U9|INCe[3]                                                                                                             ; 15      ;
; incrementos:U26|INCe[3]                                                                                                            ; 15      ;
; g00_audio_interface:U4|word_count[2]                                                                                               ; 14      ;
; g00_audio_interface:U4|BBcount[4]                                                                                                  ; 14      ;
; seleccion:U41|inter[3]                                                                                                             ; 14      ;
; sel~input                                                                                                                          ; 13      ;
; g00_audio_interface:U4|word_count[1]                                                                                               ; 13      ;
; g00_audio_interface:U4|word_count[0]                                                                                               ; 13      ;
; g00_audio_interface:U4|Equal5~1                                                                                                    ; 13      ;
; amplitud:U7|amp11[2]                                                                                                               ; 13      ;
; amplitud:U25|amp11[2]                                                                                                              ; 13      ;
; g00_audio_interface:U4|BBcount[3]                                                                                                  ; 13      ;
; g00_audio_interface:U4|BBcount[5]                                                                                                  ; 13      ;
; seleccion:U41|inter[9]                                                                                                             ; 13      ;
; seleccion:U41|inter[8]                                                                                                             ; 13      ;
; amplitud:U7|Mux95~3                                                                                                                ; 12      ;
; amplitud:U25|Mux95~3                                                                                                               ; 12      ;
; amplitud:U7|amp10[3]                                                                                                               ; 12      ;
; amplitud:U7|amp11[3]                                                                                                               ; 12      ;
; amplitud:U25|amp10[3]                                                                                                              ; 12      ;
; amplitud:U25|amp11[3]                                                                                                              ; 12      ;
; en~input                                                                                                                           ; 11      ;
; arm:U10|B12_1[3]                                                                                                                   ; 11      ;
; arm:U27|B12_1[3]                                                                                                                   ; 11      ;
; amplitud:U7|Mux41~0                                                                                                                ; 11      ;
; amplitud:U25|Mux41~0                                                                                                               ; 11      ;
; g00_audio_interface:U4|SCI_WORD1[4]~0                                                                                              ; 11      ;
; g00_audio_interface:U4|bit_count[0]                                                                                                ; 11      ;
; g00_audio_interface:U4|clk_count[5]                                                                                                ; 11      ;
; g00_audio_interface:U4|clk_count[4]                                                                                                ; 11      ;
; amplitud:U7|ampfunde~18                                                                                                            ; 10      ;
; amplitud:U25|ampfunde~20                                                                                                           ; 10      ;
; g00_audio_interface:U4|state2.sw_write                                                                                             ; 10      ;
; g00_audio_interface:U4|Equal5~0                                                                                                    ; 10      ;
; g00_audio_interface:U4|bit_count[1]                                                                                                ; 10      ;
; amplitud:U7|amp10[0]                                                                                                               ; 10      ;
; amplitud:U7|amp11[0]                                                                                                               ; 10      ;
; amplitud:U7|amp12[0]                                                                                                               ; 10      ;
; amplitud:U7|amp13[0]                                                                                                               ; 10      ;
; amplitud:U25|amp10[0]                                                                                                              ; 10      ;
; amplitud:U25|amp11[0]                                                                                                              ; 10      ;
; amplitud:U25|amp12[0]                                                                                                              ; 10      ;
; amplitud:U25|amp13[0]                                                                                                              ; 10      ;
; seleccion:U41|inter[11]                                                                                                            ; 10      ;
; seleccion:U41|inter[10]                                                                                                            ; 10      ;
; seleccion:U41|inter[1]                                                                                                             ; 10      ;
; mult:U18|lpm_mult:Mult10|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U18|lpm_mult:Mult11|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U18|lpm_mult:Mult12|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U18|lpm_mult:Mult13|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; amplitud:U7|amp14[0]                                                                                                               ; 9       ;
; amplitud:U7|amp15[0]                                                                                                               ; 9       ;
; mult:U35|lpm_mult:Mult10|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U35|lpm_mult:Mult11|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U35|lpm_mult:Mult12|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; mult:U35|lpm_mult:Mult13|mult_2at:auto_generated|le4a[9]                                                                           ; 9       ;
; amplitud:U25|amp14[0]                                                                                                              ; 9       ;
; amplitud:U25|amp15[0]                                                                                                              ; 9       ;
; g00_audio_interface:U4|LRDATA[19]~21                                                                                               ; 9       ;
; seleccion:U41|inter[0]                                                                                                             ; 9       ;
; amplitud:U7|Mux95~2                                                                                                                ; 8       ;
; amplitud:U25|Mux95~2                                                                                                               ; 8       ;
; g00_audio_interface:U4|Mcount                                                                                                      ; 8       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated|op_1~16                  ; 8       ;
; arm:U10|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated|op_1~16                  ; 8       ;
; arm:U10|Add2~28                                                                                                                    ; 8       ;
; arm:U27|lpm_mult:Mult1|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated|op_1~16                  ; 8       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_88h:auto_generated|op_1~16                  ; 8       ;
; arm:U27|Add2~28                                                                                                                    ; 8       ;
; arm:U10|B15_1[8]                                                                                                                   ; 7       ;
; arm:U27|B15_1[8]                                                                                                                   ; 7       ;
; calc_notas:U23|nota1int[0]~12                                                                                                      ; 7       ;
; calc_notas:U23|nota2int~3                                                                                                          ; 7       ;
; calc_notas:U23|nota2int~2                                                                                                          ; 7       ;
; amplitud:U25|amp6e~2                                                                                                               ; 7       ;
; g00_audio_interface:U4|word_count[3]                                                                                               ; 7       ;
; mult:U18|lpm_mult:Mult10|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U18|lpm_mult:Mult11|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U18|lpm_mult:Mult12|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U18|lpm_mult:Mult13|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U35|lpm_mult:Mult10|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U35|lpm_mult:Mult11|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U35|lpm_mult:Mult12|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; mult:U35|lpm_mult:Mult13|mult_2at:auto_generated|cs2a[1]~0                                                                         ; 7       ;
; g00_audio_interface:U4|state.s2                                                                                                    ; 7       ;
; g00_audio_interface:U4|state.sw_init1                                                                                              ; 7       ;
; g00_audio_interface:U4|state.s1                                                                                                    ; 7       ;
; arm:U10|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_g9h:auto_generated|op_1~18                  ; 7       ;
; arm:U27|lpm_mult:Mult2|multcore:mult_core|mpar_add:padder|lpm_add_sub:adder[0]|add_sub_g9h:auto_generated|op_1~18                  ; 7       ;
; amplitud:U7|amp6e~17                                                                                                               ; 6       ;
; amplitud:U25|amp6e~15                                                                                                              ; 6       ;
; g00_audio_interface:U4|state2.sw_ready                                                                                             ; 6       ;
; amplitud:U7|Mux95~0                                                                                                                ; 6       ;
; amplitud:U25|amp12e~4                                                                                                              ; 6       ;
; amplitud:U25|Mux95~0                                                                                                               ; 6       ;
; g00_audio_interface:U4|Selector12~10                                                                                               ; 6       ;
; g00_audio_interface:U4|clk_count[4]~20                                                                                             ; 6       ;
; g00_audio_interface:U4|Equal8~0                                                                                                    ; 6       ;
; g00_audio_interface:U4|bit_count[2]                                                                                                ; 6       ;
; g00_audio_interface:U4|state.sw_init0                                                                                              ; 6       ;
; g00_audio_interface:U4|Bcount[0]                                                                                                   ; 6       ;
; g00_audio_interface:U4|Bcount[1]                                                                                                   ; 6       ;
; g00_audio_interface:U4|Bcount[2]                                                                                                   ; 6       ;
; calc_notas:U23|Add10~6                                                                                                             ; 6       ;
; calc_notas:U23|Add10~4                                                                                                             ; 6       ;
; calc_notas:U23|Add10~2                                                                                                             ; 6       ;
; offset:U19|Add38~4                                                                                                                 ; 6       ;
; offset:U36|Add38~4                                                                                                                 ; 6       ;
; amplitud:U7|amp5e~10                                                                                                               ; 5       ;
; amplitud:U7|amp3e~19                                                                                                               ; 5       ;
; amplitud:U25|amp5e~10                                                                                                              ; 5       ;
; amplitud:U25|amp1e~31                                                                                                              ; 5       ;
; amplitud:U25|amp3e~19                                                                                                              ; 5       ;
; arm:U10|B15_1[9]                                                                                                                   ; 5       ;
; arm:U27|B15_1[9]                                                                                                                   ; 5       ;
; calc_notas:U23|nota2int~10                                                                                                         ; 5       ;
; g00_audio_interface:U4|SCI_READY                                                                                                   ; 5       ;
; g00_audio_interface:U4|state2.sw_init1                                                                                             ; 5       ;
; amplitud:U7|amp2e~13                                                                                                               ; 5       ;
; amplitud:U25|amp2e~13                                                                                                              ; 5       ;
; amplitud:U7|amp3e~6                                                                                                                ; 5       ;
; amplitud:U7|amp1e~17                                                                                                               ; 5       ;
; fase:U24|Mux68~0                                                                                                                   ; 5       ;
; amplitud:U25|amp3e~6                                                                                                               ; 5       ;
; amplitud:U7|Mux95~1                                                                                                                ; 5       ;
; amplitud:U7|amp12e~4                                                                                                               ; 5       ;
; control:U8|Qint[4]~15                                                                                                              ; 5       ;
; amplitud:U25|Mux95~1                                                                                                               ; 5       ;
; FF2:U17|B10_FF[1]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[2]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[3]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[4]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[6]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[5]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[7]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[1]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[2]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[3]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[4]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[6]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[5]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[7]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[1]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[2]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[3]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[4]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[6]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[5]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[7]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[1]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[2]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[3]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[4]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[6]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[5]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[7]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[1]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[2]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[3]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[4]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[6]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[5]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[7]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[1]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[2]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[3]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[4]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[6]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[5]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[7]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[1]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[2]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[3]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[4]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[6]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[5]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[7]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[1]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[2]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[3]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[4]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[6]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[5]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[7]                                                                                                                  ; 5       ;
; FF2:U17|B10_FF[0]                                                                                                                  ; 5       ;
; FF2:U17|B11_FF[0]                                                                                                                  ; 5       ;
; FF2:U17|B12_FF[0]                                                                                                                  ; 5       ;
; FF2:U17|B13_FF[0]                                                                                                                  ; 5       ;
; FF2:U34|B10_FF[0]                                                                                                                  ; 5       ;
; FF2:U34|B11_FF[0]                                                                                                                  ; 5       ;
; FF2:U34|B12_FF[0]                                                                                                                  ; 5       ;
; FF2:U34|B13_FF[0]                                                                                                                  ; 5       ;
; g00_audio_interface:U4|SCI_WRITE                                                                                                   ; 5       ;
; g00_audio_interface:U4|state.sack31                                                                                                ; 5       ;
; g00_audio_interface:U4|state.sack21                                                                                                ; 5       ;
; g00_audio_interface:U4|state.sw1b3                                                                                                 ; 5       ;
; g00_audio_interface:U4|state.sab3                                                                                                  ; 5       ;
; g00_audio_interface:U4|state.sw2b3                                                                                                 ; 5       ;
; divisor1:U1|Qint[0]                                                                                                                ; 5       ;
; g00_audio_interface:U4|state.sw2b2                                                                                                 ; 5       ;
; g00_audio_interface:U4|state.sw1b2                                                                                                 ; 5       ;
; g00_audio_interface:U4|state.sab2                                                                                                  ; 5       ;
; g00_audio_interface:U4|state.send                                                                                                  ; 5       ;
; g00_audio_interface:U4|state.s0                                                                                                    ; 5       ;
; g00_audio_interface:U4|Equal2~0                                                                                                    ; 5       ;
; g00_audio_interface:U4|BBcount[2]                                                                                                  ; 5       ;
; INIT~input                                                                                                                         ; 4       ;
; fase:U6|fase10e~16                                                                                                                 ; 4       ;
; fase:U6|fase8e~11                                                                                                                  ; 4       ;
; amplitud:U7|amp1e~31                                                                                                               ; 4       ;
; amplitud:U7|amp4e~13                                                                                                               ; 4       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|_~0                                                                                      ; 4       ;
; fase:U24|fase8e~11                                                                                                                 ; 4       ;
; fase:U24|fase10e~24                                                                                                                ; 4       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|_~3                                                                                      ; 4       ;
; arm:U10|B15_1[10]                                                                                                                  ; 4       ;
; arm:U10|B15_1[11]                                                                                                                  ; 4       ;
; arm:U10|B15_1[12]                                                                                                                  ; 4       ;
; arm:U10|B15_1[13]                                                                                                                  ; 4       ;
; arm:U10|B15_1[14]                                                                                                                  ; 4       ;
; arm:U10|B15_1[15]                                                                                                                  ; 4       ;
; arm:U10|B15_1[16]                                                                                                                  ; 4       ;
; arm:U10|B15_1[17]                                                                                                                  ; 4       ;
; arm:U10|B15_1[18]                                                                                                                  ; 4       ;
; arm:U27|B15_1[10]                                                                                                                  ; 4       ;
; arm:U27|B15_1[11]                                                                                                                  ; 4       ;
; arm:U27|B15_1[12]                                                                                                                  ; 4       ;
; arm:U27|B15_1[13]                                                                                                                  ; 4       ;
; arm:U27|B15_1[14]                                                                                                                  ; 4       ;
; arm:U27|B15_1[15]                                                                                                                  ; 4       ;
; arm:U27|B15_1[16]                                                                                                                  ; 4       ;
; arm:U27|B15_1[17]                                                                                                                  ; 4       ;
; arm:U27|B15_1[18]                                                                                                                  ; 4       ;
; calc_notas:U23|nota2int~8                                                                                                          ; 4       ;
; calc_notas:U23|nota2int~5                                                                                                          ; 4       ;
; calc_notas:U23|nota1int[0]~2                                                                                                       ; 4       ;
; calc_notas:U23|nota2int~4                                                                                                          ; 4       ;
; amplitud:U7|amp1e~29                                                                                                               ; 4       ;
; amplitud:U7|amp8e~3                                                                                                                ; 4       ;
; amplitud:U25|amp1e~29                                                                                                              ; 4       ;
; amplitud:U25|amp8e~3                                                                                                               ; 4       ;
; amplitud:U7|amp1e~16                                                                                                               ; 4       ;
; amplitud:U7|ampfunde~10                                                                                                            ; 4       ;
; amplitud:U7|Mux62~0                                                                                                                ; 4       ;
; amplitud:U7|Mux95~4                                                                                                                ; 4       ;
; amplitud:U25|amp1e~17                                                                                                              ; 4       ;
; amplitud:U25|amp1e~16                                                                                                              ; 4       ;
; amplitud:U25|ampfunde~10                                                                                                           ; 4       ;
; amplitud:U25|Mux62~0                                                                                                               ; 4       ;
; amplitud:U25|Mux95~4                                                                                                               ; 4       ;
; divisor3:U3|Equal0~2                                                                                                               ; 4       ;
; divisor3:U3|Equal0~1                                                                                                               ; 4       ;
; divisor3:U3|Equal0~0                                                                                                               ; 4       ;
; g00_audio_interface:U4|Equal9~0                                                                                                    ; 4       ;
; g00_audio_interface:U4|Selector12~8                                                                                                ; 4       ;
; g00_audio_interface:U4|state.sw1b1                                                                                                 ; 4       ;
; g00_audio_interface:U4|state.sab1                                                                                                  ; 4       ;
; g00_audio_interface:U4|state.sw2b1                                                                                                 ; 4       ;
; divisor1:U1|Equal0~2                                                                                                               ; 4       ;
; divisor1:U1|Equal0~0                                                                                                               ; 4       ;
; g00_audio_interface:U4|BBcount[1]                                                                                                  ; 4       ;
; calc_notas:U23|Add10~0                                                                                                             ; 4       ;
; incrementos:U9|Mux14~0                                                                                                             ; 3       ;
; incrementos:U26|Mux3~0                                                                                                             ; 3       ;
; amplitud:U7|amp3e~21                                                                                                               ; 3       ;
; fase:U6|fase7e~23                                                                                                                  ; 3       ;
; fase:U6|fase3e~35                                                                                                                  ; 3       ;
; fase:U6|fase12e~14                                                                                                                 ; 3       ;
; fase:U6|fase8e~10                                                                                                                  ; 3       ;
; fase:U6|fase7e~22                                                                                                                  ; 3       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[0][3]~2                                                                           ; 3       ;
; arm:U10|lpm_mult:Mult1|multcore:mult_core|_~2                                                                                      ; 3       ;
; fase:U24|fase12e~15                                                                                                                ; 3       ;
; amplitud:U25|amp3e~20                                                                                                              ; 3       ;
; fase:U24|fase8e~19                                                                                                                 ; 3       ;
; amplitud:U25|amp1e~33                                                                                                              ; 3       ;
; fase:U24|fase8e~12                                                                                                                 ; 3       ;
; fase:U24|fase10e~29                                                                                                                ; 3       ;
; fase:U24|fase8e~10                                                                                                                 ; 3       ;
; fase:U24|fase12e~9                                                                                                                 ; 3       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[0][3]~4                                                                           ; 3       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|_~2                                                                                      ; 3       ;
; arm:U10|B13_1[3]                                                                                                                   ; 3       ;
; arm:U10|B13_1[4]                                                                                                                   ; 3       ;
; arm:U10|B13_1[5]                                                                                                                   ; 3       ;
; arm:U27|B13_1[3]                                                                                                                   ; 3       ;
; arm:U27|B13_1[4]                                                                                                                   ; 3       ;
; arm:U27|B13_1[5]                                                                                                                   ; 3       ;
; calc_notas:U23|Equal0~1                                                                                                            ; 3       ;
; calc_notas:U23|Equal1~0                                                                                                            ; 3       ;
; calc_notas:U23|nota2int~9                                                                                                          ; 3       ;
; calc_notas:U23|nota2int~6                                                                                                          ; 3       ;
; calc_notas:U23|Add1~0                                                                                                              ; 3       ;
; amplitud:U7|amp2e~19                                                                                                               ; 3       ;
; amplitud:U7|amp5e~9                                                                                                                ; 3       ;
; fase:U6|fase1e~11                                                                                                                  ; 3       ;
; amplitud:U25|amp2e~20                                                                                                              ; 3       ;
; amplitud:U25|amp5e~9                                                                                                               ; 3       ;
; fase:U24|fase1e~11                                                                                                                 ; 3       ;
; amplitud:U7|Mux95~6                                                                                                                ; 3       ;
; fase:U6|Mux68~0                                                                                                                    ; 3       ;
; amplitud:U7|amp3e~5                                                                                                                ; 3       ;
; amplitud:U7|amp12e~6                                                                                                               ; 3       ;
; amplitud:U25|Mux95~6                                                                                                               ; 3       ;
; amplitud:U25|ampfunde~16                                                                                                           ; 3       ;
; amplitud:U25|amp12e~7                                                                                                              ; 3       ;
; g00_audio_interface:U4|SCI_WORD1[4]~3                                                                                              ; 3       ;
; g00_audio_interface:U4|Selector18~0                                                                                                ; 3       ;
; g00_audio_interface:U4|bit_count[2]~0                                                                                              ; 3       ;
; FF2:U17|B14_FF[1]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[2]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[3]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[4]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[5]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[6]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[7]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[1]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[2]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[3]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[4]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[5]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[6]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[7]                                                                                                                  ; 3       ;
; FF2:U17|B14_FF[0]                                                                                                                  ; 3       ;
; FF2:U34|B14_FF[0]                                                                                                                  ; 3       ;
; g00_audio_interface:U4|Selector12~7                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack33                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack23                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack13                                                                                                ; 3       ;
; g00_audio_interface:U4|WideOr3~0                                                                                                   ; 3       ;
; g00_audio_interface:U4|state.sack11                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack32                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack22                                                                                                ; 3       ;
; g00_audio_interface:U4|state.sack12                                                                                                ; 3       ;
; arm:U10|B11_1[5]                                                                                                                   ; 3       ;
; arm:U10|B11_1[6]                                                                                                                   ; 3       ;
; arm:U10|B11_1[7]                                                                                                                   ; 3       ;
; arm:U10|B11_1[8]                                                                                                                   ; 3       ;
; arm:U10|B11_1[9]                                                                                                                   ; 3       ;
; arm:U10|B11_1[10]                                                                                                                  ; 3       ;
; arm:U10|B11_1[11]                                                                                                                  ; 3       ;
; arm:U10|B11_1[12]                                                                                                                  ; 3       ;
; arm:U10|B11_1[13]                                                                                                                  ; 3       ;
; arm:U10|B11_1[14]                                                                                                                  ; 3       ;
; arm:U10|B11_1[15]                                                                                                                  ; 3       ;
; arm:U10|B11_1[16]                                                                                                                  ; 3       ;
; arm:U10|B11_1[17]                                                                                                                  ; 3       ;
; arm:U10|B11_1[18]                                                                                                                  ; 3       ;
; arm:U10|B19_1[19]                                                                                                                  ; 3       ;
; arm:U10|B19_1[6]                                                                                                                   ; 3       ;
; arm:U10|B19_1[7]                                                                                                                   ; 3       ;
; arm:U10|B19_1[8]                                                                                                                   ; 3       ;
; arm:U10|B19_1[9]                                                                                                                   ; 3       ;
; arm:U10|B19_1[10]                                                                                                                  ; 3       ;
; arm:U10|B19_1[11]                                                                                                                  ; 3       ;
; arm:U10|B19_1[12]                                                                                                                  ; 3       ;
; arm:U10|B19_1[13]                                                                                                                  ; 3       ;
; arm:U10|B19_1[14]                                                                                                                  ; 3       ;
; arm:U10|B19_1[15]                                                                                                                  ; 3       ;
; arm:U10|B19_1[16]                                                                                                                  ; 3       ;
; arm:U10|B19_1[17]                                                                                                                  ; 3       ;
; arm:U10|B19_1[18]                                                                                                                  ; 3       ;
; arm:U27|B19_1[19]                                                                                                                  ; 3       ;
; arm:U27|B11_1[5]                                                                                                                   ; 3       ;
; arm:U27|B11_1[6]                                                                                                                   ; 3       ;
; arm:U27|B11_1[7]                                                                                                                   ; 3       ;
; arm:U27|B11_1[8]                                                                                                                   ; 3       ;
; arm:U27|B11_1[9]                                                                                                                   ; 3       ;
; arm:U27|B11_1[10]                                                                                                                  ; 3       ;
; arm:U27|B11_1[11]                                                                                                                  ; 3       ;
; arm:U27|B11_1[12]                                                                                                                  ; 3       ;
; arm:U27|B11_1[13]                                                                                                                  ; 3       ;
; arm:U27|B11_1[14]                                                                                                                  ; 3       ;
; arm:U27|B11_1[15]                                                                                                                  ; 3       ;
; arm:U27|B11_1[16]                                                                                                                  ; 3       ;
; arm:U27|B11_1[17]                                                                                                                  ; 3       ;
; arm:U27|B11_1[18]                                                                                                                  ; 3       ;
; arm:U27|B19_1[6]                                                                                                                   ; 3       ;
; arm:U27|B19_1[7]                                                                                                                   ; 3       ;
; arm:U27|B19_1[8]                                                                                                                   ; 3       ;
; arm:U27|B19_1[9]                                                                                                                   ; 3       ;
; arm:U27|B19_1[10]                                                                                                                  ; 3       ;
; arm:U27|B19_1[11]                                                                                                                  ; 3       ;
; arm:U27|B19_1[12]                                                                                                                  ; 3       ;
; arm:U27|B19_1[13]                                                                                                                  ; 3       ;
; arm:U27|B19_1[14]                                                                                                                  ; 3       ;
; arm:U27|B19_1[15]                                                                                                                  ; 3       ;
; arm:U27|B19_1[16]                                                                                                                  ; 3       ;
; arm:U27|B19_1[17]                                                                                                                  ; 3       ;
; arm:U27|B19_1[18]                                                                                                                  ; 3       ;
; W_EN~input                                                                                                                         ; 2       ;
; ~GND                                                                                                                               ; 2       ;
; fase:U6|fase1e~37                                                                                                                  ; 2       ;
; fase:U24|fase10e~36                                                                                                                ; 2       ;
; amplitud:U7|amp10e~11                                                                                                              ; 2       ;
; amplitud:U25|amp10e~11                                                                                                             ; 2       ;
; incrementos:U9|Mux15~0                                                                                                             ; 2       ;
; incrementos:U9|INCe~26                                                                                                             ; 2       ;
; incrementos:U9|Mux12~0                                                                                                             ; 2       ;
; incrementos:U9|INCe~24                                                                                                             ; 2       ;
; incrementos:U9|Mux21~0                                                                                                             ; 2       ;
; incrementos:U9|INCe~14                                                                                                             ; 2       ;
; incrementos:U26|Mux21~0                                                                                                            ; 2       ;
; incrementos:U26|INCe~15                                                                                                            ; 2       ;
; incrementos:U26|Mux15~0                                                                                                            ; 2       ;
; incrementos:U26|INCe~12                                                                                                            ; 2       ;
; incrementos:U26|Mux12~0                                                                                                            ; 2       ;
; incrementos:U26|INCe~10                                                                                                            ; 2       ;
; arm:U10|lpm_mult:Mult1|multcore:mult_core|_~7                                                                                      ; 2       ;
; fase:U6|Mux265~0                                                                                                                   ; 2       ;
; fase:U6|fase2e~13                                                                                                                  ; 2       ;
; amplitud:U7|amp1e~32                                                                                                               ; 2       ;
; fase:U6|Mux309~0                                                                                                                   ; 2       ;
; fase:U6|fase8e~12                                                                                                                  ; 2       ;
; fase:U6|fase3e~32                                                                                                                  ; 2       ;
; fase:U6|Mux289~0                                                                                                                   ; 2       ;
; fase:U6|fase14e~11                                                                                                                 ; 2       ;
; fase:U6|fase14e~10                                                                                                                 ; 2       ;
; fase:U6|fase3e~12                                                                                                                  ; 2       ;
; fase:U6|fase3e~11                                                                                                                  ; 2       ;
; amplitud:U7|amp6e~16                                                                                                               ; 2       ;
; fase:U6|Mux264~0                                                                                                                   ; 2       ;
; fase:U6|fase1e~12                                                                                                                  ; 2       ;
; fase:U6|fase11e~8                                                                                                                  ; 2       ;
; arm:U10|B1_1~0                                                                                                                     ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[2][1]~1                                                                           ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[2][2]                                                                             ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[3][1]                                                                             ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[3][2]                                                                             ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[3][5]                                                                             ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[1][1]~0                                                                           ; 2       ;
; arm:U10|lpm_mult:Mult0|multcore:mult_core|romout[1][2]                                                                             ; 2       ;
; fase:U24|fase10e~32                                                                                                                ; 2       ;
; fase:U24|fase8e~21                                                                                                                 ; 2       ;
; fase:U24|fase4e~18                                                                                                                 ; 2       ;
; fase:U24|Mux265~0                                                                                                                  ; 2       ;
; fase:U24|fase2e~29                                                                                                                 ; 2       ;
; fase:U24|fase3e~13                                                                                                                 ; 2       ;
; fase:U24|Mux309~0                                                                                                                  ; 2       ;
; fase:U24|Mux289~0                                                                                                                  ; 2       ;
; fase:U24|fase14e~11                                                                                                                ; 2       ;
; fase:U24|fase14e~10                                                                                                                ; 2       ;
; fase:U24|fase3e~11                                                                                                                 ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|_~7                                                                                      ; 2       ;
; amplitud:U25|amp1e~30                                                                                                              ; 2       ;
; fase:U24|fase10e~12                                                                                                                ; 2       ;
; fase:U24|fase7e~18                                                                                                                 ; 2       ;
; fase:U24|fase15e~8                                                                                                                 ; 2       ;
; amplitud:U25|amp6e~14                                                                                                              ; 2       ;
; fase:U24|fase1e~12                                                                                                                 ; 2       ;
; fase:U24|fase11e~8                                                                                                                 ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[2][1]~3                                                                           ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[2][2]~2                                                                           ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[3][1]                                                                             ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[3][2]                                                                             ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[3][5]                                                                             ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[1][1]~1                                                                           ; 2       ;
; arm:U27|lpm_mult:Mult0|multcore:mult_core|romout[1][2]~0                                                                           ; 2       ;
; fase:U24|Mux264~0                                                                                                                  ; 2       ;
; arm:U27|B1_1~1                                                                                                                     ; 2       ;
; fase:U6|fase6e[8]                                                                                                                  ; 2       ;
; fase:U6|fase15e[3]                                                                                                                 ; 2       ;
; fase:U6|fase2e[0]                                                                                                                  ; 2       ;
; fase:U6|fase11e[2]                                                                                                                 ; 2       ;
; fase:U6|fase9e[4]                                                                                                                  ; 2       ;
; fase:U24|fase6e[8]                                                                                                                 ; 2       ;
; fase:U24|fase15e[3]                                                                                                                ; 2       ;
; fase:U24|fase11e[2]                                                                                                                ; 2       ;
; fase:U24|fase9e[4]                                                                                                                 ; 2       ;
; fase:U24|fase2e[0]                                                                                                                 ; 2       ;
; FF2:U34|Equal0~26                                                                                                                  ; 2       ;
; FF2:U34|Equal0~24                                                                                                                  ; 2       ;
; FF2:U34|Equal0~21                                                                                                                  ; 2       ;
; FF2:U34|Equal0~19                                                                                                                  ; 2       ;
; g00_audio_interface:U4|state2.sw_init0                                                                                             ; 2       ;
; FF2:U34|Equal0~15                                                                                                                  ; 2       ;
; FF2:U34|Equal0~11                                                                                                                  ; 2       ;
; calc_notas:U23|nota2int~36                                                                                                         ; 2       ;
; calc_notas:U23|Equal0~0                                                                                                            ; 2       ;
; calc_notas:U23|nota1int~13                                                                                                         ; 2       ;
; calc_notas:U23|nota1int[0]~10                                                                                                      ; 2       ;
; calc_notas:U23|nota1int[0]~7                                                                                                       ; 2       ;
; calc_notas:U23|Add2~1                                                                                                              ; 2       ;
; calc_notas:U23|Add1~1                                                                                                              ; 2       ;
; calc_notas:U23|Add2~0                                                                                                              ; 2       ;
; FF2:U34|Equal0~9                                                                                                                   ; 2       ;
; FF2:U34|Equal0~5                                                                                                                   ; 2       ;
; g00_audio_interface:U4|Selector2~0                                                                                                 ; 2       ;
; g00_audio_interface:U4|word_count~3                                                                                                ; 2       ;
; amplitud:U7|amp12e~8                                                                                                               ; 2       ;
; amplitud:U7|amp6e~11                                                                                                               ; 2       ;
; amplitud:U7|ampfunde~25                                                                                                            ; 2       ;
; amplitud:U7|amp1e~28                                                                                                               ; 2       ;
; amplitud:U7|amp1e~27                                                                                                               ; 2       ;
; amplitud:U7|Mux1~0                                                                                                                 ; 2       ;
; amplitud:U25|amp2e~17                                                                                                              ; 2       ;
; amplitud:U25|amp12e~9                                                                                                              ; 2       ;
; amplitud:U25|amp6e~8                                                                                                               ; 2       ;
; amplitud:U25|amp1e~28                                                                                                              ; 2       ;
; amplitud:U25|amp1e~27                                                                                                              ; 2       ;
; amplitud:U25|Mux1~0                                                                                                                ; 2       ;
; amplitud:U7|Mux138~0                                                                                                               ; 2       ;
; amplitud:U7|amp6e~6                                                                                                                ; 2       ;
; amplitud:U7|Mux42~0                                                                                                                ; 2       ;
; sen:U15|Mux4~36                                                                                                                    ; 2       ;
; sen:U15|Mux4~23                                                                                                                    ; 2       ;
; sen:U15|Mux4~22                                                                                                                    ; 2       ;
; sen:U15|Mux4~21                                                                                                                    ; 2       ;
; sen:U15|Mux4~12                                                                                                                    ; 2       ;
; sen:U15|Mux4~2                                                                                                                     ; 2       ;
; sen:U15|Mux4~1                                                                                                                     ; 2       ;
; sen:U15|Mux4~0                                                                                                                     ; 2       ;
; sen:U15|Mux2~14                                                                                                                    ; 2       ;
; sen:U15|Mux3~1                                                                                                                     ; 2       ;
; sen:U15|Mux2~5                                                                                                                     ; 2       ;
; sen:U15|Mux3~0                                                                                                                     ; 2       ;
; sen:U15|Mux2~2                                                                                                                     ; 2       ;
; sen:U15|Mux0~0                                                                                                                     ; 2       ;
; amplitud:U25|Mux138~0                                                                                                              ; 2       ;
; amplitud:U25|amp6e~3                                                                                                               ; 2       ;
; amplitud:U25|amp3e~5                                                                                                               ; 2       ;
; amplitud:U25|Mux42~0                                                                                                               ; 2       ;
; sen:U32|Mux4~36                                                                                                                    ; 2       ;
; sen:U32|Mux4~21                                                                                                                    ; 2       ;
; sen:U32|Mux4~12                                                                                                                    ; 2       ;
; sen:U32|Mux4~2                                                                                                                     ; 2       ;
; sen:U32|Mux4~1                                                                                                                     ; 2       ;
; sen:U32|Mux4~0                                                                                                                     ; 2       ;
; sen:U32|Mux2~14                                                                                                                    ; 2       ;
; sen:U32|Mux3~1                                                                                                                     ; 2       ;
; sen:U32|Mux2~5                                                                                                                     ; 2       ;
; sen:U32|Mux3~0                                                                                                                     ; 2       ;
; sen:U32|Mux2~2                                                                                                                     ; 2       ;
; sen:U32|Mux0~0                                                                                                                     ; 2       ;
; FF2:U34|Equal0~4                                                                                                                   ; 2       ;
; divisor3:U3|Qint[1]                                                                                                                ; 2       ;
; divisor3:U3|Qint[2]                                                                                                                ; 2       ;
; divisor3:U3|Qint[3]                                                                                                                ; 2       ;
; divisor3:U3|Qint[6]                                                                                                                ; 2       ;
; divisor3:U3|Qint[7]                                                                                                                ; 2       ;
; divisor3:U3|Qint[4]                                                                                                                ; 2       ;
; divisor3:U3|Qint[5]                                                                                                                ; 2       ;
; divisor3:U3|Qint[8]                                                                                                                ; 2       ;
; divisor3:U3|Qint[9]                                                                                                                ; 2       ;
; divisor3:U3|Qint[10]                                                                                                               ; 2       ;
; FF2:U34|Equal0~2                                                                                                                   ; 2       ;
; amplitud:U7|amp1e[6]                                                                                                               ; 2       ;
; amplitud:U25|amp1e[6]                                                                                                              ; 2       ;
; amplitud:U7|amp8e[1]                                                                                                               ; 2       ;
; amplitud:U7|amp2e[1]                                                                                                               ; 2       ;
; FF2:U17|B15_FF[1]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[2]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[3]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[4]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[5]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[6]                                                                                                                  ; 2       ;
; FF2:U17|B15_FF[7]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[1]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[2]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[3]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[4]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[5]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[6]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[7]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[1]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[2]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[3]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[4]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[5]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[6]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[7]                                                                                                                  ; 2       ;
; amplitud:U25|amp8e[1]                                                                                                              ; 2       ;
; amplitud:U25|amp2e[1]                                                                                                              ; 2       ;
; FF2:U34|B15_FF[1]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[2]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[3]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[4]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[5]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[6]                                                                                                                  ; 2       ;
; FF2:U34|B15_FF[7]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[1]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[2]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[3]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[4]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[5]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[6]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[7]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[1]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[2]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[3]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[4]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[5]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[6]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[7]                                                                                                                  ; 2       ;
; amplitud:U7|amp10e[1]                                                                                                              ; 2       ;
; FF2:U17|B15_FF[0]                                                                                                                  ; 2       ;
; FF2:U17|B16_FF[0]                                                                                                                  ; 2       ;
; FF2:U17|B17_FF[0]                                                                                                                  ; 2       ;
; FF2:U34|Equal0~0                                                                                                                   ; 2       ;
; amplitud:U25|amp10e[1]                                                                                                             ; 2       ;
; FF2:U34|B15_FF[0]                                                                                                                  ; 2       ;
; FF2:U34|B16_FF[0]                                                                                                                  ; 2       ;
; FF2:U34|B17_FF[0]                                                                                                                  ; 2       ;
; g00_audio_interface:U4|WideOr5~0                                                                                                   ; 2       ;
; g00_audio_interface:U4|WideOr3~1                                                                                                   ; 2       ;
; g00_audio_interface:U4|SCI_WORD1[0]                                                                                                ; 2       ;
; amplitud:U7|amp8[2]                                                                                                                ; 2       ;
; amplitud:U7|amp8[3]                                                                                                                ; 2       ;
; amplitud:U7|amp9[2]                                                                                                                ; 2       ;
; amplitud:U7|amp4[2]                                                                                                                ; 2       ;
; amplitud:U7|amp4[3]                                                                                                                ; 2       ;
; amplitud:U7|amp4[4]                                                                                                                ; 2       ;
; amplitud:U7|amp4[5]                                                                                                                ; 2       ;
; amplitud:U7|amp4[6]                                                                                                                ; 2       ;
; amplitud:U7|amp5[2]                                                                                                                ; 2       ;
; amplitud:U7|amp5[3]                                                                                                                ; 2       ;
; amplitud:U7|amp5[4]                                                                                                                ; 2       ;
; amplitud:U7|amp7[2]                                                                                                                ; 2       ;
; amplitud:U7|amp7[3]                                                                                                                ; 2       ;
; amplitud:U7|amp7[4]                                                                                                                ; 2       ;
; amplitud:U7|amp6[2]                                                                                                                ; 2       ;
; amplitud:U7|amp6[3]                                                                                                                ; 2       ;
; amplitud:U7|amp6[4]                                                                                                                ; 2       ;
; amplitud:U7|amp2[2]                                                                                                                ; 2       ;
; amplitud:U7|amp2[3]                                                                                                                ; 2       ;
; amplitud:U7|amp2[4]                                                                                                                ; 2       ;
; amplitud:U7|amp2[5]                                                                                                                ; 2       ;
; amplitud:U7|amp2[6]                                                                                                                ; 2       ;
; amplitud:U7|amp2[7]                                                                                                                ; 2       ;
; amplitud:U7|amp3[2]                                                                                                                ; 2       ;
; amplitud:U7|amp3[3]                                                                                                                ; 2       ;
; amplitud:U7|amp3[4]                                                                                                                ; 2       ;
; amplitud:U7|amp3[5]                                                                                                                ; 2       ;
; amplitud:U7|amp3[6]                                                                                                                ; 2       ;
; amplitud:U7|ampfund[2]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[3]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[4]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[5]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[6]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[7]                                                                                                             ; 2       ;
; amplitud:U7|amp1[2]                                                                                                                ; 2       ;
; amplitud:U7|amp1[3]                                                                                                                ; 2       ;
; amplitud:U7|amp1[4]                                                                                                                ; 2       ;
; amplitud:U7|amp1[5]                                                                                                                ; 2       ;
; amplitud:U7|amp1[6]                                                                                                                ; 2       ;
; amplitud:U25|amp8[2]                                                                                                               ; 2       ;
; amplitud:U25|amp8[3]                                                                                                               ; 2       ;
; amplitud:U25|amp9[2]                                                                                                               ; 2       ;
; amplitud:U25|amp4[2]                                                                                                               ; 2       ;
; amplitud:U25|amp4[3]                                                                                                               ; 2       ;
; amplitud:U25|amp4[4]                                                                                                               ; 2       ;
; amplitud:U25|amp4[5]                                                                                                               ; 2       ;
; amplitud:U25|amp4[6]                                                                                                               ; 2       ;
; amplitud:U25|amp5[2]                                                                                                               ; 2       ;
; amplitud:U25|amp5[3]                                                                                                               ; 2       ;
; amplitud:U25|amp5[4]                                                                                                               ; 2       ;
; amplitud:U25|amp7[2]                                                                                                               ; 2       ;
; amplitud:U25|amp7[3]                                                                                                               ; 2       ;
; amplitud:U25|amp7[4]                                                                                                               ; 2       ;
; amplitud:U25|amp6[2]                                                                                                               ; 2       ;
; amplitud:U25|amp6[3]                                                                                                               ; 2       ;
; amplitud:U25|amp6[4]                                                                                                               ; 2       ;
; amplitud:U25|amp2[2]                                                                                                               ; 2       ;
; amplitud:U25|amp2[3]                                                                                                               ; 2       ;
; amplitud:U25|amp2[4]                                                                                                               ; 2       ;
; amplitud:U25|amp2[5]                                                                                                               ; 2       ;
; amplitud:U25|amp2[6]                                                                                                               ; 2       ;
; amplitud:U25|amp2[7]                                                                                                               ; 2       ;
; amplitud:U25|amp3[2]                                                                                                               ; 2       ;
; amplitud:U25|amp3[3]                                                                                                               ; 2       ;
; amplitud:U25|amp3[4]                                                                                                               ; 2       ;
; amplitud:U25|amp3[5]                                                                                                               ; 2       ;
; amplitud:U25|amp3[6]                                                                                                               ; 2       ;
; amplitud:U25|ampfund[2]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[3]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[4]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[5]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[6]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[7]                                                                                                            ; 2       ;
; amplitud:U25|amp1[2]                                                                                                               ; 2       ;
; amplitud:U25|amp1[3]                                                                                                               ; 2       ;
; amplitud:U25|amp1[4]                                                                                                               ; 2       ;
; amplitud:U25|amp1[5]                                                                                                               ; 2       ;
; amplitud:U25|amp1[6]                                                                                                               ; 2       ;
; amplitud:U7|amp8[0]                                                                                                                ; 2       ;
; amplitud:U7|amp8[1]                                                                                                                ; 2       ;
; amplitud:U7|amp9[0]                                                                                                                ; 2       ;
; amplitud:U7|amp9[1]                                                                                                                ; 2       ;
; amplitud:U7|amp4[0]                                                                                                                ; 2       ;
; amplitud:U7|amp4[1]                                                                                                                ; 2       ;
; amplitud:U7|amp5[0]                                                                                                                ; 2       ;
; amplitud:U7|amp5[1]                                                                                                                ; 2       ;
; amplitud:U7|amp6[0]                                                                                                                ; 2       ;
; amplitud:U7|amp6[1]                                                                                                                ; 2       ;
; amplitud:U7|amp7[0]                                                                                                                ; 2       ;
; amplitud:U7|amp7[1]                                                                                                                ; 2       ;
; amplitud:U7|amp2[0]                                                                                                                ; 2       ;
; amplitud:U7|amp2[1]                                                                                                                ; 2       ;
; amplitud:U7|amp3[0]                                                                                                                ; 2       ;
; amplitud:U7|amp3[1]                                                                                                                ; 2       ;
; amplitud:U7|ampfund[0]                                                                                                             ; 2       ;
; amplitud:U7|ampfund[1]                                                                                                             ; 2       ;
; amplitud:U7|amp1[0]                                                                                                                ; 2       ;
; amplitud:U7|amp1[1]                                                                                                                ; 2       ;
; amplitud:U25|amp8[0]                                                                                                               ; 2       ;
; amplitud:U25|amp8[1]                                                                                                               ; 2       ;
; amplitud:U25|amp9[0]                                                                                                               ; 2       ;
; amplitud:U25|amp9[1]                                                                                                               ; 2       ;
; amplitud:U25|amp4[0]                                                                                                               ; 2       ;
; amplitud:U25|amp4[1]                                                                                                               ; 2       ;
; amplitud:U25|amp5[0]                                                                                                               ; 2       ;
; amplitud:U25|amp5[1]                                                                                                               ; 2       ;
; amplitud:U25|amp6[0]                                                                                                               ; 2       ;
; amplitud:U25|amp6[1]                                                                                                               ; 2       ;
; amplitud:U25|amp7[0]                                                                                                               ; 2       ;
; amplitud:U25|amp7[1]                                                                                                               ; 2       ;
; amplitud:U25|amp2[0]                                                                                                               ; 2       ;
; amplitud:U25|amp2[1]                                                                                                               ; 2       ;
; amplitud:U25|amp3[0]                                                                                                               ; 2       ;
; amplitud:U25|amp3[1]                                                                                                               ; 2       ;
; amplitud:U25|ampfund[0]                                                                                                            ; 2       ;
; amplitud:U25|ampfund[1]                                                                                                            ; 2       ;
; amplitud:U25|amp1[0]                                                                                                               ; 2       ;
; amplitud:U25|amp1[1]                                                                                                               ; 2       ;
; invertir:U42|Salint[11]                                                                                                            ; 2       ;
; invertir:U42|Salint[10]                                                                                                            ; 2       ;
; invertir:U42|Salint[9]                                                                                                             ; 2       ;
; invertir:U42|Salint[8]                                                                                                             ; 2       ;
; invertir:U42|Salint[7]                                                                                                             ; 2       ;
; invertir:U42|Salint[6]                                                                                                             ; 2       ;
; invertir:U42|Salint[5]                                                                                                             ; 2       ;
; invertir:U42|Salint[3]                                                                                                             ; 2       ;
; invertir:U42|Salint[2]                                                                                                             ; 2       ;
; invertir:U42|Salint[1]                                                                                                             ; 2       ;
; divisor1:U1|Qint[1]                                                                                                                ; 2       ;
; divisor1:U1|Qint[2]                                                                                                                ; 2       ;
; divisor1:U1|Qint[3]                                                                                                                ; 2       ;
; divisor1:U1|Qint[5]                                                                                                                ; 2       ;
; divisor1:U1|Qint[6]                                                                                                                ; 2       ;
; divisor1:U1|Qint[4]                                                                                                                ; 2       ;
; divisor1:U1|Qint[7]                                                                                                                ; 2       ;
; divisor1:U1|Qint[8]                                                                                                                ; 2       ;
; divisor1:U1|Qint[9]                                                                                                                ; 2       ;
; divisor1:U1|Qint[10]                                                                                                               ; 2       ;
; invertir:U42|Salint[0]                                                                                                             ; 2       ;
; g00_audio_interface:U4|WideOr4~2                                                                                                   ; 2       ;
; g00_audio_interface:U4|Mux0~19                                                                                                     ; 2       ;
; g00_audio_interface:U4|Mux0~2                                                                                                      ; 2       ;
; g00_audio_interface:U4|AUD_BCLK                                                                                                    ; 2       ;
; arm:U10|Add2~26                                                                                                                    ; 2       ;
; arm:U10|Add2~24                                                                                                                    ; 2       ;
; arm:U10|Add2~22                                                                                                                    ; 2       ;
; arm:U10|Add2~20                                                                                                                    ; 2       ;
; arm:U10|Add2~18                                                                                                                    ; 2       ;
; arm:U10|Add2~16                                                                                                                    ; 2       ;
; arm:U10|Add2~14                                                                                                                    ; 2       ;
; arm:U10|Add2~12                                                                                                                    ; 2       ;
; arm:U10|Add2~10                                                                                                                    ; 2       ;
; arm:U10|Add2~8                                                                                                                     ; 2       ;
; arm:U10|Add2~6                                                                                                                     ; 2       ;
; arm:U27|Add2~26                                                                                                                    ; 2       ;
; arm:U27|Add2~24                                                                                                                    ; 2       ;
; arm:U27|Add2~22                                                                                                                    ; 2       ;
; arm:U27|Add2~20                                                                                                                    ; 2       ;
; arm:U27|Add2~18                                                                                                                    ; 2       ;
; arm:U27|Add2~16                                                                                                                    ; 2       ;
; arm:U27|Add2~14                                                                                                                    ; 2       ;
; arm:U27|Add2~12                                                                                                                    ; 2       ;
; arm:U27|Add2~10                                                                                                                    ; 2       ;
; arm:U27|Add2~8                                                                                                                     ; 2       ;
; arm:U27|Add2~6                                                                                                                     ; 2       ;
; arm:U10|B17_1[19]                                                                                                                  ; 2       ;
; arm:U10|B13_1[6]                                                                                                                   ; 2       ;
; arm:U10|B13_1[7]                                                                                                                   ; 2       ;
; arm:U10|B13_1[8]                                                                                                                   ; 2       ;
; arm:U10|B13_1[9]                                                                                                                   ; 2       ;
; arm:U10|B13_1[10]                                                                                                                  ; 2       ;
; arm:U10|B13_1[11]                                                                                                                  ; 2       ;
; arm:U10|B13_1[12]                                                                                                                  ; 2       ;
; arm:U10|B13_1[13]                                                                                                                  ; 2       ;
; arm:U10|B13_1[14]                                                                                                                  ; 2       ;
; arm:U10|B13_1[15]                                                                                                                  ; 2       ;
; arm:U10|B13_1[16]                                                                                                                  ; 2       ;
; arm:U10|B13_1[17]                                                                                                                  ; 2       ;
; arm:U10|B13_1[18]                                                                                                                  ; 2       ;
; arm:U10|B13_1[19]                                                                                                                  ; 2       ;
; arm:U10|B17_1[6]                                                                                                                   ; 2       ;
; arm:U10|B17_1[7]                                                                                                                   ; 2       ;
; arm:U10|B17_1[8]                                                                                                                   ; 2       ;
; arm:U10|B17_1[9]                                                                                                                   ; 2       ;
; arm:U10|B17_1[10]                                                                                                                  ; 2       ;
; arm:U10|B17_1[11]                                                                                                                  ; 2       ;
; arm:U10|B17_1[12]                                                                                                                  ; 2       ;
; arm:U10|B17_1[13]                                                                                                                  ; 2       ;
; arm:U10|B17_1[14]                                                                                                                  ; 2       ;
; arm:U10|B17_1[15]                                                                                                                  ; 2       ;
; arm:U10|B17_1[16]                                                                                                                  ; 2       ;
; arm:U10|B17_1[17]                                                                                                                  ; 2       ;
; arm:U10|B17_1[18]                                                                                                                  ; 2       ;
; arm:U27|B17_1[19]                                                                                                                  ; 2       ;
; arm:U27|B13_1[6]                                                                                                                   ; 2       ;
; arm:U27|B13_1[7]                                                                                                                   ; 2       ;
; arm:U27|B13_1[8]                                                                                                                   ; 2       ;
; arm:U27|B13_1[9]                                                                                                                   ; 2       ;
; arm:U27|B13_1[10]                                                                                                                  ; 2       ;
; arm:U27|B13_1[11]                                                                                                                  ; 2       ;
; arm:U27|B13_1[12]                                                                                                                  ; 2       ;
; arm:U27|B13_1[13]                                                                                                                  ; 2       ;
; arm:U27|B13_1[14]                                                                                                                  ; 2       ;
; arm:U27|B13_1[15]                                                                                                                  ; 2       ;
; arm:U27|B13_1[16]                                                                                                                  ; 2       ;
; arm:U27|B13_1[17]                                                                                                                  ; 2       ;
; arm:U27|B13_1[18]                                                                                                                  ; 2       ;
; arm:U27|B13_1[19]                                                                                                                  ; 2       ;
; arm:U27|B17_1[6]                                                                                                                   ; 2       ;
; arm:U27|B17_1[7]                                                                                                                   ; 2       ;
; arm:U27|B17_1[8]                                                                                                                   ; 2       ;
; arm:U27|B17_1[9]                                                                                                                   ; 2       ;
; arm:U27|B17_1[10]                                                                                                                  ; 2       ;
; arm:U27|B17_1[11]                                                                                                                  ; 2       ;
; arm:U27|B17_1[12]                                                                                                                  ; 2       ;
; arm:U27|B17_1[13]                                                                                                                  ; 2       ;
; arm:U27|B17_1[14]                                                                                                                  ; 2       ;
; arm:U27|B17_1[15]                                                                                                                  ; 2       ;
; arm:U27|B17_1[16]                                                                                                                  ; 2       ;
; arm:U27|B17_1[17]                                                                                                                  ; 2       ;
; arm:U27|B17_1[18]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[12]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[11]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[17]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[13]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[15]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[14]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[16]                                                                                                                  ; 2       ;
; acum:U11|B15_2[19]                                                                                                                 ; 2       ;
; acum:U11|B10_2[19]                                                                                                                 ; 2       ;
; acum:U11|B14_2[19]                                                                                                                 ; 2       ;
; acum:U11|B11_2[19]                                                                                                                 ; 2       ;
; acum:U11|B5_2[19]                                                                                                                  ; 2       ;
; acum:U11|Bf_2[19]                                                                                                                  ; 2       ;
; acum:U11|B1_2[19]                                                                                                                  ; 2       ;
; acum:U11|B4_2[19]                                                                                                                  ; 2       ;
; acum:U11|B13_2[19]                                                                                                                 ; 2       ;
; acum:U11|B8_2[19]                                                                                                                  ; 2       ;
; acum:U11|B9_2[19]                                                                                                                  ; 2       ;
; acum:U11|B12_2[19]                                                                                                                 ; 2       ;
; acum:U11|B7_2[19]                                                                                                                  ; 2       ;
; acum:U11|B2_2[19]                                                                                                                  ; 2       ;
; acum:U11|B6_2[19]                                                                                                                  ; 2       ;
; acum:U11|B3_2[19]                                                                                                                  ; 2       ;
; acum:U11|B19_2[19]                                                                                                                 ; 2       ;
; acum:U11|B16_2[19]                                                                                                                 ; 2       ;
; acum:U11|B18_2[19]                                                                                                                 ; 2       ;
; acum:U11|B17_2[19]                                                                                                                 ; 2       ;
; acum:U11|B15_2[11]                                                                                                                 ; 2       ;
; acum:U11|B15_2[12]                                                                                                                 ; 2       ;
; acum:U11|B15_2[13]                                                                                                                 ; 2       ;
; acum:U11|B15_2[14]                                                                                                                 ; 2       ;
; acum:U11|B15_2[15]                                                                                                                 ; 2       ;
; acum:U11|B15_2[16]                                                                                                                 ; 2       ;
; acum:U11|B15_2[17]                                                                                                                 ; 2       ;
; acum:U11|B15_2[18]                                                                                                                 ; 2       ;
; acum:U11|B5_2[11]                                                                                                                  ; 2       ;
; acum:U11|B5_2[12]                                                                                                                  ; 2       ;
; acum:U11|B5_2[13]                                                                                                                  ; 2       ;
; acum:U11|B5_2[14]                                                                                                                  ; 2       ;
; acum:U11|B5_2[15]                                                                                                                  ; 2       ;
; acum:U11|B5_2[16]                                                                                                                  ; 2       ;
; acum:U11|B5_2[17]                                                                                                                  ; 2       ;
; acum:U11|B5_2[18]                                                                                                                  ; 2       ;
; acum:U11|B13_2[11]                                                                                                                 ; 2       ;
; acum:U11|B13_2[12]                                                                                                                 ; 2       ;
; acum:U11|B13_2[13]                                                                                                                 ; 2       ;
; acum:U11|B13_2[14]                                                                                                                 ; 2       ;
+------------------------------------------------------------------------------------------------------------------------------------+---------+


+-----------------------------------------------------------------------------------------------+
; Fitter DSP Block Usage Summary                                                                ;
+---------------------------------------+-------------+---------------------+-------------------+
; Statistic                             ; Number Used ; Available per Block ; Maximum Available ;
+---------------------------------------+-------------+---------------------+-------------------+
; Simple Multipliers (9-bit)            ; 20          ; 2                   ; 532               ;
; Simple Multipliers (18-bit)           ; 0           ; 1                   ; 266               ;
; Embedded Multiplier Blocks            ; 11          ; --                  ; 266               ;
; Embedded Multiplier 9-bit elements    ; 20          ; 2                   ; 532               ;
; Signed Embedded Multipliers           ; 0           ; --                  ; --                ;
; Unsigned Embedded Multipliers         ; 20          ; --                  ; --                ;
; Mixed Sign Embedded Multipliers       ; 0           ; --                  ; --                ;
; Variable Sign Embedded Multipliers    ; 0           ; --                  ; --                ;
; Dedicated Input Shift Register Chains ; 0           ; --                  ; --                ;
+---------------------------------------+-------------+---------------------+-------------------+


+------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; DSP Block Details                                                                                                                                                                                                                                          ;
+--------------------------------------------------------------+---------------------------+--------------------+---------------------+--------------------------------+-----------------------+-----------------------+-------------------+-----------------+
; Name                                                         ; Mode                      ; Location           ; Sign Representation ; Has Input Shift Register Chain ; Data A Input Register ; Data B Input Register ; Pipeline Register ; Output Register ;
+--------------------------------------------------------------+---------------------------+--------------------+---------------------+--------------------------------+-----------------------+-----------------------+-------------------+-----------------+
; mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X44_Y43_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X44_Y43_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X44_Y43_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ;                           ; DSPMULT_X44_Y43_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y42_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y42_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y43_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y43_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y43_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y43_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y40_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y40_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y40_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y40_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X44_Y41_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X44_Y41_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X44_Y41_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X44_Y41_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X44_Y42_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U35|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X44_Y42_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y50_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult1|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y50_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y47_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult0|mult_aat:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y47_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y47_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult3|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y47_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y49_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult2|mult_aat:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y49_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y49_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult7|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y49_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y48_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult6|mult_7at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y48_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y46_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult5|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y46_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y46_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult4|mult_8at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y46_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X71_Y48_N3  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult9|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X71_Y48_N1 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
; mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_out2     ; Simple Multiplier (9-bit) ; DSPOUT_X93_Y50_N2  ;                     ; No                             ;                       ;                       ;                   ; no              ;
;    mult:U18|lpm_mult:Mult8|mult_4at:auto_generated|mac_mult1 ;                           ; DSPMULT_X93_Y50_N0 ; Unsigned            ;                                ; yes                   ; no                    ; no                ;                 ;
+--------------------------------------------------------------+---------------------------+--------------------+---------------------+--------------------------------+-----------------------+-----------------------+-------------------+-----------------+


+--------------------------------------------------------+
; Interconnect Usage Summary                             ;
+----------------------------+---------------------------+
; Interconnect Resource Type ; Usage                     ;
+----------------------------+---------------------------+
; Block interconnects        ; 9,683 / 342,891 ( 3 % )   ;
; C16 interconnects          ; 244 / 10,120 ( 2 % )      ;
; C4 interconnects           ; 4,243 / 209,544 ( 2 % )   ;
; Direct links               ; 1,874 / 342,891 ( < 1 % ) ;
; Global clocks              ; 4 / 20 ( 20 % )           ;
; Local interconnects        ; 3,159 / 119,088 ( 3 % )   ;
; R24 interconnects          ; 298 / 9,963 ( 3 % )       ;
; R4 interconnects           ; 6,179 / 289,782 ( 2 % )   ;
+----------------------------+---------------------------+


+-----------------------------------------------------------------------------+
; LAB Logic Elements                                                          ;
+---------------------------------------------+-------------------------------+
; Number of Logic Elements  (Average = 13.09) ; Number of LABs  (Total = 577) ;
+---------------------------------------------+-------------------------------+
; 1                                           ; 14                            ;
; 2                                           ; 6                             ;
; 3                                           ; 7                             ;
; 4                                           ; 7                             ;
; 5                                           ; 6                             ;
; 6                                           ; 7                             ;
; 7                                           ; 6                             ;
; 8                                           ; 23                            ;
; 9                                           ; 59                            ;
; 10                                          ; 26                            ;
; 11                                          ; 15                            ;
; 12                                          ; 13                            ;
; 13                                          ; 17                            ;
; 14                                          ; 22                            ;
; 15                                          ; 47                            ;
; 16                                          ; 302                           ;
+---------------------------------------------+-------------------------------+


+--------------------------------------------------------------------+
; LAB-wide Signals                                                   ;
+------------------------------------+-------------------------------+
; LAB-wide Signals  (Average = 1.78) ; Number of LABs  (Total = 577) ;
+------------------------------------+-------------------------------+
; 1 Async. clear                     ; 16                            ;
; 1 Clock                            ; 416                           ;
; 1 Clock enable                     ; 275                           ;
; 1 Sync. clear                      ; 98                            ;
; 1 Sync. load                       ; 91                            ;
; 2 Clock enables                    ; 86                            ;
; 2 Clocks                           ; 43                            ;
+------------------------------------+-------------------------------+


+------------------------------------------------------------------------------+
; LAB Signals Sourced                                                          ;
+----------------------------------------------+-------------------------------+
; Number of Signals Sourced  (Average = 18.41) ; Number of LABs  (Total = 577) ;
+----------------------------------------------+-------------------------------+
; 0                                            ; 0                             ;
; 1                                            ; 4                             ;
; 2                                            ; 11                            ;
; 3                                            ; 1                             ;
; 4                                            ; 6                             ;
; 5                                            ; 3                             ;
; 6                                            ; 7                             ;
; 7                                            ; 1                             ;
; 8                                            ; 20                            ;
; 9                                            ; 28                            ;
; 10                                           ; 20                            ;
; 11                                           ; 8                             ;
; 12                                           ; 11                            ;
; 13                                           ; 7                             ;
; 14                                           ; 9                             ;
; 15                                           ; 24                            ;
; 16                                           ; 50                            ;
; 17                                           ; 25                            ;
; 18                                           ; 52                            ;
; 19                                           ; 23                            ;
; 20                                           ; 53                            ;
; 21                                           ; 30                            ;
; 22                                           ; 40                            ;
; 23                                           ; 26                            ;
; 24                                           ; 14                            ;
; 25                                           ; 12                            ;
; 26                                           ; 14                            ;
; 27                                           ; 10                            ;
; 28                                           ; 14                            ;
; 29                                           ; 10                            ;
; 30                                           ; 10                            ;
; 31                                           ; 8                             ;
; 32                                           ; 26                            ;
+----------------------------------------------+-------------------------------+


+---------------------------------------------------------------------------------+
; LAB Signals Sourced Out                                                         ;
+-------------------------------------------------+-------------------------------+
; Number of Signals Sourced Out  (Average = 8.92) ; Number of LABs  (Total = 577) ;
+-------------------------------------------------+-------------------------------+
; 0                                               ; 12                            ;
; 1                                               ; 22                            ;
; 2                                               ; 18                            ;
; 3                                               ; 22                            ;
; 4                                               ; 36                            ;
; 5                                               ; 40                            ;
; 6                                               ; 44                            ;
; 7                                               ; 26                            ;
; 8                                               ; 44                            ;
; 9                                               ; 80                            ;
; 10                                              ; 49                            ;
; 11                                              ; 25                            ;
; 12                                              ; 24                            ;
; 13                                              ; 30                            ;
; 14                                              ; 24                            ;
; 15                                              ; 27                            ;
; 16                                              ; 28                            ;
; 17                                              ; 8                             ;
; 18                                              ; 2                             ;
; 19                                              ; 1                             ;
; 20                                              ; 6                             ;
; 21                                              ; 2                             ;
; 22                                              ; 1                             ;
; 23                                              ; 0                             ;
; 24                                              ; 1                             ;
; 25                                              ; 2                             ;
; 26                                              ; 1                             ;
; 27                                              ; 2                             ;
+-------------------------------------------------+-------------------------------+


+------------------------------------------------------------------------------+
; LAB Distinct Inputs                                                          ;
+----------------------------------------------+-------------------------------+
; Number of Distinct Inputs  (Average = 15.51) ; Number of LABs  (Total = 577) ;
+----------------------------------------------+-------------------------------+
; 0                                            ; 0                             ;
; 1                                            ; 0                             ;
; 2                                            ; 6                             ;
; 3                                            ; 9                             ;
; 4                                            ; 5                             ;
; 5                                            ; 10                            ;
; 6                                            ; 11                            ;
; 7                                            ; 15                            ;
; 8                                            ; 34                            ;
; 9                                            ; 26                            ;
; 10                                           ; 35                            ;
; 11                                           ; 44                            ;
; 12                                           ; 32                            ;
; 13                                           ; 31                            ;
; 14                                           ; 28                            ;
; 15                                           ; 33                            ;
; 16                                           ; 34                            ;
; 17                                           ; 30                            ;
; 18                                           ; 27                            ;
; 19                                           ; 19                            ;
; 20                                           ; 14                            ;
; 21                                           ; 22                            ;
; 22                                           ; 4                             ;
; 23                                           ; 13                            ;
; 24                                           ; 13                            ;
; 25                                           ; 15                            ;
; 26                                           ; 7                             ;
; 27                                           ; 8                             ;
; 28                                           ; 8                             ;
; 29                                           ; 11                            ;
; 30                                           ; 15                            ;
; 31                                           ; 4                             ;
; 32                                           ; 9                             ;
; 33                                           ; 1                             ;
; 34                                           ; 3                             ;
+----------------------------------------------+-------------------------------+


+------------------------------------------+
; I/O Rules Summary                        ;
+----------------------------------+-------+
; I/O Rules Statistic              ; Total ;
+----------------------------------+-------+
; Total I/O Rules                  ; 30    ;
; Number of I/O Rules Passed       ; 12    ;
; Number of I/O Rules Failed       ; 0     ;
; Number of I/O Rules Unchecked    ; 0     ;
; Number of I/O Rules Inapplicable ; 18    ;
+----------------------------------+-------+


+-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; I/O Rules Details                                                                                                                                                                                                                                                                                   ;
+--------------+-----------+-----------------------------------+------------------------------------------------------------------------------------------------------+----------+--------------------------------------------------------------------------+---------------------+-------------------+
; Status       ; ID        ; Category                          ; Rule Description                                                                                     ; Severity ; Information                                                              ; Area                ; Extra Information ;
+--------------+-----------+-----------------------------------+------------------------------------------------------------------------------------------------------+----------+--------------------------------------------------------------------------+---------------------+-------------------+
; Pass         ; IO_000001 ; Capacity Checks                   ; Number of pins in an I/O bank should not exceed the number of locations available.                   ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000002 ; Capacity Checks                   ; Number of clocks in an I/O bank should not exceed the number of clocks available.                    ; Critical ; No Global Signal assignments found.                                      ; I/O                 ;                   ;
; Pass         ; IO_000003 ; Capacity Checks                   ; Number of pins in a Vrefgroup should not exceed the number of locations available.                   ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000004 ; Voltage Compatibility Checks      ; The I/O bank should support the requested VCCIO.                                                     ; Critical ; No IOBANK_VCCIO assignments found.                                       ; I/O                 ;                   ;
; Inapplicable ; IO_000005 ; Voltage Compatibility Checks      ; The I/O bank should not have competing VREF values.                                                  ; Critical ; No VREF I/O Standard assignments found.                                  ; I/O                 ;                   ;
; Pass         ; IO_000006 ; Voltage Compatibility Checks      ; The I/O bank should not have competing VCCIO values.                                                 ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Pass         ; IO_000007 ; Valid Location Checks             ; Checks for unavailable locations.                                                                    ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000008 ; Valid Location Checks             ; Checks for reserved locations.                                                                       ; Critical ; No reserved LogicLock region found.                                      ; I/O                 ;                   ;
; Pass         ; IO_000009 ; I/O Properties Checks for One I/O ; The location should support the requested I/O standard.                                              ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Pass         ; IO_000010 ; I/O Properties Checks for One I/O ; The location should support the requested I/O direction.                                             ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000011 ; I/O Properties Checks for One I/O ; The location should support the requested Current Strength.                                          ; Critical ; No Current Strength assignments found.                                   ; I/O                 ;                   ;
; Pass         ; IO_000012 ; I/O Properties Checks for One I/O ; The location should support the requested On Chip Termination value.                                 ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000013 ; I/O Properties Checks for One I/O ; The location should support the requested Bus Hold value.                                            ; Critical ; No Enable Bus-Hold Circuitry assignments found.                          ; I/O                 ;                   ;
; Inapplicable ; IO_000014 ; I/O Properties Checks for One I/O ; The location should support the requested Weak Pull Up value.                                        ; Critical ; No Weak Pull-Up Resistor assignments found.                              ; I/O                 ;                   ;
; Pass         ; IO_000015 ; I/O Properties Checks for One I/O ; The location should support the requested PCI Clamp Diode.                                           ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000018 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested Current Strength.                                      ; Critical ; No Current Strength assignments found.                                   ; I/O                 ;                   ;
; Pass         ; IO_000019 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested On Chip Termination value.                             ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Pass         ; IO_000020 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested PCI Clamp Diode.                                       ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000021 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested Weak Pull Up value.                                    ; Critical ; No Weak Pull-Up Resistor assignments found.                              ; I/O                 ;                   ;
; Inapplicable ; IO_000022 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested Bus Hold value.                                        ; Critical ; No Enable Bus-Hold Circuitry assignments found.                          ; I/O                 ;                   ;
; Inapplicable ; IO_000023 ; I/O Properties Checks for One I/O ; The I/O standard should support the Open Drain value.                                                ; Critical ; No open drain assignments found.                                         ; I/O                 ;                   ;
; Pass         ; IO_000024 ; I/O Properties Checks for One I/O ; The I/O direction should support the On Chip Termination value.                                      ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000026 ; I/O Properties Checks for One I/O ; On Chip Termination and Current Strength should not be used at the same time.                        ; Critical ; No Current Strength assignments found.                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000027 ; I/O Properties Checks for One I/O ; Weak Pull Up and Bus Hold should not be used at the same time.                                       ; Critical ; No Enable Bus-Hold Circuitry or Weak Pull-Up Resistor assignments found. ; I/O                 ;                   ;
; Inapplicable ; IO_000045 ; I/O Properties Checks for One I/O ; The I/O standard should support the requested Slew Rate value.                                       ; Critical ; No Slew Rate assignments found.                                          ; I/O                 ;                   ;
; Inapplicable ; IO_000046 ; I/O Properties Checks for One I/O ; The location should support the requested Slew Rate value.                                           ; Critical ; No Slew Rate assignments found.                                          ; I/O                 ;                   ;
; Inapplicable ; IO_000047 ; I/O Properties Checks for One I/O ; On Chip Termination and Slew Rate should not be used at the same time.                               ; Critical ; No Slew Rate assignments found.                                          ; I/O                 ;                   ;
; Pass         ; IO_000033 ; Electromigration Checks           ; Current density for consecutive I/Os should not exceed 240mA for row I/Os and 240mA for column I/Os. ; Critical ; 0 such failures found.                                                   ; I/O                 ;                   ;
; Inapplicable ; IO_000034 ; SI Related Distance Checks        ; Single-ended outputs should be 5 LAB row(s) away from a differential I/O.                            ; High     ; No Differential I/O Standard assignments found.                          ; I/O                 ;                   ;
; Inapplicable ; IO_000042 ; SI Related SSO Limit Checks       ; No more than 20 outputs are allowed in a VREF group when VREF is being read from.                    ; High     ; No VREF I/O Standard assignments found.                                  ; I/O                 ;                   ;
; ----         ; ----      ; Disclaimer                        ; OCT rules are checked but not reported.                                                              ; None     ; ----                                                                     ; On Chip Termination ;                   ;
+--------------+-----------+-----------------------------------+------------------------------------------------------------------------------------------------------+----------+--------------------------------------------------------------------------+---------------------+-------------------+


+--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+
; I/O Rules Matrix                                                                                                                                                                                                                                                                                                                                                                                                                                                         ;
+--------------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+-----------+-----------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+
; Pin/Rules          ; IO_000001    ; IO_000002    ; IO_000003    ; IO_000004    ; IO_000005    ; IO_000006 ; IO_000007    ; IO_000008    ; IO_000009 ; IO_000010 ; IO_000011    ; IO_000012    ; IO_000013    ; IO_000014    ; IO_000015    ; IO_000018    ; IO_000019    ; IO_000020    ; IO_000021    ; IO_000022    ; IO_000023    ; IO_000024    ; IO_000026    ; IO_000027    ; IO_000045    ; IO_000046    ; IO_000047    ; IO_000033 ; IO_000034    ; IO_000042    ;
+--------------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+-----------+-----------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+
; Total Pass         ; 56           ; 0            ; 56           ; 0            ; 0            ; 57        ; 56           ; 0            ; 57        ; 57        ; 0            ; 25           ; 0            ; 0            ; 33           ; 0            ; 25           ; 33           ; 0            ; 0            ; 0            ; 25           ; 0            ; 0            ; 0            ; 0            ; 0            ; 57        ; 0            ; 0            ;
; Total Unchecked    ; 0            ; 0            ; 0            ; 0            ; 0            ; 0         ; 0            ; 0            ; 0         ; 0         ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0         ; 0            ; 0            ;
; Total Inapplicable ; 1            ; 57           ; 1            ; 57           ; 57           ; 0         ; 1            ; 57           ; 0         ; 0         ; 57           ; 32           ; 57           ; 57           ; 24           ; 57           ; 32           ; 24           ; 57           ; 57           ; 57           ; 32           ; 57           ; 57           ; 57           ; 57           ; 57           ; 0         ; 57           ; 57           ;
; Total Fail         ; 0            ; 0            ; 0            ; 0            ; 0            ; 0         ; 0            ; 0            ; 0         ; 0         ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0            ; 0         ; 0            ; 0            ;
; LED_config[0]      ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; LED_config[1]      ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; LED_config[2]      ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; LED_modo           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; LED_inst[0]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; LED_inst[1]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[0]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[1]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[2]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[3]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[4]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[5]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[6]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[7]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[8]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[9]         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[10]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sal_LED[11]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; pulse_48KHz        ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; AUD_MCLK           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; AUD_BCLK           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; AUD_DACDAT         ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; AUD_DACLRCK        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; I2C_SDAT           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Pass         ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; I2C_SCLK           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; sel                ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; num_inst[0]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; num_inst[1]        ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; RST                ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; CLK                ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; W_EN               ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; INIT               ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[0]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[1]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[2]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[3]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[4]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[5]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[6]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[7]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[8]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[9]       ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[10]      ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas_int[11]      ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[0]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; en                 ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[1]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[2]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[3]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[5]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[6]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[7]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[8]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[9]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[10]          ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[11]          ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
; notas[4]           ; Pass         ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass      ; Pass         ; Inapplicable ; Pass      ; Pass      ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Pass         ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Inapplicable ; Pass      ; Inapplicable ; Inapplicable ;
+--------------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+-----------+-----------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+--------------+-----------+--------------+--------------+


+---------------------------------------------------------------------------------------------+
; Fitter Device Options                                                                       ;
+------------------------------------------------------------------+--------------------------+
; Option                                                           ; Setting                  ;
+------------------------------------------------------------------+--------------------------+
; Enable user-supplied start-up clock (CLKUSR)                     ; Off                      ;
; Enable device-wide reset (DEV_CLRn)                              ; Off                      ;
; Enable device-wide output enable (DEV_OE)                        ; Off                      ;
; Enable INIT_DONE output                                          ; Off                      ;
; Configuration scheme                                             ; Active Serial            ;
; Error detection CRC                                              ; Off                      ;
; Enable open drain on CRC_ERROR pin                               ; Off                      ;
; Enable input tri-state on active configuration pins in user mode ; Off                      ;
; Configuration Voltage Level                                      ; Auto                     ;
; Force Configuration Voltage Level                                ; Off                      ;
; nCEO                                                             ; As output driving ground ;
; Data[0]                                                          ; As input tri-stated      ;
; Data[1]/ASDO                                                     ; As input tri-stated      ;
; Data[7..2]                                                       ; Unreserved               ;
; FLASH_nCE/nCSO                                                   ; As input tri-stated      ;
; Other Active Parallel pins                                       ; Unreserved               ;
; DCLK                                                             ; As output driving ground ;
; Base pin-out file on sameframe device                            ; Off                      ;
+------------------------------------------------------------------+--------------------------+


+------------------------------------+
; Operating Settings and Conditions  ;
+---------------------------+--------+
; Setting                   ; Value  ;
+---------------------------+--------+
; Nominal Core Voltage      ; 1.20 V ;
; Low Junction Temperature  ; 0 °C   ;
; High Junction Temperature ; 85 °C  ;
+---------------------------+--------+


+------------------------------------------------------------+
; Estimated Delay Added for Hold Timing Summary              ;
+-----------------+----------------------+-------------------+
; Source Clock(s) ; Destination Clock(s) ; Delay Added in ns ;
+-----------------+----------------------+-------------------+
Note: For more information on problematic transfers, consider running the Fitter again with the Optimize hold timing option (Settings Menu) turned off.
This will disable optimization of problematic paths and expose them for further analysis using either the TimeQuest Timing Analyzer or the Classic Timing Analyzer.


+-----------------------------------------------------------------------------------------+
; Estimated Delay Added for Hold Timing Details                                           ;
+----------------------------------+----------------------------------+-------------------+
; Source Register                  ; Destination Register             ; Delay Added in ns ;
+----------------------------------+----------------------------------+-------------------+
; g00_audio_interface:U4|Bcount[1] ; g00_audio_interface:U4|Bcount[2] ; 0.021             ;
; fase:U24|fase18[8]               ; FF1:U30|F18[8]                   ; 0.021             ;
; fase:U6|fase10[8]                ; FF1:U13|F10[8]                   ; 0.020             ;
; fase:U6|fase1[8]                 ; FF1:U13|F1[8]                    ; 0.020             ;
; fase:U6|fase6[8]                 ; FF1:U13|F6[8]                    ; 0.020             ;
; fase:U6|fase11[8]                ; FF1:U13|F11[8]                   ; 0.018             ;
+----------------------------------+----------------------------------+-------------------+


+-----------------+
; Fitter Messages ;
+-----------------+
Info: *******************************************************************
Info: Running Quartus II 32-bit Fitter
    Info: Version 12.0 Build 263 08/02/2012 Service Pack 2 SJ Web Edition
    Info: Processing started: Sat Jun 29 12:50:48 2013
Info: Command: quartus_fit --read_settings_files=off --write_settings_files=off Proyecto -c Proyecto
Warning (20028): Parallel compilation is not licensed and has been disabled
Info (119006): Selected device EP4CE115F29C7 for design "Proyecto"
Info (21077): Core supply voltage is 1.2V
Info (21077): Low junction temperature is 0 degrees C
Info (21077): High junction temperature is 85 degrees C
Info (171003): Fitter is performing an Auto Fit compilation, which may decrease Fitter effort to reduce compilation time
Warning (292013): Feature LogicLock is only available with a valid subscription license. You can purchase a software subscription to gain full access to this feature.
Info (176444): Device migration not selected. If you intend to use device migration later, you may need to change the pin assignments as they may be incompatible with other devices
    Info (176445): Device EP4CE40F29C7 is compatible
    Info (176445): Device EP4CE40F29I7 is compatible
    Info (176445): Device EP4CE30F29C7 is compatible
    Info (176445): Device EP4CE30F29I7 is compatible
    Info (176445): Device EP4CE55F29C7 is compatible
    Info (176445): Device EP4CE55F29I7 is compatible
    Info (176445): Device EP4CE75F29C7 is compatible
    Info (176445): Device EP4CE75F29I7 is compatible
    Info (176445): Device EP4CE115F29I7 is compatible
Info (169124): Fitter converted 5 user pins into dedicated programming pins
    Info (169125): Pin ~ALTERA_ASDO_DATA1~ is reserved at location F4
    Info (169125): Pin ~ALTERA_FLASH_nCE_nCSO~ is reserved at location E2
    Info (169125): Pin ~ALTERA_DCLK~ is reserved at location P3
    Info (169125): Pin ~ALTERA_DATA0~ is reserved at location N7
    Info (169125): Pin ~ALTERA_nCEO~ is reserved at location P28
Warning (15714): Some pins have incomplete I/O assignments. Refer to the I/O Assignment Warnings report for details
Critical Warning (169085): No exact pin location assignment(s) for 1 pins of 57 total pins
    Info (169086): Pin pulse_48KHz not assigned to an exact location on the device
Critical Warning (332012): Synopsys Design Constraints File file not found: 'Proyecto.sdc'. A Synopsys Design Constraints File is required by the TimeQuest Timing Analyzer to get proper timing constraints. Without it, the Compiler will not properly optimize the design.
Info (332144): No user constrained base clocks found in the design
Info (332143): No user constrained clock uncertainty found in the design. Calling "derive_clock_uncertainty"
Info (332123): Deriving Clock Uncertainty. Please refer to report_sdc in TimeQuest to see clock uncertainties.
Info (332130): Timing requirements not specified -- quality metrics such as performance may be sacrificed to reduce compilation time.
Info (176353): Automatically promoted node CLK~input (placed in PIN Y2 (CLK2, DIFFCLK_1p))
    Info (176355): Automatically promoted destinations to use location or clock signal Global Clock CLKCTRL_G4
Info (176353): Automatically promoted node divisor1:U1|sint 
    Info (176355): Automatically promoted destinations to use location or clock signal Global Clock
Info (176353): Automatically promoted node divisor3:U3|sint 
    Info (176355): Automatically promoted destinations to use location or clock signal Global Clock
Info (176353): Automatically promoted node divisor2:U2|sint 
    Info (176355): Automatically promoted destinations to use location or clock signal Global Clock
Info (176233): Starting register packing
Extra Info (176273): Performing register packing on registers with non-logic cell location assignments
Extra Info (176274): Completed register packing on registers with non-logic cell location assignments
Extra Info (176236): Started Fast Input/Output/OE register processing
Extra Info (176237): Finished Fast Input/Output/OE register processing
Extra Info (176248): Moving registers into I/O cells, Multiplier Blocks, and RAM blocks to improve timing and density
Extra Info (176249): Finished moving registers into I/O cells, Multiplier Blocks, and RAM blocks
Info (176235): Finished register packing
    Extra Info (176218): Packed 160 registers into blocks of type Embedded multiplier block
Info (176214): Statistics of I/O pins that need to be placed that use the same VCCIO and VREF, before I/O pin placement
    Info (176211): Number of I/O pins in group: 1 (unused VREF, 2.5V VCCIO, 0 input, 1 output, 0 bidirectional)
        Info (176212): I/O standards used: 2.5 V.
Info (176215): I/O bank details before I/O pin placement
    Info (176214): Statistics of I/O banks
        Info (176213): I/O bank number 1 does not use VREF pins and has 2.5V VCCIO pins. 8 total pin(s) used --  48 pins available
        Info (176213): I/O bank number 2 does not use VREF pins and has undetermined VCCIO pins. 1 total pin(s) used --  62 pins available
        Info (176213): I/O bank number 3 does not use VREF pins and has undetermined VCCIO pins. 0 total pin(s) used --  73 pins available
        Info (176213): I/O bank number 4 does not use VREF pins and has undetermined VCCIO pins. 12 total pin(s) used --  59 pins available
        Info (176213): I/O bank number 5 does not use VREF pins and has undetermined VCCIO pins. 19 total pin(s) used --  46 pins available
        Info (176213): I/O bank number 6 does not use VREF pins and has undetermined VCCIO pins. 1 total pin(s) used --  57 pins available
        Info (176213): I/O bank number 7 does not use VREF pins and has 2.5V VCCIO pins. 18 total pin(s) used --  54 pins available
        Info (176213): I/O bank number 8 does not use VREF pins and has 2.5V VCCIO pins. 2 total pin(s) used --  69 pins available
Info (171121): Fitter preparation operations ending: elapsed time is 00:00:25
Info (170189): Fitter placement preparation operations beginning
Info (170190): Fitter placement preparation operations ending: elapsed time is 00:00:13
Info (170191): Fitter placement operations beginning
Info (170137): Fitter placement was successful
Info (170192): Fitter placement operations ending: elapsed time is 00:01:12
Info (170193): Fitter routing operations beginning
Info (170195): Router estimated average interconnect usage is 1% of the available device resources
    Info (170196): Router estimated peak interconnect usage is 22% of the available device resources in the region that extends from location X69_Y37 to location X80_Y48
Info (170194): Fitter routing operations ending: elapsed time is 00:00:47
Info (170199): The Fitter performed an Auto Fit compilation.  Optimizations were skipped to reduce compilation time.
    Info (170201): Optimizations that may affect the design's routability were skipped
Info (334003): Started post-fitting delay annotation
Info (334004): Delay annotation completed successfully
Info (334003): Started post-fitting delay annotation
Info (334004): Delay annotation completed successfully
Info: Quartus II 32-bit Fitter was successful. 0 errors, 5 warnings
    Info: Peak virtual memory: 593 megabytes
    Info: Processing ended: Sat Jun 29 12:54:44 2013
    Info: Elapsed time: 00:03:56
    Info: Total CPU time (on all processors): 00:03:18


