


ARM Macro Assembler    Page 1 


    1 00000000         ;******************** (C) COPYRIGHT 2014 STMicroelectron
                       ics ********************
    2 00000000         ;* File Name          : startup_stm32f401xx.s
    3 00000000         ;* Author             : MCD Application Team
    4 00000000         ;* @version           : V1.4.0
    5 00000000         ;* @date              : 04-August-2014
    6 00000000         ;* Description        : STM32F401xx devices vector table
                        for MDK-ARM toolchain. 
    7 00000000         ;*                      This module performs:
    8 00000000         ;*                      - Set the initial SP
    9 00000000         ;*                      - Set the initial PC == Reset_Ha
                       ndler
   10 00000000         ;*                      - Set the vector table entries w
                       ith the exceptions ISR address
   11 00000000         ;*                      - Configure the system clock
   12 00000000         ;*                      - Branches to __main in the C li
                       brary (which eventually
   13 00000000         ;*                        calls main()).
   14 00000000         ;*                      After Reset the CortexM4 process
                       or is in Thread mode,
   15 00000000         ;*                      priority is Privileged, and the 
                       Stack is set to Main.
   16 00000000         ;* <<< Use Configuration Wizard in Context Menu >>>   
   17 00000000         ;*******************************************************
                       ************************
   18 00000000         ; 
   19 00000000         ; Licensed under MCD-ST Liberty SW License Agreement V2,
                        (the "License");
   20 00000000         ; You may not use this file except in compliance with th
                       e License.
   21 00000000         ; You may obtain a copy of the License at:
   22 00000000         ; 
   23 00000000         ;        http://www.st.com/software_license_agreement_li
                       berty_v2
   24 00000000         ; 
   25 00000000         ; Unless required by applicable law or agreed to in writ
                       ing, software 
   26 00000000         ; distributed under the License is distributed on an "AS
                        IS" BASIS, 
   27 00000000         ; WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either e
                       xpress or implied.
   28 00000000         ; See the License for the specific language governing pe
                       rmissions and
   29 00000000         ; limitations under the License.
   30 00000000         ; 
   31 00000000         ;*******************************************************
                       ************************
   32 00000000         
   33 00000000         ; Amount of memory (in bytes) allocated for Stack
   34 00000000         ; Tailor this value to your application needs
   35 00000000         ; <h> Stack Configuration
   36 00000000         ;   <o> Stack Size (in Bytes) <0x0-0xFFFFFFFF:8>
   37 00000000         ; </h>
   38 00000000         
   39 00000000 00000400 
                       Stack_Size
                               EQU              0x00000400
   40 00000000         
   41 00000000                 AREA             STACK, NOINIT, READWRITE, ALIGN



ARM Macro Assembler    Page 2 


=3
   42 00000000         Stack_Mem
                               SPACE            Stack_Size
   43 00000400         __initial_sp
   44 00000400         
   45 00000400         
   46 00000400         ; <h> Heap Configuration
   47 00000400         ;   <o>  Heap Size (in Bytes) <0x0-0xFFFFFFFF:8>
   48 00000400         ; </h>
   49 00000400         
   50 00000400 00000200 
                       Heap_Size
                               EQU              0x00000200
   51 00000400         
   52 00000400                 AREA             HEAP, NOINIT, READWRITE, ALIGN=
3
   53 00000000         __heap_base
   54 00000000         Heap_Mem
                               SPACE            Heap_Size
   55 00000200         __heap_limit
   56 00000200         
   57 00000200                 PRESERVE8
   58 00000200                 THUMB
   59 00000200         
   60 00000200         
   61 00000200         ; Vector Table Mapped to Address 0 at Reset
   62 00000200                 AREA             RESET, DATA, READONLY
   63 00000000                 EXPORT           __Vectors
   64 00000000                 EXPORT           __Vectors_End
   65 00000000                 EXPORT           __Vectors_Size
   66 00000000         
   67 00000000 00000000 
                       __Vectors
                               DCD              __initial_sp ; Top of Stack
   68 00000004 00000000        DCD              Reset_Handler ; Reset Handler
   69 00000008 00000000        DCD              NMI_Handler ; NMI Handler
   70 0000000C 00000000        DCD              HardFault_Handler ; Hard Fault 
                                                            Handler
   71 00000010 00000000        DCD              MemManage_Handler 
                                                            ; MPU Fault Handler
                                                            
   72 00000014 00000000        DCD              BusFault_Handler 
                                                            ; Bus Fault Handler
                                                            
   73 00000018 00000000        DCD              UsageFault_Handler ; Usage Faul
                                                            t Handler
   74 0000001C 00000000        DCD              0           ; Reserved
   75 00000020 00000000        DCD              0           ; Reserved
   76 00000024 00000000        DCD              0           ; Reserved
   77 00000028 00000000        DCD              0           ; Reserved
   78 0000002C 00000000        DCD              SVC_Handler ; SVCall Handler
   79 00000030 00000000        DCD              DebugMon_Handler ; Debug Monito
                                                            r Handler
   80 00000034 00000000        DCD              0           ; Reserved
   81 00000038 00000000        DCD              PendSV_Handler ; PendSV Handler
                                                            
   82 0000003C 00000000        DCD              SysTick_Handler 
                                                            ; SysTick Handler
   83 00000040         



ARM Macro Assembler    Page 3 


   84 00000040         ; External Interrupts
   85 00000040 00000000        DCD              WWDG_IRQHandler ; Window WatchD
                                                            og                 
                                                                               
                                                                
   86 00000044 00000000        DCD              PVD_IRQHandler ; PVD through EX
                                                            TI Line detection  
                                                                               
                                                               
   87 00000048 00000000        DCD              TAMP_STAMP_IRQHandler ; Tamper 
                                                            and TimeStamps thro
                                                            ugh the EXTI line  
                                                                      
   88 0000004C 00000000        DCD              RTC_WKUP_IRQHandler ; RTC Wakeu
                                                            p through the EXTI 
                                                            line               
                                                                    
   89 00000050 00000000        DCD              FLASH_IRQHandler ; FLASH       
                                                                               
                                                                             
   90 00000054 00000000        DCD              RCC_IRQHandler ; RCC           
                                                                               
                                                                           
   91 00000058 00000000        DCD              EXTI0_IRQHandler ; EXTI Line0  
                                                                               
                                                                               
                                                                 
   92 0000005C 00000000        DCD              EXTI1_IRQHandler ; EXTI Line1  
                                                                               
                                                                               
                                                                 
   93 00000060 00000000        DCD              EXTI2_IRQHandler ; EXTI Line2  
                                                                               
                                                                               
                                                                 
   94 00000064 00000000        DCD              EXTI3_IRQHandler ; EXTI Line3  
                                                                               
                                                                               
                                                                 
   95 00000068 00000000        DCD              EXTI4_IRQHandler ; EXTI Line4  
                                                                               
                                                                               
                                                                 
   96 0000006C 00000000        DCD              DMA1_Stream0_IRQHandler ; DMA1 
                                                            Stream 0           
                                                                               
                                                                 
   97 00000070 00000000        DCD              DMA1_Stream1_IRQHandler ; DMA1 
                                                            Stream 1           
                                                                               
                                                                 
   98 00000074 00000000        DCD              DMA1_Stream2_IRQHandler ; DMA1 
                                                            Stream 2           
                                                                               
                                                                 
   99 00000078 00000000        DCD              DMA1_Stream3_IRQHandler ; DMA1 
                                                            Stream 3           
                                                                               
                                                                 



ARM Macro Assembler    Page 4 


  100 0000007C 00000000        DCD              DMA1_Stream4_IRQHandler ; DMA1 
                                                            Stream 4           
                                                                               
                                                                 
  101 00000080 00000000        DCD              DMA1_Stream5_IRQHandler ; DMA1 
                                                            Stream 5           
                                                                               
                                                                 
  102 00000084 00000000        DCD              DMA1_Stream6_IRQHandler ; DMA1 
                                                            Stream 6           
                                                                               
                                                                 
  103 00000088 00000000        DCD              ADC_IRQHandler ; ADC1          
                                                                              
  104 0000008C 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                            
  105 00000090 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                            
  106 00000094 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                             
  107 00000098 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                            
  108 0000009C 00000000        DCD              EXTI9_5_IRQHandler ; External L
                                                            ine[9:5]s          
                                                                               
                                                                   
  109 000000A0 00000000        DCD              TIM1_BRK_TIM9_IRQHandler ; TIM1
                                                             Break and TIM9    
                                                                           
  110 000000A4 00000000        DCD              TIM1_UP_TIM10_IRQHandler ; TIM1
                                                             Update and TIM10  
                                                                           
  111 000000A8 00000000        DCD              TIM1_TRG_COM_TIM11_IRQHandler ;
                                                             TIM1 Trigger and C
                                                            ommutation and TIM1
                                                            1
  112 000000AC 00000000        DCD              TIM1_CC_IRQHandler ; TIM1 Captu
                                                            re Compare         
                                                                               
                                                                   
  113 000000B0 00000000        DCD              TIM2_IRQHandler ; TIM2         
                                                                               
                                                                            
  114 000000B4 00000000        DCD              TIM3_IRQHandler ; TIM3         
                                                                               
                                                                            
  115 000000B8 00000000        DCD              TIM4_IRQHandler ; TIM4         
                                                                               
                                                                            
  116 000000BC 00000000        DCD              I2C1_EV_IRQHandler ; I2C1 Event
                                                                               



ARM Macro Assembler    Page 5 


                                                                               
                                                                   
  117 000000C0 00000000        DCD              I2C1_ER_IRQHandler ; I2C1 Error
                                                                               
                                                                               
                                                                   
  118 000000C4 00000000        DCD              I2C2_EV_IRQHandler ; I2C2 Event
                                                                               
                                                                               
                                                                   
  119 000000C8 00000000        DCD              I2C2_ER_IRQHandler ; I2C2 Error
                                                                               
                                                                               
                                                                     
  120 000000CC 00000000        DCD              SPI1_IRQHandler ; SPI1         
                                                                               
                                                                            
  121 000000D0 00000000        DCD              SPI2_IRQHandler ; SPI2         
                                                                               
                                                                            
  122 000000D4 00000000        DCD              USART1_IRQHandler ; USART1     
                                                                               
                                                                              
  123 000000D8 00000000        DCD              USART2_IRQHandler ; USART2     
                                                                               
                                                                              
  124 000000DC 00000000        DCD              0           ; Reserved         
                                                                               
                                                                           
  125 000000E0 00000000        DCD              EXTI15_10_IRQHandler ; External
                                                             Line[15:10]s      
                                                                               
                                                                     
  126 000000E4 00000000        DCD              RTC_Alarm_IRQHandler ; RTC Alar
                                                            m (A and B) through
                                                             EXTI Line         
                                                                     
  127 000000E8 00000000        DCD              OTG_FS_WKUP_IRQHandler ; USB OT
                                                            G FS Wakeup through
                                                             EXTI line         
                                                                           
  128 000000EC 00000000        DCD              0           ; Reserved         
                                                                      
  129 000000F0 00000000        DCD              0           ; Reserved         
                                                                     
  130 000000F4 00000000        DCD              0           ; Reserved 
  131 000000F8 00000000        DCD              0           ; Reserved         
                                                                               
                                                                    
  132 000000FC 00000000        DCD              DMA1_Stream7_IRQHandler ; DMA1 
                                                            Stream7            
                                                                               
                                                                        
  133 00000100 00000000        DCD              0           ; Reserved         
                                                                               
                                                                             
  134 00000104 00000000        DCD              SDIO_IRQHandler ; SDIO         
                                                                               
                                                                            



ARM Macro Assembler    Page 6 


  135 00000108 00000000        DCD              TIM5_IRQHandler ; TIM5         
                                                                               
                                                                            
  136 0000010C 00000000        DCD              SPI3_IRQHandler ; SPI3         
                                                                               
                                                                            
  137 00000110 00000000        DCD              0           ; Reserved         
                                                                               
                                                                           
  138 00000114 00000000        DCD              0           ; Reserved         
                                                                               
                                                                            
  139 00000118 00000000        DCD              0           ; Reserved         
                                                                      
  140 0000011C 00000000        DCD              0           ; Reserved         
                                                                      
  141 00000120 00000000        DCD              DMA2_Stream0_IRQHandler ; DMA2 
                                                            Stream 0           
                                                                               
                                                                 
  142 00000124 00000000        DCD              DMA2_Stream1_IRQHandler ; DMA2 
                                                            Stream 1           
                                                                               
                                                                 
  143 00000128 00000000        DCD              DMA2_Stream2_IRQHandler ; DMA2 
                                                            Stream 2           
                                                                               
                                                                 
  144 0000012C 00000000        DCD              DMA2_Stream3_IRQHandler ; DMA2 
                                                            Stream 3           
                                                                               
                                                                 
  145 00000130 00000000        DCD              DMA2_Stream4_IRQHandler ; DMA2 
                                                            Stream 4           
                                                                               
                                                                 
  146 00000134 00000000        DCD              0           ; Reserved         
                                                                               
                                                                         
  147 00000138 00000000        DCD              0           ; Reserved         
                                                                         
  148 0000013C 00000000        DCD              0           ; Reserved         
                                                                               
                                                                              
  149 00000140 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                            
  150 00000144 00000000        DCD              0           ; Reserved         
                                                                               
                                                                               
                                                            
  151 00000148 00000000        DCD              0           ; Reserved         
                                                                               
                                                                              
  152 0000014C 00000000        DCD              OTG_FS_IRQHandler ; USB OTG FS 
                                                                               
                                                                              
  153 00000150 00000000        DCD              DMA2_Stream5_IRQHandler ; DMA2 



ARM Macro Assembler    Page 7 


                                                            Stream 5           
                                                                               
                                                                 
  154 00000154 00000000        DCD              DMA2_Stream6_IRQHandler ; DMA2 
                                                            Stream 6           
                                                                               
                                                                 
  155 00000158 00000000        DCD              DMA2_Stream7_IRQHandler ; DMA2 
                                                            Stream 7           
                                                                               
                                                                 
  156 0000015C 00000000        DCD              USART6_IRQHandler ; USART6     
                                                                               
                                                                               
                                                            
  157 00000160 00000000        DCD              I2C3_EV_IRQHandler ; I2C3 event
                                                                               
                                                                               
                                                                   
  158 00000164 00000000        DCD              I2C3_ER_IRQHandler ; I2C3 error
                                                                               
                                                                               
                                                                   
  159 00000168 00000000        DCD              0           ; Reserved         
                                                                          
  160 0000016C 00000000        DCD              0           ; Reserved         
                                                                          
  161 00000170 00000000        DCD              0           ; Reserved         
                                                                           
  162 00000174 00000000        DCD              0           ; Reserved         
                                                                               
                                                                      
  163 00000178 00000000        DCD              0           ; Reserved         
                                                                               
                                                                            
  164 0000017C 00000000        DCD              0           ; Reserved         
                                                                               
                                                                     
  165 00000180 00000000        DCD              0           ; Reserved 
  166 00000184 00000000        DCD              FPU_IRQHandler ; FPU
  167 00000188 00000000        DCD              0           ; Reserved  
  168 0000018C 00000000        DCD              0           ; Reserved  
  169 00000190 00000000        DCD              SPI4_IRQHandler ; SPI4
  170 00000194         
  171 00000194         __Vectors_End
  172 00000194         
  173 00000194 00000194 
                       __Vectors_Size
                               EQU              __Vectors_End - __Vectors
  174 00000194         
  175 00000194                 AREA             |.text|, CODE, READONLY
  176 00000000         
  177 00000000         ; Reset handler
  178 00000000         Reset_Handler
                               PROC
  179 00000000                 EXPORT           Reset_Handler             [WEAK
]
  180 00000000                 IMPORT           SystemInit
  181 00000000                 IMPORT           __main



ARM Macro Assembler    Page 8 


  182 00000000         
  183 00000000 4809            LDR              R0, =SystemInit
  184 00000002 4780            BLX              R0
  185 00000004 4809            LDR              R0, =__main
  186 00000006 4700            BX               R0
  187 00000008                 ENDP
  188 00000008         
  189 00000008         ; Dummy Exception Handlers (infinite loops which can be 
                       modified)
  190 00000008         
  191 00000008         NMI_Handler
                               PROC
  192 00000008                 EXPORT           NMI_Handler                [WEA
K]
  193 00000008 E7FE            B                .
  194 0000000A                 ENDP
  196 0000000A         HardFault_Handler
                               PROC
  197 0000000A                 EXPORT           HardFault_Handler          [WEA
K]
  198 0000000A E7FE            B                .
  199 0000000C                 ENDP
  201 0000000C         MemManage_Handler
                               PROC
  202 0000000C                 EXPORT           MemManage_Handler          [WEA
K]
  203 0000000C E7FE            B                .
  204 0000000E                 ENDP
  206 0000000E         BusFault_Handler
                               PROC
  207 0000000E                 EXPORT           BusFault_Handler           [WEA
K]
  208 0000000E E7FE            B                .
  209 00000010                 ENDP
  211 00000010         UsageFault_Handler
                               PROC
  212 00000010                 EXPORT           UsageFault_Handler         [WEA
K]
  213 00000010 E7FE            B                .
  214 00000012                 ENDP
  215 00000012         SVC_Handler
                               PROC
  216 00000012                 EXPORT           SVC_Handler                [WEA
K]
  217 00000012 E7FE            B                .
  218 00000014                 ENDP
  220 00000014         DebugMon_Handler
                               PROC
  221 00000014                 EXPORT           DebugMon_Handler           [WEA
K]
  222 00000014 E7FE            B                .
  223 00000016                 ENDP
  224 00000016         PendSV_Handler
                               PROC
  225 00000016                 EXPORT           PendSV_Handler             [WEA
K]
  226 00000016 E7FE            B                .
  227 00000018                 ENDP
  228 00000018         SysTick_Handler



ARM Macro Assembler    Page 9 


                               PROC
  229 00000018                 EXPORT           SysTick_Handler            [WEA
K]
  230 00000018 E7FE            B                .
  231 0000001A                 ENDP
  232 0000001A         
  233 0000001A         Default_Handler
                               PROC
  234 0000001A         
  235 0000001A                 EXPORT           WWDG_IRQHandler                
   [WEAK]
  236 0000001A                 EXPORT           PVD_IRQHandler                 
   [WEAK]
  237 0000001A                 EXPORT           TAMP_STAMP_IRQHandler          
   [WEAK]
  238 0000001A                 EXPORT           RTC_WKUP_IRQHandler            
   [WEAK]
  239 0000001A                 EXPORT           FLASH_IRQHandler               
   [WEAK]
  240 0000001A                 EXPORT           RCC_IRQHandler                 
   [WEAK]
  241 0000001A                 EXPORT           EXTI0_IRQHandler               
   [WEAK]
  242 0000001A                 EXPORT           EXTI1_IRQHandler               
   [WEAK]
  243 0000001A                 EXPORT           EXTI2_IRQHandler               
   [WEAK]
  244 0000001A                 EXPORT           EXTI3_IRQHandler               
   [WEAK]
  245 0000001A                 EXPORT           EXTI4_IRQHandler               
   [WEAK]
  246 0000001A                 EXPORT           DMA1_Stream0_IRQHandler        
   [WEAK]
  247 0000001A                 EXPORT           DMA1_Stream1_IRQHandler        
   [WEAK]
  248 0000001A                 EXPORT           DMA1_Stream2_IRQHandler        
   [WEAK]
  249 0000001A                 EXPORT           DMA1_Stream3_IRQHandler        
   [WEAK]
  250 0000001A                 EXPORT           DMA1_Stream4_IRQHandler        
   [WEAK]
  251 0000001A                 EXPORT           DMA1_Stream5_IRQHandler        
   [WEAK]
  252 0000001A                 EXPORT           DMA1_Stream6_IRQHandler        
   [WEAK]
  253 0000001A                 EXPORT           ADC_IRQHandler                 
   [WEAK]
  254 0000001A                 EXPORT           EXTI9_5_IRQHandler             
   [WEAK]
  255 0000001A                 EXPORT           TIM1_BRK_TIM9_IRQHandler       
   [WEAK]
  256 0000001A                 EXPORT           TIM1_UP_TIM10_IRQHandler       
   [WEAK]
  257 0000001A                 EXPORT           TIM1_TRG_COM_TIM11_IRQHandler  
   [WEAK]
  258 0000001A                 EXPORT           TIM1_CC_IRQHandler             
   [WEAK]
  259 0000001A                 EXPORT           TIM2_IRQHandler                
   [WEAK]



ARM Macro Assembler    Page 10 


  260 0000001A                 EXPORT           TIM3_IRQHandler                
   [WEAK]
  261 0000001A                 EXPORT           TIM4_IRQHandler                
   [WEAK]
  262 0000001A                 EXPORT           I2C1_EV_IRQHandler             
   [WEAK]
  263 0000001A                 EXPORT           I2C1_ER_IRQHandler             
   [WEAK]
  264 0000001A                 EXPORT           I2C2_EV_IRQHandler             
   [WEAK]
  265 0000001A                 EXPORT           I2C2_ER_IRQHandler             
   [WEAK]
  266 0000001A                 EXPORT           SPI1_IRQHandler                
   [WEAK]
  267 0000001A                 EXPORT           SPI2_IRQHandler                
   [WEAK]
  268 0000001A                 EXPORT           USART1_IRQHandler              
   [WEAK]
  269 0000001A                 EXPORT           USART2_IRQHandler              
   [WEAK]
  270 0000001A                 EXPORT           EXTI15_10_IRQHandler           
   [WEAK]
  271 0000001A                 EXPORT           RTC_Alarm_IRQHandler           
   [WEAK]
  272 0000001A                 EXPORT           OTG_FS_WKUP_IRQHandler         
   [WEAK]
  273 0000001A                 EXPORT           DMA1_Stream7_IRQHandler        
   [WEAK]
  274 0000001A                 EXPORT           SDIO_IRQHandler                
   [WEAK]
  275 0000001A                 EXPORT           TIM5_IRQHandler                
   [WEAK]
  276 0000001A                 EXPORT           SPI3_IRQHandler                
   [WEAK]
  277 0000001A                 EXPORT           DMA2_Stream0_IRQHandler        
   [WEAK]
  278 0000001A                 EXPORT           DMA2_Stream1_IRQHandler        
   [WEAK]
  279 0000001A                 EXPORT           DMA2_Stream2_IRQHandler        
   [WEAK]
  280 0000001A                 EXPORT           DMA2_Stream3_IRQHandler        
   [WEAK]
  281 0000001A                 EXPORT           DMA2_Stream4_IRQHandler        
   [WEAK]
  282 0000001A                 EXPORT           OTG_FS_IRQHandler              
   [WEAK]
  283 0000001A                 EXPORT           DMA2_Stream5_IRQHandler        
   [WEAK]
  284 0000001A                 EXPORT           DMA2_Stream6_IRQHandler        
   [WEAK]
  285 0000001A                 EXPORT           DMA2_Stream7_IRQHandler        
   [WEAK]
  286 0000001A                 EXPORT           USART6_IRQHandler              
   [WEAK]
  287 0000001A                 EXPORT           I2C3_EV_IRQHandler             
   [WEAK]
  288 0000001A                 EXPORT           I2C3_ER_IRQHandler             
   [WEAK]
  289 0000001A                 EXPORT           FPU_IRQHandler                 



ARM Macro Assembler    Page 11 


   [WEAK]
  290 0000001A                 EXPORT           SPI4_IRQHandler                
   [WEAK]
  291 0000001A         
  292 0000001A         WWDG_IRQHandler
  293 0000001A         PVD_IRQHandler
  294 0000001A         TAMP_STAMP_IRQHandler
  295 0000001A         RTC_WKUP_IRQHandler
  296 0000001A         FLASH_IRQHandler
  297 0000001A         RCC_IRQHandler
  298 0000001A         EXTI0_IRQHandler
  299 0000001A         EXTI1_IRQHandler
  300 0000001A         EXTI2_IRQHandler
  301 0000001A         EXTI3_IRQHandler
  302 0000001A         EXTI4_IRQHandler
  303 0000001A         DMA1_Stream0_IRQHandler
  304 0000001A         DMA1_Stream1_IRQHandler
  305 0000001A         DMA1_Stream2_IRQHandler
  306 0000001A         DMA1_Stream3_IRQHandler
  307 0000001A         DMA1_Stream4_IRQHandler
  308 0000001A         DMA1_Stream5_IRQHandler
  309 0000001A         DMA1_Stream6_IRQHandler
  310 0000001A         ADC_IRQHandler
  311 0000001A         EXTI9_5_IRQHandler
  312 0000001A         TIM1_BRK_TIM9_IRQHandler
  313 0000001A         TIM1_UP_TIM10_IRQHandler
  314 0000001A         TIM1_TRG_COM_TIM11_IRQHandler
  315 0000001A         TIM1_CC_IRQHandler
  316 0000001A         TIM2_IRQHandler
  317 0000001A         TIM3_IRQHandler
  318 0000001A         TIM4_IRQHandler
  319 0000001A         I2C1_EV_IRQHandler
  320 0000001A         I2C1_ER_IRQHandler
  321 0000001A         I2C2_EV_IRQHandler
  322 0000001A         I2C2_ER_IRQHandler
  323 0000001A         SPI1_IRQHandler
  324 0000001A         SPI2_IRQHandler
  325 0000001A         USART1_IRQHandler
  326 0000001A         USART2_IRQHandler
  327 0000001A         EXTI15_10_IRQHandler
  328 0000001A         RTC_Alarm_IRQHandler
  329 0000001A         OTG_FS_WKUP_IRQHandler
  330 0000001A         DMA1_Stream7_IRQHandler
  331 0000001A         SDIO_IRQHandler
  332 0000001A         TIM5_IRQHandler
  333 0000001A         SPI3_IRQHandler
  334 0000001A         DMA2_Stream0_IRQHandler
  335 0000001A         DMA2_Stream1_IRQHandler
  336 0000001A         DMA2_Stream2_IRQHandler
  337 0000001A         DMA2_Stream3_IRQHandler
  338 0000001A         DMA2_Stream4_IRQHandler
  339 0000001A         ETH_IRQHandler
  340 0000001A         OTG_FS_IRQHandler
  341 0000001A         DMA2_Stream5_IRQHandler
  342 0000001A         DMA2_Stream6_IRQHandler
  343 0000001A         DMA2_Stream7_IRQHandler
  344 0000001A         USART6_IRQHandler
  345 0000001A         I2C3_EV_IRQHandler
  346 0000001A         I2C3_ER_IRQHandler



ARM Macro Assembler    Page 12 


  347 0000001A         FPU_IRQHandler
  348 0000001A         SPI4_IRQHandler
  349 0000001A         
  350 0000001A E7FE            B                .
  351 0000001C         
  352 0000001C                 ENDP
  353 0000001C         
  354 0000001C                 ALIGN
  355 0000001C         
  356 0000001C         ;*******************************************************
                       ************************
  357 0000001C         ; User Stack and Heap initialization
  358 0000001C         ;*******************************************************
                       ************************
  359 0000001C                 IF               :DEF:__MICROLIB
  366 0000001C         
  367 0000001C                 IMPORT           __use_two_region_memory
  368 0000001C                 EXPORT           __user_initial_stackheap
  369 0000001C         
  370 0000001C         __user_initial_stackheap
  371 0000001C         
  372 0000001C 4804            LDR              R0, =  Heap_Mem
  373 0000001E 4905            LDR              R1, =(Stack_Mem + Stack_Size)
  374 00000020 4A05            LDR              R2, = (Heap_Mem +  Heap_Size)
  375 00000022 4B06            LDR              R3, = Stack_Mem
  376 00000024 4770            BX               LR
  377 00000026         
  378 00000026 00 00           ALIGN
  379 00000028         
  380 00000028                 ENDIF
  381 00000028         
  382 00000028                 END
              00000000 
              00000000 
              00000000 
              00000400 
              00000200 
              00000000 
Command Line: --debug --xref --cpu=Cortex-M4.fp --apcs=interwork --depend=.\tar
gets\nucleo_f401_ext_8mhz\startup_stm32f401xx.d -o.\targets\nucleo_f401_ext_8mh
z\startup_stm32f401xx.o -I"C:\Users\tilz0R\Google Drive\JAVNO\ELEKTRONIKA\ARM\S
TM32F429\majerle.eu\01-STM32F4xx_Keil_CMSIS_USB_Default_Project_All\RTE" -IC:\K
eil_v5\ARM\PACK\Keil\STM32F4xx_DFP\2.2.0\Drivers\CMSIS\Device\ST\STM32F4xx\Incl
ude -IC:\Keil_v5\ARM\CMSIS\Include --predefine="__UVISION_VERSION SETA 513" --p
redefine="STM32F401xE SETA 1" --list=.\startup_stm32f401xx.lst ..\00-STM32F4xx_
STANDARD_PERIPHERAL_DRIVERS\CMSIS\Device\ST\STM32F4xx\Source\Templates\arm\star
tup_stm32f401xx.s



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

STACK 00000000

Symbol: STACK
   Definitions
      At line 41 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: STACK unused
Stack_Mem 00000000

Symbol: Stack_Mem
   Definitions
      At line 42 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 373 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 375 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

__initial_sp 00000400

Symbol: __initial_sp
   Definitions
      At line 43 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 67 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
Comment: __initial_sp used once
3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

HEAP 00000000

Symbol: HEAP
   Definitions
      At line 52 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: HEAP unused
Heap_Mem 00000000

Symbol: Heap_Mem
   Definitions
      At line 54 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 372 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 374 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

__heap_base 00000000

Symbol: __heap_base
   Definitions
      At line 53 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: __heap_base unused
__heap_limit 00000200

Symbol: __heap_limit
   Definitions
      At line 55 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: __heap_limit unused
4 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

RESET 00000000

Symbol: RESET
   Definitions
      At line 62 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: RESET unused
__Vectors 00000000

Symbol: __Vectors
   Definitions
      At line 67 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 63 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 173 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

__Vectors_End 00000194

Symbol: __Vectors_End
   Definitions
      At line 171 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 64 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 173 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Relocatable symbols

.text 00000000

Symbol: .text
   Definitions
      At line 175 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: .text unused
ADC_IRQHandler 0000001A

Symbol: ADC_IRQHandler
   Definitions
      At line 310 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 103 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 253 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

BusFault_Handler 0000000E

Symbol: BusFault_Handler
   Definitions
      At line 206 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 72 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 207 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream0_IRQHandler 0000001A

Symbol: DMA1_Stream0_IRQHandler
   Definitions
      At line 303 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 96 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 246 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream1_IRQHandler 0000001A

Symbol: DMA1_Stream1_IRQHandler
   Definitions
      At line 304 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 97 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 247 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream2_IRQHandler 0000001A




ARM Macro Assembler    Page 2 Alphabetic symbol ordering
Relocatable symbols

Symbol: DMA1_Stream2_IRQHandler
   Definitions
      At line 305 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 98 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 248 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream3_IRQHandler 0000001A

Symbol: DMA1_Stream3_IRQHandler
   Definitions
      At line 306 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 99 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 249 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream4_IRQHandler 0000001A

Symbol: DMA1_Stream4_IRQHandler
   Definitions
      At line 307 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 100 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 250 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream5_IRQHandler 0000001A

Symbol: DMA1_Stream5_IRQHandler
   Definitions
      At line 308 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 101 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 251 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream6_IRQHandler 0000001A

Symbol: DMA1_Stream6_IRQHandler
   Definitions
      At line 309 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 102 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 252 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA1_Stream7_IRQHandler 0000001A



ARM Macro Assembler    Page 3 Alphabetic symbol ordering
Relocatable symbols


Symbol: DMA1_Stream7_IRQHandler
   Definitions
      At line 330 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 132 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 273 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream0_IRQHandler 0000001A

Symbol: DMA2_Stream0_IRQHandler
   Definitions
      At line 334 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 141 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 277 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream1_IRQHandler 0000001A

Symbol: DMA2_Stream1_IRQHandler
   Definitions
      At line 335 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 142 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 278 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream2_IRQHandler 0000001A

Symbol: DMA2_Stream2_IRQHandler
   Definitions
      At line 336 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 143 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 279 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream3_IRQHandler 0000001A

Symbol: DMA2_Stream3_IRQHandler
   Definitions
      At line 337 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 144 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 280 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s




ARM Macro Assembler    Page 4 Alphabetic symbol ordering
Relocatable symbols

DMA2_Stream4_IRQHandler 0000001A

Symbol: DMA2_Stream4_IRQHandler
   Definitions
      At line 338 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 145 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 281 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream5_IRQHandler 0000001A

Symbol: DMA2_Stream5_IRQHandler
   Definitions
      At line 341 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 153 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 283 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream6_IRQHandler 0000001A

Symbol: DMA2_Stream6_IRQHandler
   Definitions
      At line 342 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 154 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 284 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DMA2_Stream7_IRQHandler 0000001A

Symbol: DMA2_Stream7_IRQHandler
   Definitions
      At line 343 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 155 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 285 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

DebugMon_Handler 00000014

Symbol: DebugMon_Handler
   Definitions
      At line 220 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 79 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 221 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s



ARM Macro Assembler    Page 5 Alphabetic symbol ordering
Relocatable symbols


Default_Handler 0000001A

Symbol: Default_Handler
   Definitions
      At line 233 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: Default_Handler unused
ETH_IRQHandler 0000001A

Symbol: ETH_IRQHandler
   Definitions
      At line 339 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: ETH_IRQHandler unused
EXTI0_IRQHandler 0000001A

Symbol: EXTI0_IRQHandler
   Definitions
      At line 298 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 91 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 241 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI15_10_IRQHandler 0000001A

Symbol: EXTI15_10_IRQHandler
   Definitions
      At line 327 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 125 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 270 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI1_IRQHandler 0000001A

Symbol: EXTI1_IRQHandler
   Definitions
      At line 299 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 92 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 242 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI2_IRQHandler 0000001A

Symbol: EXTI2_IRQHandler
   Definitions



ARM Macro Assembler    Page 6 Alphabetic symbol ordering
Relocatable symbols

      At line 300 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 93 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 243 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI3_IRQHandler 0000001A

Symbol: EXTI3_IRQHandler
   Definitions
      At line 301 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 94 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 244 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI4_IRQHandler 0000001A

Symbol: EXTI4_IRQHandler
   Definitions
      At line 302 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 95 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 245 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

EXTI9_5_IRQHandler 0000001A

Symbol: EXTI9_5_IRQHandler
   Definitions
      At line 311 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 108 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 254 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

FLASH_IRQHandler 0000001A

Symbol: FLASH_IRQHandler
   Definitions
      At line 296 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 89 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 239 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

FPU_IRQHandler 0000001A

Symbol: FPU_IRQHandler



ARM Macro Assembler    Page 7 Alphabetic symbol ordering
Relocatable symbols

   Definitions
      At line 347 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 166 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 289 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

HardFault_Handler 0000000A

Symbol: HardFault_Handler
   Definitions
      At line 196 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 70 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 197 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C1_ER_IRQHandler 0000001A

Symbol: I2C1_ER_IRQHandler
   Definitions
      At line 320 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 117 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 263 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C1_EV_IRQHandler 0000001A

Symbol: I2C1_EV_IRQHandler
   Definitions
      At line 319 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 116 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 262 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C2_ER_IRQHandler 0000001A

Symbol: I2C2_ER_IRQHandler
   Definitions
      At line 322 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 119 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 265 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C2_EV_IRQHandler 0000001A




ARM Macro Assembler    Page 8 Alphabetic symbol ordering
Relocatable symbols

Symbol: I2C2_EV_IRQHandler
   Definitions
      At line 321 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 118 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 264 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C3_ER_IRQHandler 0000001A

Symbol: I2C3_ER_IRQHandler
   Definitions
      At line 346 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 158 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 288 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

I2C3_EV_IRQHandler 0000001A

Symbol: I2C3_EV_IRQHandler
   Definitions
      At line 345 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 157 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 287 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

MemManage_Handler 0000000C

Symbol: MemManage_Handler
   Definitions
      At line 201 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 71 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 202 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

NMI_Handler 00000008

Symbol: NMI_Handler
   Definitions
      At line 191 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 69 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 192 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

OTG_FS_IRQHandler 0000001A



ARM Macro Assembler    Page 9 Alphabetic symbol ordering
Relocatable symbols


Symbol: OTG_FS_IRQHandler
   Definitions
      At line 340 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 152 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 282 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

OTG_FS_WKUP_IRQHandler 0000001A

Symbol: OTG_FS_WKUP_IRQHandler
   Definitions
      At line 329 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 127 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 272 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

PVD_IRQHandler 0000001A

Symbol: PVD_IRQHandler
   Definitions
      At line 293 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 86 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 236 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

PendSV_Handler 00000016

Symbol: PendSV_Handler
   Definitions
      At line 224 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 81 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 225 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

RCC_IRQHandler 0000001A

Symbol: RCC_IRQHandler
   Definitions
      At line 297 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 90 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 240 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s




ARM Macro Assembler    Page 10 Alphabetic symbol ordering
Relocatable symbols

RTC_Alarm_IRQHandler 0000001A

Symbol: RTC_Alarm_IRQHandler
   Definitions
      At line 328 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 126 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 271 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

RTC_WKUP_IRQHandler 0000001A

Symbol: RTC_WKUP_IRQHandler
   Definitions
      At line 295 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 88 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 238 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

Reset_Handler 00000000

Symbol: Reset_Handler
   Definitions
      At line 178 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 68 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 179 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SDIO_IRQHandler 0000001A

Symbol: SDIO_IRQHandler
   Definitions
      At line 331 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 134 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 274 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SPI1_IRQHandler 0000001A

Symbol: SPI1_IRQHandler
   Definitions
      At line 323 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 120 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 266 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s



ARM Macro Assembler    Page 11 Alphabetic symbol ordering
Relocatable symbols


SPI2_IRQHandler 0000001A

Symbol: SPI2_IRQHandler
   Definitions
      At line 324 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 121 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 267 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SPI3_IRQHandler 0000001A

Symbol: SPI3_IRQHandler
   Definitions
      At line 333 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 136 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 276 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SPI4_IRQHandler 0000001A

Symbol: SPI4_IRQHandler
   Definitions
      At line 348 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 169 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 290 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SVC_Handler 00000012

Symbol: SVC_Handler
   Definitions
      At line 215 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 78 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 216 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

SysTick_Handler 00000018

Symbol: SysTick_Handler
   Definitions
      At line 228 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 82 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 229 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev



ARM Macro Assembler    Page 12 Alphabetic symbol ordering
Relocatable symbols

ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TAMP_STAMP_IRQHandler 0000001A

Symbol: TAMP_STAMP_IRQHandler
   Definitions
      At line 294 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 87 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 237 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM1_BRK_TIM9_IRQHandler 0000001A

Symbol: TIM1_BRK_TIM9_IRQHandler
   Definitions
      At line 312 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 109 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 255 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM1_CC_IRQHandler 0000001A

Symbol: TIM1_CC_IRQHandler
   Definitions
      At line 315 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 112 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 258 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM1_TRG_COM_TIM11_IRQHandler 0000001A

Symbol: TIM1_TRG_COM_TIM11_IRQHandler
   Definitions
      At line 314 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 111 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 257 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM1_UP_TIM10_IRQHandler 0000001A

Symbol: TIM1_UP_TIM10_IRQHandler
   Definitions
      At line 313 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 110 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s



ARM Macro Assembler    Page 13 Alphabetic symbol ordering
Relocatable symbols

      At line 256 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM2_IRQHandler 0000001A

Symbol: TIM2_IRQHandler
   Definitions
      At line 316 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 113 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 259 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM3_IRQHandler 0000001A

Symbol: TIM3_IRQHandler
   Definitions
      At line 317 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 114 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 260 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM4_IRQHandler 0000001A

Symbol: TIM4_IRQHandler
   Definitions
      At line 318 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 115 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 261 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

TIM5_IRQHandler 0000001A

Symbol: TIM5_IRQHandler
   Definitions
      At line 332 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 135 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 275 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

USART1_IRQHandler 0000001A

Symbol: USART1_IRQHandler
   Definitions
      At line 325 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 122 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev



ARM Macro Assembler    Page 14 Alphabetic symbol ordering
Relocatable symbols

ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 268 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

USART2_IRQHandler 0000001A

Symbol: USART2_IRQHandler
   Definitions
      At line 326 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 123 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 269 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

USART6_IRQHandler 0000001A

Symbol: USART6_IRQHandler
   Definitions
      At line 344 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 156 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 286 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

UsageFault_Handler 00000010

Symbol: UsageFault_Handler
   Definitions
      At line 211 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 73 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 212 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

WWDG_IRQHandler 0000001A

Symbol: WWDG_IRQHandler
   Definitions
      At line 292 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 85 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 235 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

__user_initial_stackheap 0000001C

Symbol: __user_initial_stackheap
   Definitions
      At line 370 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses



ARM Macro Assembler    Page 15 Alphabetic symbol ordering
Relocatable symbols

      At line 368 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
Comment: __user_initial_stackheap used once
70 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
Absolute symbols

Heap_Size 00000200

Symbol: Heap_Size
   Definitions
      At line 50 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 54 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 374 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

Stack_Size 00000400

Symbol: Stack_Size
   Definitions
      At line 39 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 42 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
      At line 373 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s

__Vectors_Size 00000194

Symbol: __Vectors_Size
   Definitions
      At line 173 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 65 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Devi
ce\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
Comment: __Vectors_Size used once
3 symbols



ARM Macro Assembler    Page 1 Alphabetic symbol ordering
External symbols

SystemInit 00000000

Symbol: SystemInit
   Definitions
      At line 180 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 183 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
Comment: SystemInit used once
__main 00000000

Symbol: __main
   Definitions
      At line 181 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      At line 185 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
Comment: __main used once
__use_two_region_memory 00000000

Symbol: __use_two_region_memory
   Definitions
      At line 367 in file ..\00-STM32F4xx_STANDARD_PERIPHERAL_DRIVERS\CMSIS\Dev
ice\ST\STM32F4xx\Source\Templates\arm\startup_stm32f401xx.s
   Uses
      None
Comment: __use_two_region_memory unused
3 symbols
423 symbols in table
